Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation RS/6000 43P-150 (250MHz)

SPECfp2000 = SPECfp_base2000 = -- 84.4

SPEC license #: 11 Tested by: IBM, Austin, TX Test date: Apr-2000 Hardware Avail: May-2000 Software Avail: May-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 20 40 60 80 100 120

168.wupwise 1600 1472 109

171.swim 3100 4528 68.5

172.mgrid 1800 3222 55.9

173.applu 2100 3162 66.4

177.mesa 1400 1257 111

178.galgel 2900 4282 67.7

179.art 2600 2393 109

183.equake 1300 1520 85.5

187.facerec 1900 2162 87.9

188.ammp 2200 2724 80.8

189.lucas 2000 2294 87.2

191.fma3d 2100 2104 99.8

200.sixtrack 1100 1344 81.8

301.apsi 2600 2716 95.7

Hardware

CPU: 250MHz IBM PowerPC 604e CPU MHz: 250 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 32KBI+32KBD (on chip) Secondary Cache: 1MB unified (off chip) L3 Cache: None Other Cache: None Memory: 512MB Disk Subsystem: 1X4.5GB Ultra SCSI, 7200 RPM Other Hardware: None

Software

Operating System: AIX 4.3.3 plus APAR IY09807 Compiler: IBM XL Fortran 7.1.0 IBM C 5.01 File System: AIX/JFS System State: Multi-user

Notes/Tuning Information

 Portability Flags
     -qfixed        used in: wupwise, swim, mgrid, applu, galgel, sixtrack, apsi
     -qsuffix=f=f90 used in: galgel, facerec, lucas, fma3d
 Base Flags:
     Fortran: -O3 -qarch=ppc
     C:       -O3 -qarch=ppc