Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 615 Model 6C3 (1200 Mhz, 1 CPU)

SPECint2000 = SPECint_base2000 = -- 727 SPEC license #: 11 Tested by: IBM, Austin, Tx Test date: May-2003 Hardware Avail: Jun-2003 Software Avail: May-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 300 600 900 1200

164.gzip 1400 266 526

175.vpr 1400 210 666

176.gcc 1100 140 786

181.mcf 1800 190 948

186.crafty 1000 154 648

197.parser 1800 291 618

252.eon 1300 157 829

253.perlbmk 1800 312 577

254.gap 1100 169 651

255.vortex 1900 212 896

256.bzip2 1500 195 769

300.twolf 3000 312 963

Hardware

CPU: POWER4+ CPU MHz: 1200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 2 cores/chip, 1 processor chip/DCM CPU(s) orderable: 1,2 (order by # cores) Parallel: No Primary Cache: 64KBI+32KBD (on chip) per core Secondary Cache: 1536KB unified (on chip) per chip L3 Cache: 8MB unified (off-chip) per DCM, 1 DCM in SUT Other Cache: None Memory: 8 GB Disk Subsystem: 1x36GB Ultra3 SCSI 10K RPM Other Hardware: None

Software

Operating System: SLES 8 Service Release 1 for pSeries w/2.4.19 kernel Compiler: IBM VisualAge C++ Version 6.0 for Linux on pSeries

IBM XL Fortran Version 8.1 for Linux on pSeries

File System: ext2 System State: Multi-user

Notes/Tuning Information

 cfg file:  ppc32-linux-ibm-ref-o5.cfg

 Compiled 32-bit applications

 CC  = /opt/ibmcmp/vac/6.0/bin/cc
 CXX = /opt/ibmcmp/vacpp/6.0/bin/xlC

 DCM: Acronym for "Dual-chip module"
 SUT: Acronym for "System under test"

 IBM eServer pSeries 615 Model 6C3 (rack-mount server) and pSeries
 615 Model 6E3 (deskside server) are electronically equivalent.
 1 processor was deconfigured through the configuration menu.
 SLES: SuSE Linux Enterprise Server
 Integer optimization flags
    Int: -qpdf1/pdf2 -O5

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

IBM Corporation

IBM eServer pSeries 615 Model 6C3 (1200 Mhz, 1 CPU)

SPECint2000 = SPECint_base2000 = -- 727 SPEC license #: 11 Tested by: IBM, Austin, Tx Test date: May-2003 Hardware Avail: Jun-2003 Software Avail: May-2003

Notes/Tuning Information (Continued)

 Integer portability flags
    gcc:  -DHOST_WORDS_BIG_ENDIAN
    mcf: None
    crafty: -DLINUX_PPC32
    parser: None
    eon: -DHAS_ERRLIST
    eon:
    eon: Using srcalt=fmax_errno

    perlbmk: -DSPEC_CPU2000_LINUX_PPC32 -DSPEC_CPU2000_NEED_BOOL
             -DHAS_FGETPOS -DHAS_FSETPOS
    gap: -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_CALLOC_PROTO
    vortex: None
    bzip2: None
    twolf: -DHAVE_SIGNED_CHAR