Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER850 (1890MHz)

SPECint_rate2000 = SPECint_rate_base2000 = 118 102 SPEC license #: 19 Tested by: Fujitsu Limited Test date: May-2004 Hardware Avail: Aug-2004 Software Avail: Apr-2004

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 50 100 150 200 250 164.gzip 8 163 79.7 8 147 88.2

175.vpr 8 133 98.0 8 130 99.6

176.gcc 8 151 67.6 8 82.3 124

181.mcf 8 165 101 8 141 118

186.crafty 8 83.8 111 8 77.5 120

197.parser 8 172 97.2 8 158 106

252.eon 8 145 83.0 8 96.5 125

253.perlbmk 8 145 115 8 142 118

254.gap 8 110 92.6 8 108 94.5

255.vortex 8 94.0 188 8 81.0 218

256.bzip2 8 134 104 8 129 108

300.twolf 8 214 130 8 197 141

Hardware

CPU: SPARC64 V CPU MHz: 1890 FPU: Integrated CPU(s) enabled: 8 cores, 8 chips, 1 core/chip CPU(s) orderable: 1 to 16 (increments of 1) Parallel: None Primary Cache: 128KBI + 128KBD on chip Secondary Cache: 3MB(I+D) on chip L3 Cache: None Other Cache: None Memory: 32768MB Disk Subsystem: 1 x 36.4GB SCSI (10000rpm) Other Hardware: None

Software

Operating System: Solaris 9 4/04 Compiler: Fujitsu Parallelnavi 2.3 with patch 913287-01

Sun Studio 8 Sun Performance Library 8

File System: ufs System State: multi user

Notes/Tuning Information

 FDO: (for Parallelnavi 2.3)
 fdo_pre0=rm -rf ‘pwd‘/*.f.d
 PASS1=-Kpg
 PASS2=-Kpu=$(EXEBASE).fbk
 FDO: (for Sun Studio 8)
 fdo_pre0=rm -rf ./feedback.profile ./SunWS_cache
 PASS1=-xprofile=collect:./feedback
 PASS2=-xprofile=use:./feedback

 Integer base flags:
 (using C compiler of Sun Studio 8)
    -fast -xtarget=ultra3cu -xipo=2 ONESTEP=yes FDO
 (using C++ compiler of Sun Studio 8)
    -fast -xchip=ultra3cu -xarch=v8plusb -xipo=2 ONESTEP=yes

 Integer peak flags:
 (using C compiler of Parallelnavi 2.3)
 300.twolf:    -Kfast_GP2=3,GREG,eval,preex,cfunc -O3 ONESTEP=yes FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER850 (1890MHz)

SPECint_rate2000 = SPECint_rate_base2000 = 118 102 SPEC license #: 19 Tested by: Fujitsu Limited Test date: May-2004 Hardware Avail: Aug-2004 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

 (using C compiler of Sun Studio 8)
 164.gzip:     -xO5 -xarch=v8plusb -xchip=ultra2 -xcache=128/64/2:4096/64/4
               -xalias_level=std -xipo=2 -xprefetch -W2,-whole,-Ainline
               -Wc,-Qiselect-funcalign=64 ONESTEP=yes FDO
 175.vpr:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xalias_level=std -xchip=ultra -xipo=2 -xprefetch=latx:1.6
               -xsfpconst -W2,-whole -Wc,-Qeps:do_spec_load=1,
               -Qeps:enabled=1,-Qeps:rp_filtering_margin=100,
               -Qiselect-funcalign=64 -lmopt -lm ONESTEP=yes FDO
 176.gcc:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 -W2,-whole -Wc,-Qgsched-T4,-Qgsched-trace_late=1,
               -Qiselect-funcalign=64 -ll2amm ONESTEP=yes FDO
 181.mcf:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 -xprefetch_level=3 -W2,-Apf:llist=3:noinnerllist
               -Wc,-Qeps:enabled=1 ONESTEP=yes FDO
 186.crafty:   -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xalias_level=strong -xipo=2 -xpagesize=512K -W2,-Ashort_ldst
               ONESTEP=yes FDO
 197.parser:   -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xalias_level=strong -xipo=2 -xregs=syst
               -Wc,-Qgsched-T6,-Qgsched-trace_late=1,
               -Qipa:valueprediction,-Qiselect-funcalign=64
               ONESTEP=yes FDO
 253.perlbmk:  -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo=2 -xalias_level=std -Wc,-Qeps:enabled=1,
               -Qiselect-funcalign=64 ONESTEP=yes FDO
 254.gap:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xalias_level=strong -xipo=2 -xprefetch_level=3
               -xprefetch=latx:2.0 -xvector -W2,-Abcopy
               -Wc,-Qiselect-funcalign=64 ONESTEP=yes FDO
 255.vortex:   -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xchip=ultra -xipo=2 -xrestrict -xprefetch=latx:1.6
               -W2,-Aheap,-Ainline:recursion=1:cs=500:irs=6000,-Aunroll,-crit,
               -Ms15,-Mt300,-Mr6000,-reroll=1 -Wc,-Qdepgraph-early_cross_call=1,
               -Qeps:do_spec_load=1,-Qeps:enabled=1,-Qiselect-funcalign=64,
               -Qpeep-Sh0 -ll2amm ONESTEP=yes FDO
 256.bzip2:    -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -xipo -xalias_level=strong -xregs=syst -xrestrict
               -xprefetch=latx:1.8 -W2,-Abopt -Wc,-Qiselect-funcalign=64,
               -Qeps:enabled ONESTEP=yes FDO

 (using C++ compiler of Sun Studio 8)
 252.eon:      -fast -xarch=v8plusb -xchip=ultra3cu -xcache=128/64/2:4096/64/4
               -noex -xalias_level=compatible -xipo=2 -xregs=syst -xunroll=3
               -Qoption cg -Qeps:enabled=1,-Qeps:ws=32,-Qgsched-T4,
               -Qgsched-trace_late=1,-Qiselect-funcalign=64
               -Qoption iropt -Mt2000 -lmopt ONESTEP=yes FDO

 Portability:
 176.gcc:      -Dalloca=__builtin_alloca -DHOST_WORDS_BIG_ENDIAN
 186.crafty:   -DSUN
 252.eon:      -library=iostream
 253.perlbmk:  -DSPEC_CPU2000_SOLARIS
 254.gap:      -DSYS_IS_USG -DSYS_HAS_TIME_PROTO -DSYS_HAS_SIGNAL_PROTO
               -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_IOCTL_PROTO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER850 (1890MHz)

SPECint_rate2000 = SPECint_rate_base2000 = 118 102 SPEC license #: 19 Tested by: Fujitsu Limited Test date: May-2004 Hardware Avail: Aug-2004 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

 System Tunables:
 (for /etc/system)
       set consistent_coloring=1
       set tune_t_fsflushr=86400
       set autoup=86400
       set memscrub_period_sec=172800

 Shell Environments:
       Stack size set to unlimited via "ulimit -s unlimited"
       MPSSHEAP=4M
       MPSSSTACK=4M
       LD_PRELOAD=mpss.so.1

 Processes were bound to CPUs using "submit=pbind".

 Extended Interleave Mode enabled.

 4 CPUs each on 2 system board. Unused CPUs have physically removed.

 Sun Studio 8, posted at URL http://wwws.sun.com/software/products/studio/
 was used for this submission.

 This result was measured on model PRIMEPOWER900.
 Model PRIMEPOWER850 and model PRIMEPOWER900 are electronically equivalent.