Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

TYAN S2865 K8E Tomcat, AMD Opteron (TM) 144

SPECint2000 = SPECint_base2000 =

1325 1255

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 139 1009 139 1009

175.vpr 1400 131 1067 126 1110

176.gcc 1100 80.3 1371 79.8 1378

181.mcf 1800 173 1041 144 1250

186.crafty 1000 85.8 1166 77.2 1296

197.parser 1800 151 1192 151 1194

252.eon 1300 76.7 1695 68.5 1898

253.perlbmk 1800 145 1242 145 1242

254.gap 1100 83.4 1319 83.4 1319

255.vortex 1900 100 1898 92.5 2053

256.bzip2 1500 144 1041 142 1055

300.twolf 3000 229 1309 206 1458

Hardware

CPU: AMD Opteron (TM) 144 (939-pin) CPU MHz: 1800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x512 MB DDR400 CL2.0 Disk Subsystem: SATA, Western Digital WD740GD, 10000 rpm Other Hardware: None

Software

Operating System: Microsoft Windows XP Pro SP2 Compiler: Intel C++ 8.0 build 20040714Z

Microsoft Visual Studio .NET 7.0.9466 (libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

  shlW32M7.lib is the SmartHeap library V7.0 from MicroQuill www.microquill.com
  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  Portability:
    176.gcc:      -Dalloca=_alloca /F10000000
    186.crafty:   -DNT_i386
    253.perlbmk:  -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:      -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
  Baseline C:   -fast -arch:SSE2 -Oi- +FDO
  Baseline C++: -fast -arch:SSE2 -GX -GR
 Peak Tuning:
  164.gzip:     basepeak=yes
  175.vpr:      -fast -arch:SSE2 +FDO
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  176.gcc:      -fast -arch:SSE2 +FDO -Oi- -Qunroll3
  181.mcf:      -fast -QaxN      +FDO
  186.crafty:   -fast -arch:SSE2 +FDO
  197.parser:         -arch:SSE2 +FDO -Oi- -Qipo
  252.eon:      -fast -arch:SSE2 +FDO -Qansi_alias
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  253.perlbmk:  basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

TYAN S2865 K8E Tomcat, AMD Opteron (TM) 144

SPECint2000 = SPECint_base2000 =

1325 1255

SPEC license #: 49 Tested by: AMD, Austin, TX Test date: Jul-2005 Hardware Avail: Aug-2005 Software Avail: Aug-2004

Notes/Tuning Information (Continued)

  254.gap:      basepeak=yes
  255.vortex:   -fast -arch:SSE  +FDO -Oi- shlW32M7.lib
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  256.bzip2:    -fast                      -Qunroll2
  300.twolf:    -fast -arch:SSE2 +FDO      -Qunroll3 shlW32M7.lib -Qansi_alias
 The tested system can be assembled using a standard ATX footprint, an Antec True 550
 Watt EPS12V power supply, and a PCI or PCIe graphics card.
 All memory slots were populated with Corsair CMX512-3200XL.
 Memory timings manually set in BIOS: CAS=2, TRCD=2, TRAS=5, TRP=2
 BIOS version 1.01