Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro

Supermicro X7DBE Motherboard (Intel Xeon processor 5160 3.0GHz)

SPECint_rate2000 = SPECint_rate_base2000 = -- 85.9

SPEC license #: 49 Tested by: AMD Austin, TX Test date: Aug-2006 Hardware Avail: Aug-2006 Software Avail: Jul-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 30 60 90 120 150 164.gzip 4 88.0 73.8

175.vpr 4 89.1 72.9

176.gcc 4 49.0 104

181.mcf 4 256 32.6

186.crafty 4 32.7 142

197.parser 4 142 59.0

252.eon 4 41.8 144

253.perlbmk 4 70.6 118

254.gap 4 81.5 62.7

255.vortex 4 76.2 116

256.bzip2 4 96.9 71.8

300.twolf 4 117 119

Hardware

CPU: Intel Xeon processor 5160 (1333MHz system bus) CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 1,2 chips Parallel: No Primary Cache: 32KB(I) + 32KB(D) on chip per core Secondary Cache: 4MB(I+D) on chip per chip L3 Cache: N/A Other Cache: N/A Memory: 8 x 1GB DDR2-667 CL5 FBDIMM Disk Subsystem: 1 X 250GB Western Digital WD2500 SATA 7200rpm Other Hardware: None

Software

Operating System: SuSE Linux 10.1 for x86_64 Compiler: SuSE gcc,g++ 4.1 File System: Linux/ext3 System State: Multi-user SuSE Run level 3

Notes/Tuning Information

  Portability:
   255.vortex=  CPORTABILITY=-DSPEC_CPU2000_LP64
   186.crafty:  CPORTABILITY=-DLINUX_i386
   252.eon:     CXXPORTABILITY=-DHAS_ERRLIST -DSPEC_CPU2000_LP64
   253.perlbmk: CPORTABILITY=-DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
                             -DSPEC_CPU2000_LP64
   254.gap:     CPORTABILITY=-DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                             -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
                             -DSPEC_CPU2000_LP64
  Baseline C:   gcc -O3 -fno-strict-aliasing
  Baseline C++: g++ -O3
Binaries are 64 bit running on a 64 bit OS
Prefetch settings in BIOS are defaults: Hardware Prefetch: ON,
                                        Adjacent Cache Line Prefetch: OFF
The system can be built using an SSI EEB form-factor
case, and a Zippy/Emacs 700 watt PSL-6701P Power Supply.