Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro

Motherboard H8DM8-2, AMD Opteron(TM) 2220 SE

SPECint_rate2000 = SPECint_rate_base2000 = -- 79.9

SPEC license #:001176 Tested by: Supermicro Test date: Oct-2006 Hardware Avail: Sep-2006 Software Avail: Mar-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 30 60 90 120 150 164.gzip 4 91.6 70.9

175.vpr 4 100 64.9

176.gcc 4 55.0 92.7

181.mcf 4 183 45.6

186.crafty 4 54.6 85.0

197.parser 4 107 78.1

252.eon 4 59.6 101

253.perlbmk 4 95.8 87.2

254.gap 4 58.0 88.0

255.vortex 4 71.1 124

256.bzip2 4 109 63.8

300.twolf 4 164 85.1

Hardware

CPU: AMD Opteron(TM) 2220 SE processor CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 64KBI + 64KBD on chip, per core Secondary Cache: 1024KB (I+D) on chip, per core L3 Cache: N/A Other Cache: N/A Memory: 8x2048MB DDR2-667 Dual Rank CL4 ECC Reg Disk Subsystem: IDE Other Hardware: None

Software

Operating System: Windows Server 2003 Enterprise Edition SP1 (32 bit) Compiler: Intel C++ 8.0

Build 20040318Z (for 32-bit applications), Microsoft Visual Studio .Net 2003

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1= -Qprof_gen  PASS2= -Qprof_use

 Portability flags
    176.gcc:     -Dalloca=_alloca /F10000000
    186.crafty:  -DNT_i386
    253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:     -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO

 Base tuning flags
    for C programs:   -fast -arch:SSE2 -Oi- +FDO
    for C++ programs: -fast -GX -GR +FDO

 ’start /b /wait /affinity’ command is used to bind CPU(s) to processes

 Memory populated at location DIMMA 1A, DIMMA 1B, DIMMA 2A, DIMMA 2B for CPU1 and DIMMB 1A, DIMMB 1B, DIMMB 2A, DIMMB 2B for CPU2

 Tested systems can be used with SC811S-520 case,

 To ensure system stability, a 550W (minimum) ATX power supply [ 4-pin (+12V), 8-pin (+12V) and 24-pin are required]

 Product description located as of H8DM8: http://www.supermicro.com/Aplus/motherboard/Opteron2000/MCP55/H8DM8-2.cfm