Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro

Motherboard X7DB8( 2.00GHz, Intel Xeon E5335 processor)

SPECfp2000 = SPECfp_base2000 =

2107 2102

SPEC license #:001176 Tested by: Supermicro Test date: Nov-2006 Hardware Avail: Nov-2006 Software Avail: Mar-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 53.8 2976 53.7 2978

171.swim 3100 114 2722 114 2723

172.mgrid 1800 137 1309 137 1311

173.applu 2100 126 1670 126 1670

177.mesa 1400 73.6 1902 73.6 1902

178.galgel 2900 59.5 4871 59.5 4870

179.art 2600 37.2 6983 37.2 6983

183.equake 1300 49.9 2607 48.3 2689

187.facerec 1900 87.4 2173 87.5 2171

188.ammp 2200 150 1468 148 1484

189.lucas 2000 89.5 2233 89.4 2237

191.fma3d 2100 135 1556 135 1556

200.sixtrack 1100 137 802 139 792

301.apsi 2600 210 1237 210 1237

Hardware

CPU: Intel Xeon E5335 processor ( 2.00 GHz,1333MHz bus) CPU MHz: 2000 FPU: Integrated CPU(s) enabled: 4 cores, 1 chip, 4 cores/chip CPU(s) orderable: 1 chip Parallel: N/A Primary Cache: 32KBI + 32KBD on chip per core Secondary Cache: 8MB(I+D) on chip, per chip (4MB shared per 2 cores) L3 Cache: N/A Other Cache: N/A Memory: 8 X 2GB DDR2 ECC CL5 667MHz FBDIMM Disk Subsystem: 1 X Seagate Barracuda 120GB 7200 RPM Other Hardware: N/A

Software

Operating System: Windows Server 2003 Enterprise Edition 32-bits w/ SP1 Compiler: Intel C++ and Fortran Compiler 9.1 for 32-bit applications

Build 20060323Z Package ID: W_FC_P_9.1.020 Microsoft Visual Studio 2005(for libraries) SmartHeap Library Version 8.0 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning for Fortran programs:  -fast -Qansi_alias +FDO
 Base tuning for 177.mesa:  -fast    +FDO shlW32M.lib
 Base tuning for 179.art:  -fast     +FDO shlW32M.lib
 Base tuning for 183.equake:  -fast  +FDO shlW32M.lib
 Base tuning for 188.ammp:  -fast    +FDO shlW32M.lib
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -fast -Qansi_alias +FDO
 171.swim:     -fast -Qansi_alias +FDO
 172.mgrid:    -fast -Qansi_alias +FDO
 173.applu:  basepeak=yes
 177.mesa:   basepeak=yes
 178.galgel:   -fast -Qansi_alias +FDO
 179.art:      basepeak=yes
 183.equake:   -QxP -Oa -Qrcd -Qipo  +FDO  shlW32M.lib

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Supermicro

Motherboard X7DB8( 2.00GHz, Intel Xeon E5335 processor)

SPECfp2000 = SPECfp_base2000 =

2107 2102

SPEC license #:001176 Tested by: Supermicro Test date: Nov-2006 Hardware Avail: Nov-2006 Software Avail: Mar-2006

Notes/Tuning Information (Continued)

 187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     -fast -Oa +FDO  shlW32M.lib
 189.lucas:    -fast -Qprefetch- +FDO
 191.fma3d:    basepeak=yes
 200.sixtrack: -Qipo -QxP +FDO
 301.apsi:     -fast +FDO

      Tested systems can be used with SC816S-R700 case,

      To ensure system stability, a 500W (minimum) ATX power supply [4-pin (+12V), 8-pin (+12V) and 24-pin are required]

      Product description located as of http://www.supermicro.com/products/motherboard/Xeon1333/5000P/X7DB8.cfm

      The system bus runs at 1333 MHz
      shlw32m-80.lib is the V8.0 SmartHeap library renamed to co-exist with older versions