Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V830, Opteron 256, Linux 64-bit

SPECint^®2006 = 13.3

SPECint_base2006 = 11.9

CPU2006 license: 22 Test date: Apr-2006 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Sep-2005 Tested by: Fujitsu Siemens Computers Software Availability: Mar-2006

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

SPECint2006 = 13.3

SPECint_base2006 = 11.9

0 24.0

1.00 2.00 3.00 4.00 5.00 6.00 7.00 8.00 9.00 10.0 11.0 12.0 13.0 14.0 15.0 16.0 17.0 18.0 19.0 20.0 21.0 22.0

13.2

16.1

10.5

10.5

9.89

11.6

7.86

11.5

14.6

17.3

13.4

18.4

13.9

14.5

15.4

15.5

22.2

23.3

9.49

9.47

9.59

9.99

8.42

8.43

Hardware

CPU Name: AMD Opteron 256 CPU Characteristics: Opteron 256 CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2 chips Primary Cache: 64 KB I + 64 KB D on chip per chip Secondary Cache: 1 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 2 GB (4 x 512 MB PC3200 CL3-3-3 DDR SDRAM) Disk Subsystem: SCSI U320 Other Hardware: None

Software

Operating System: SuSE Linux Enterprise Server 9 (x86_64) + SP3 Compiler: QLogic Pathscale Compiler Suite 2.4 Auto Parallel: No File System: ReiserFS System State: Multi-User SuSE Run Level 3 Base Pointers: 32/64-bit Peak Pointers: 32/64-bit Other Software: --

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V830, Opteron 256, Linux 64-bit

SPECint2006 = 13.3 SPECint_base2006 = 11.9

CPU2006 license: 22 Test date: Apr-2006 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Sep-2005 Tested by: Fujitsu Siemens Computers Software Availability: Mar-2006

Results Table

Benchmark Seconds Ratio Seconds Ratio Seconds Ratio

Base Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 741 13.2 739 13.2 739 13.2 608 16.1 606 16.1 608 16.1 401.bzip2 919 10.5 921 10.5 920 10.5 921 10.5 917 10.5 919 10.5 403.gcc 814 9.89 818 9.84 814 9.89 692 11.6 693 11.6 696 11.6 429.mcf 1162 7.85 1160 7.86 1161 7.86 795 11.5 795 11.5 796 11.5 445.gobmk 719 14.6 718 14.6 719 14.6 607 17.3 607 17.3 607 17.3 456.hmmer 697 13.4 697 13.4 698 13.4 508 18.4 507 18.4 509 18.3 458.sjeng 870 13.9 870 13.9 870 13.9 832 14.5 832 14.5 832 14.5 462.libquantum 1340 15.5 1344 15.4 1342 15.4 1343 15.4 1327 15.6 1339 15.5 464.h264ref 995 22.2 995 22.2 995 22.2 949 23.3 949 23.3 950 23.3 471.omnetpp 659 9.49 659 9.48 659 9.49 657 9.51 660 9.47 662 9.45 473.astar 732 9.59 732 9.60 732 9.59 701 10.0 703 9.99 703 9.99 483.xalancbmk 820 8.42 820 8.42 819 8.42 818 8.43 823 8.38 819 8.43

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

General Notes

BIOS default settings with
Node memory interleave disabled, SRAT enabled
For information about Fujitsu Siemens Computers in your country please see:
http://www.fujitsu-siemens.com/countries

Base Compiler Invocation

C benchmarks:

pathcc

C++ benchmarks:

pathCC

Base Portability Flags

400.perlbench: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX_X64 401.bzip2: -DSPEC_CPU_LP64

403.gcc: -DSPEC_CPU_LP64 429.mcf: -DSPEC_CPU_LP64 445.gobmk: -DSPEC_CPU_LP64

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V830, Opteron 256, Linux 64-bit

SPECint2006 = 13.3

SPECint_base2006 = 11.9

CPU2006 license: 22 Test date: Apr-2006 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Sep-2005 Tested by: Fujitsu Siemens Computers Software Availability: Mar-2006

Base Portability Flags (Continued)

456.hmmer: -DSPEC_CPU_LP64

458.sjeng: -DSPEC_CPU_LP64 462.libquantum: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX 464.h264ref: -DSPEC_CPU_LP64 483.xalancbmk: -DSPEC_CPU_LINUX

Base Optimization Flags

C benchmarks:

-Ofast

C++ benchmarks:

-Ofast -m32

Peak Compiler Invocation

C benchmarks:

pathcc

C++ benchmarks:

pathCC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX_X64

401.bzip2: -DSPEC_CPU_LP64 429.mcf: -DSPEC_CPU_LP64 445.gobmk: -DSPEC_CPU_LP64 456.hmmer: -DSPEC_CPU_LP64

458.sjeng: -DSPEC_CPU_LP64 462.libquantum: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX 464.h264ref: -DSPEC_CPU_LP64 483.xalancbmk: -DSPEC_CPU_LINUX

Peak Optimization Flags

C benchmarks:

400.perlbench: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -Ofast

-IPA:plimit=525 -IPA:pu_reorder=1

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

CELSIUS V830, Opteron 256, Linux 64-bit

SPECint2006 = 13.3 SPECint_base2006 = 11.9

CPU2006 license: 22 Test date: Apr-2006 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Sep-2005 Tested by: Fujitsu Siemens Computers Software Availability: Mar-2006

Peak Optimization Flags (Continued)

401.bzip2: -O3 -LNO:ou_prod_max=10

403.gcc: -m32 -O3 -OPT:Ofast 429.mcf: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -m32 -O2

-ipa

445.gobmk: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -O3

-OPT:alias=disjoint -LNO:simd=0 -LNO:minvariant=off

456.hmmer: -O2 -OPT:alias=disjoint -WOPT:aggstr=0 -CG:cflow=0 458.sjeng: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -O3

-IPA:callee_limit=5000 -IPA:linear=on

462.libquantum: -O3 -ipa -CG:local_fwd_sched=on -IPA:space=1000 464.h264ref: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -O3

-IPA:plimit=20000 -OPT:alias=disjoint -LNO:prefetch=0

C++ benchmarks:

471.omnetpp: -Ofast -IPA:pu_reorder=2 -CG:gcm=off -m32 473.astar: -fb_create fbdata(pass 1) -fb_opt fbdata(pass 2) -Ofast 483.xalancbmk: -Ofast -m32

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090715.03.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090715.03.xml

Originally published on 24 August 2006.

Report generated on Tue Jul 22 10:00:37 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v91.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance