Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 2000

SPECfp^®2006 = -- SPECfp_base2006 = 3.67

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-2003 Tested by: Sun Microsystems Software Availability: May-2006

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

SPECfp_base2006 = 3.67

0 8.00

1.00 2.00 3.00 4.00 5.00 6.00 7.00 4.34

3.91

2.18

3.60

3.53

2.20

4.05

3.87

4.38

2.42

4.48

3.72

3.54

3.90

3.01

4.45

7.37

Hardware

CPU Name: UltraSPARC III Cu CPU Characteristics: CPU MHz: 1200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 64 KB D on chip per chip Secondary Cache: 8 MB I+D off chip per chip

Software

Operating System: Solaris 10 3/05 Compiler: Sun Studio 11 with patch 120760-03 Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: Not Applicable Other Software: None

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 2000

SPECfp2006 = -- SPECfp_base2006 = 3.67

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-2003 Tested by: Sun Microsystems Software Availability: May-2006 L3 Cache: None Other Cache: None Memory: 8 GB (4-way interleaved) Disk Subsystem: 6x36GB 10,000RPM SCSI (RAID 1+0) for SPEC

2x73GB 10,000RPM FC-AL (RAID 1) for system

Other Hardware: None

Results Table

Benchmark Seconds Ratio Seconds Ratio Seconds Ratio

Base Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 3117 4.36 3135 4.34 3135 4.34 416.gamess 5066 3.86 5008 3.91 5008 3.91 433.milc 4209 2.18 4211 2.18 4210 2.18 434.zeusmp 2494 3.65 2529 3.60 2528 3.60 435.gromacs 2021 3.53 2024 3.53 2023 3.53 436.cactusADM 5425 2.20 5425 2.20 5424 2.20 437.leslie3d 2318 4.05 2320 4.05 2319 4.05 444.namd 2070 3.87 2069 3.88 2070 3.87 447.dealII 2611 4.38 2610 4.38 2609 4.38 450.soplex 3448 2.42 3440 2.42 3534 2.36 453.povray 1183 4.50 1188 4.48 1187 4.48 454.calculix 2201 3.75 2216 3.72 2216 3.72 459.GemsFDTD 2984 3.56 3045 3.48 3001 3.54 465.tonto 2528 3.89 2523 3.90 2520 3.91 470.lbm 4569 3.01 4567 3.01 4568 3.01 481.wrf 2564 4.36 2513 4.45 2505 4.46 482.sphinx3 2644 7.37 2645 7.37 2651 7.35

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 Stack limit set to 131072

Platform Notes

 Only 1 CPU enabled in firmware
 (prior to boot)

Base Compiler Invocation

C benchmarks:

cc

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 2000

SPECfp2006 = --

SPECfp_base2006 = 3.67

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-2003 Tested by: Sun Microsystems Software Availability: May-2006

Base Compiler Invocation (Continued)

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Base Optimization Flags

C benchmarks:

-g -fast -xpagesize=4M

C++ benchmarks:

-g0 -library=stlport4 -fast -xpagesize=4M

Fortran benchmarks:

-g -fast -xpagesize=4M

Benchmarks using both Fortran and C:

-g -fast(cc) -fast(f90) -xpagesize=4M

Base Other Flags

C benchmarks:

-V

C++ benchmarks:

-verbose=version

Fortran benchmarks:

-V

Benchmarks using both Fortran and C:

-V

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/sun-studio.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/sun-studio.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 2000

SPECfp2006 = -- SPECfp_base2006 = 3.67

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-2003 Tested by: Sun Microsystems Software Availability: May-2006

Originally published on 24 August 2006.

Report generated on Tue Jul 22 10:01:13 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v89.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance