Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

SuperServer 8025C-3RB, Intel Xeon X7350

SPECfp^®_rate2006 = Not Run SPECfp_rate_base2006 = 88.0

CPU2006 license: 49 Test date: Apr-2008 Test sponsor: Advanced Micro Devices Hardware Availability: May-2007 Tested by: Advanced Micro Devices Software Availability: Mar-2008

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

Copies

SPECfp_rate_base2006 = 88.0

0 310

10.0 25.0 40.0 55.0 70.0 85.0 100 110 120 130 140 150 160 170 180 190 200 210 220 230 240 250 260 270 280 290 16 47.7 16 279 16 33.6 16 106 16 143 16 92.9 16 37.7 16 233 16 201 16 46.1 16 306 16 114 16 35.7 16 91.7 16 35.0 16 71.6 16 76.6

Hardware

CPU Name: Intel Xeon X7350 CPU Characteristics: CPU MHz: 2933 FPU: Integrated CPU(s) enabled: 16 cores, 4 chips, 4 cores/chip CPU(s) orderable: 2,4 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 8 MB I+D on chip per chip, 4 MB shared / 2 cores

Software

Operating System: SuSE Linux Enterprise Server 10 (x86_64) SP1,

Kernel 2.6.16.46-0.12-smp

Compiler: gcc, g++, gfortran 4.3.0 Auto Parallel: No File System: ext3 System State: Runlevel 3 (Full multiuser with network) Base Pointers: 64-bit Peak Pointers: Not Applicable Other Software: None

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro SuperServer 8025C-3RB, Intel Xeon X7350

SPECfp_rate2006 = Not Run SPECfp_rate_base2006 = 88.0

CPU2006 license: 49 Test date: Apr-2008 Test sponsor: Advanced Micro Devices Hardware Availability: May-2007 Tested by: Advanced Micro Devices Software Availability: Mar-2008 L3 Cache: None Other Cache: None Memory: 32 GB (16 x 2GB DDR2-667 FBDIMM CL5 Dual Rank) Disk Subsystem: 1 x 120 GB SATA, 7200 RPM Other Hardware: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 16 4624 47.0 4557 47.7 4534 48.0 416.gamess 16 1122 279 1121 280 1123 279 433.milc 16 4379 33.5 4367 33.6 4362 33.7 434.zeusmp 16 1380 106 1377 106 1385 105 435.gromacs 16 796 143 794 144 796 143 436.cactusADM 16 2062 92.7 2057 92.9 2055 93.1 437.leslie3d 16 4032 37.3 3988 37.7 3986 37.7 444.namd 16 550 233 549 234 550 233 447.dealII 16 915 200 911 201 883 207 450.soplex 16 2913 45.8 2897 46.1 2894 46.1 453.povray 16 280 305 278 306 277 308 454.calculix 16 1155 114 1155 114 1161 114 459.GemsFDTD 16 4749 35.7 4757 35.7 4783 35.5 465.tonto 16 1901 82.8 1713 91.9 1718 91.7 470.lbm 16 6362 34.6 6284 35.0 6279 35.0 481.wrf 16 2553 70.0 2465 72.5 2497 71.6 482.sphinx3 16 4093 76.2 4069 76.6 4073 76.6

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 ’numactl’ was used to bind copies to the cores

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Fortran benchmarks:

gfortran

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

SuperServer 8025C-3RB, Intel Xeon X7350

SPECfp_rate2006 = Not Run

SPECfp_rate_base2006 = 88.0

CPU2006 license: 49 Test date: Apr-2008 Test sponsor: Advanced Micro Devices Hardware Availability: May-2007 Tested by: Advanced Micro Devices Software Availability: Mar-2008

Base Compiler Invocation (Continued)

Benchmarks using both Fortran and C:

gcc gfortran

Base Portability Flags

410.bwaves: -DSPEC_CPU_LP64 416.gamess: -DSPEC_CPU_LP64

433.milc: -DSPEC_CPU_LP64 434.zeusmp: -DSPEC_CPU_LP64 435.gromacs: -DSPEC_CPU_LP64 436.cactusADM: -DSPEC_CPU_LP64

437.leslie3d: -DSPEC_CPU_LP64

444.namd: -DSPEC_CPU_LP64 447.dealII: -DSPEC_CPU_LP64 450.soplex: -DSPEC_CPU_LP64 453.povray: -DSPEC_CPU_LP64 454.calculix: -DSPEC_CPU_LP64 459.GemsFDTD: -DSPEC_CPU_LP64

465.tonto: -DSPEC_CPU_LP64 470.lbm: -DSPEC_CPU_LP64 481.wrf: -DSPEC_CPU_LP64 -DSPEC_CPU_LINUX -DSPEC_CPU_CASE_FLAG 482.sphinx3: -DSPEC_CPU_LP64

Base Optimization Flags

C benchmarks:

-O3 -funroll-loops -fno-strict-aliasing

C++ benchmarks:

-O3 -funroll-loops -fno-strict-aliasing

Fortran benchmarks:

-O3 -funroll-loops -fno-strict-aliasing

Benchmarks using both Fortran and C:

-O3 -funroll-loops -fno-strict-aliasing

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090713.05.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/CPU2006_flags.20090713.05.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

(Test Sponsor: Advanced Micro Devices)

Supermicro

SuperServer 8025C-3RB, Intel Xeon X7350

SPECfp_rate2006 = Not Run SPECfp_rate_base2006 = 88.0

CPU2006 license: 49 Test date: Apr-2008 Test sponsor: Advanced Micro Devices Hardware Availability: May-2007 Tested by: Advanced Micro Devices Software Availability: Mar-2008

Originally published on 5 August 2008.

Report generated on Tue Jul 22 18:49:19 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance