Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp^®_rate2006 = 270

SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

Copies

SPECfp_rate2006 = 270

SPECfp_rate_base2006 = 254

0 440

15.0 35.0 55.0 75.0 95.0 110 125 140 155 170 185 200 215 230 245 260 275 290 305 320 335 350 365 380 395 410 255 310 255 310

255 236 255 236

255 355 255 355

255 318

255 219 255 224

255 236

255 214 192 225

255 248 255 248

255 426

255 241

255 313 255 430

255 177 255 178

255 202 255 204

255 260 224 287

255 124 32 202

255 284 255 289

255 319 255 323

Hardware

CPU Name: UltraSPARC T2 Plus CPU Characteristics: CPU MHz: 1596 FPU: Integrated CPU(s) enabled: 32 cores, 4 chips, 8 cores/chip, 8 threads/core CPU(s) orderable: 1 to 4 chips Primary Cache: 16 KB I + 8 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip

Software

Operating System: Solaris 10 5/09 Compiler: Sun Studio 12 Update 1 Auto Parallel: No File System: zfs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270 SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009 L3 Cache: None Other Cache: None Memory: 256 GB (64 x 4 GB) Disk Subsystem: 536 GB using ZFS 3-way mirroring on 24x 15K SUN72G FC (on 2x SE3510) Other Hardware: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 255 11053 314 11297 307 11190 310 255 11189 310 11180 310 11215 309 416.gamess 255 21186 236 21187 236 21151 236 255 21153 236 21163 236 21177 236 433.milc 255 6600 355 6606 354 6602 355 255 6597 355 6594 355 6593 355 434.zeusmp 255 7258 320 7311 317 7289 318 255 7258 320 7311 317 7289 318 435.gromacs 255 8326 219 8304 219 8314 219 255 8153 223 8102 225 8125 224 436.cactusADM 255 12910 236 12921 236 12895 236 255 12910 236 12921 236 12895 236 437.leslie3d 255 11238 213 11227 214 11218 214 192 8032 225 7978 226 8043 224 444.namd 255 8233 248 8207 249 8285 247 255 8191 250 8236 248 8231 248 447.dealII 255 6839 427 6842 426 6858 425 255 6839 427 6842 426 6858 425 450.soplex 255 8989 237 8834 241 8827 241 255 8989 237 8834 241 8827 241 453.povray 255 4336 313 4042 336 5064 268 255 3178 427 3110 436 3152 430 454.calculix 255 11846 178 11885 177 11883 177 255 11837 178 11826 178 11831 178 459.GemsFDTD 255 13373 202 13272 204 13423 202 255 13276 204 13227 205 13385 202 465.tonto 255 9630 261 9634 260 9634 260 224 7670 287 7668 287 7659 288 470.lbm 255 28328 124 28242 124 28409 123 32 2176 202 2177 202 2177 202 481.wrf 255 10036 284 10046 284 10009 285 255 9869 289 9860 289 9867 289 482.sphinx3 255 15558 319 15571 319 15583 319 255 15349 324 15371 323 15368 323

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Invocation Notes

 Sun Studio 12 Update 1 pre-release build 41.1 was used.

Submit Notes

 A processor set was created using
   psrset -c 1-255
 and the runspec process was placed into the set using
   psrset -e 1
 The config file option ’submit’ was used to select specific
 processors within the set, along with the pbind command.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270

SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Operating System Notes

 ulimit -s 131072 was used to allow the stack to grow
 up to 131072 KB (aka 128 MB).  Note that saying "131072"
 is preferable to "unlimited", because there is a tradeoff
 between space for the stack vs. space for the heap.

 /etc/system parameters
    autoup=600
       Causes pages older than the listed number of seconds to
       be written by fsflush.
    tune_t_fsflushr=10
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush.
    tsb_rss_factor=128
       Suggests that the the size of the TSB (Translation Storage Buffer)
       may be increased if it is more than 25% (128/512) full.  Doing so
       may reduce TSB traps, at the cost of additional kernel memory.
    zfs:zfs_arc_max = 0x10000000
       Limits the consumption of memory by the zfs file system

 The "webconsole" service was turned off using
     svcadm disable webconsole

 The system had 229 GB of swap space.

Platform Notes

 This result was measured on a Sun SPARC Enterprise T5440.
 The Sun SPARC Enterprise T5440 and the Fujitsu SPARC
 Enterprise T5440 are electrically equivalent.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270

SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Base Optimization Flags

C benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2 -xalias_level=std
-xprefetch_level=3 -xprefetch_auto_type=indirect_array_access
-M /usr/lib/ld/map.bssalign

C++ benchmarks:

-g0 -library=stlport4 -fast -xipo=2 -xpagesize=4M -xprefetch_level=2
-xdepend -xalias_level=compatible -M /usr/lib/ld/map.bssalign

Fortran benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2
-M /usr/lib/ld/map.bssalign

Benchmarks using both Fortran and C:

-g -fast(cc) -fast(f90) -xipo=2 -xpagesize=4M -xprefetch_level=2
-xalias_level=std -xprefetch_level=3
-xprefetch_auto_type=indirect_array_access -M /usr/lib/ld/map.bssalign

Base Other Flags

C benchmarks:

-xjobs=32 -V -#

C++ benchmarks:

-xjobs=32 -verbose=diags,version

Fortran benchmarks:

-xjobs=32 -V -v

Benchmarks using both Fortran and C:

-xjobs=32 -V -# -v

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270

SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Peak Optimization Flags

C benchmarks:

433.milc: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xipo=2 -xprefetch_level=2
-xprefetch_auto_type=indirect_array_access -xalias_level=std
-fsimple=1

470.lbm: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xprefetch_level=3 -xipo=2
-xrestrict

482.sphinx3: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xinline= -xprefetch_level=2
-Wc,-Qlp-ol=1 -xrestrict -xalias_level=strong -fsimple=1
-xlinkopt=2 -lfast

C++ benchmarks:

444.namd: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xdepend -xalias_level=compatible
-M /usr/lib/ld/map.bssalign -xprefetch_level=1 -xlinkopt=2

447.dealII: basepeak = yes

450.soplex: basepeak = yes

453.povray: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=64K
-xdepend -xalias_level=compatible -xipo=2 -xrestrict
-xlinkopt=2

Fortran benchmarks:

410.bwaves: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xipo=2 -xprefetch_level=2

416.gamess: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-M /usr/lib/ld/map.bssalign -xlinkopt=2

434.zeusmp: basepeak = yes

437.leslie3d: -g -fast -xpagesize_heap=4M -xpagesize_stack=64K

-M /usr/lib/ld/map.bssalign -xprefetch_level=3
-xprefetch=latx:1.6 -qoption cg -Qlp=1 -qoption cg -Qlp-fa=0
-qoption cg -Qlp-fl=1 -qoption cg -Qlp-av=448

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270 SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Peak Optimization Flags (Continued)

437.leslie3d (continued):

-qoption cg -Qlp-t=4

459.GemsFDTD: -g -fast -xpagesize=4M -M /usr/lib/ld/map.bssalign

-fsimple=1

465.tonto: -g -fast -xpagesize=4M -M /usr/lib/ld/map.bssalign -xipo=2

-lfast

Benchmarks using both Fortran and C:

435.gromacs: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xipo=1 -xinline=
-xarch=generic -xchip=generic -fsimple=0

436.cactusADM: basepeak = yes

454.calculix: -g -fast(cc) -fast(f90) -xpagesize=4M

-M /usr/lib/ld/map.bssalign -xipo=2 -xvector
-xprefetch_level=1

481.wrf: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xlinkopt=2

Peak Other Flags

C benchmarks:

-xjobs=32 -V -#

C++ benchmarks:

-xjobs=32 -verbose=diags,version

Fortran benchmarks:

-xjobs=32 -V -v

Benchmarks using both Fortran and C:

-xjobs=32 -V -# -v

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-12u1-and-gccfss4.2.r3.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-12u1-and-gccfss4.2.r3.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 7 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Fujitsu SPARC Enterprise T5440

SPECfp_rate2006 = 270 SPECfp_rate_base2006 = 254

CPU2006 license: 6 Test date: May-2009 Test sponsor: Fujitsu Hardware Availability: Jul-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Originally published on 5 August 2009.

Report generated on Wed Jul 23 03:24:01 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance