Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

503.bwaves_r

507.cactuBSSN_r

508.namd_r

510.parest_r

511.povray_r

519.lbm_r

521.wrf_r

526.blender_r

527.cam4_r

538.imagick_r

544.nab_r

549.fotonik3d_r

554.roms_r

Copies

(118)

SPECrate^®2017_fp_peak

(111)

SPECrate^®2017_fp_base

0 270

15.0 30.0 45.0 60.0 75.0 90.0 105 120 135 150 165 180 195 210 225 240 255 224 268 224 137 192 142 224 110 256 110 224 52.7 256 54.6 224 146 256 172 224 64.8 256 77.3 224 103 104 224 142 256 163 224 114 160 114 224 127 133 224 181 256 201 224 112 224 42.9 32 50.9

Hardware

CPU Name: SPARC M7 Max MHz: 4133 Nominal: 4133 Enabled: 32 cores, 1 chip, 8 threads/core Orderable: 1-16 CMIOU (on host) Cache L1: 16 KB I + 16 KB D on chip per core L2: 2 MB I on chip per chip (256 KB / 4 cores); 4 MB D on chip per chip (256 KB / 2 cores) L3: 64 MB I+D on chip per chip (8 MB / 4 cores) Other: None Memory: 480 GB (16 x 32 GB 2Rx4 PC4-2400T-L, running at 2133, 16-way interleaved) Storage: 2.4 TB on 16 x 300 GB 10K RPM SAS disks served via COMSTAR over 8 Gb/s Fibre Channel from a Sun Fire X4270M2, arranged as 8 x 2-way mirrors

Software

OS: Oracle Solaris 11.3.10.5.0 Compiler: C/C++/Fortran: Version 12.5 of Oracle Developer

Studio

Parallel: No Firmware: Sun System Firmware 9.5.2.g File System: zfs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other: None Power Management: --

(Continued on next page)

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Hardware (Continued)

Other: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

503.bwaves_r 224 8372 268 8376 268 224 8372 268 8376 268 507.cactuBSSN_r 224 2063 137 2069 137 192 1699 143 1710 142 508.namd_r 224 1930 110 1931 110 256 2203 110 2197 111 510.parest_r 224 11127 52.7 11123 52.7 256 12259 54.6 12263 54.6 511.povray_r 224 3565 147 3585 146 256 3466 172 3464 173 519.lbm_r 224 3601 65.6 3645 64.8 256 3484 77.5 3489 77.3 521.wrf_r 224 4886 103 4882 103 224 4815 104 4817 104 526.blender_r 224 2394 142 2388 143 256 2388 163 2386 163 527.cam4_r 224 3446 114 3444 114 160 2459 114 2456 114 538.imagick_r 224 4388 127 4391 127 224 4202 133 4201 133 544.nab_r 224 2080 181 2080 181 256 2144 201 2146 201 549.fotonik3d_r 224 7824 112 7825 112 224 7824 112 7825 112 554.roms_r 224 8299 42.9 8298 42.9 32 995 51.1 999 50.9 SPECrate^®2017_fp_base = 111 SPECrate^®2017_fp_peak = 118

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

The config file option ’submit’ was used.

Operating System Notes

 The ZFS cache was limited to 12% of memory, and the
 fsflush daemon was told to run once every 10 seconds,
 checking for dirty pages more than 10 minutes old,
 using these settings in /etc/system:
 set user_reserve_hint_pct=88
 set autoup=600
 set tune_t_fsflushr=10

Platform Notes

   The System Under Test (SUT),
   "1-chip VM with SPARC M7",
   contains:
    - 1 physical CPU chip
    - 256 virtual CPUs

(Continued on next page)

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Platform Notes (Continued)

    - 32 cores
    - 480 GB memory
    - OS: Oracle Solaris 11.3.10.5.0

   The SUT is managed by a HOST with:
    - OS: Oracle Solaris 11.3.5.1.0
    - Oracle VM Server for SPARC v3.3
      (included with Oracle Solaris)
   From the standpoint of the HOST, the SUT is:
    - A Logical Domain (LDom)
    - One CMIOU (CPU, Memory, IO unit), containing:
      - 1 SPARC M7 chip
      - 16x 32 GB memory DIMMs
        - 1x DIMM is reserved
        - Therefore the SUT sees 480 GB, not 512

   The HOST is part of an M7-16 server that has:
     - Sun System Firmware 9.5.2.g 2015/12/07 11:57
     - 16x CMIOUs
     - 4x Domain Configurable Units (DCUs)
        - Each DCU has 4x CMIOUs
        - Each DCU is a Physical Domain (PDom)
   From the standpoint of the M7-16, the HOST
   is one PDom containing one DCU.

   Additional information about SUT, LDom, and
   PDom commands are in the platform flags file.

   For Oracle VM Server information, see
   Oracle Technical Network (OTN)

 Sysinfo program /cpu2017/rc3/Docs/sysinfo
 Rev: r4961 of 2016-10-02 93f3ce875d5c7794a1fec4785739b79b
 running on m7-16-002c-ld3 Wed Oct 19 12:37:15 2016

 This section contains SUT (System Under Test) info as seen by
 some common utilities.  To remove or add to this section, see:
   http://www.spec.org/cpu2017/Docs/config.html#sysinfo

 From /usr/sbin/psrinfo
    SPARC-M7 (chipid 3, clock 4133 MHz)
    1 chips
    256 threads
    4133 MHz

 From kstat:       32 cores

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Platform Notes (Continued)

 From prtconf: 489984 Megabytes

 /etc/release:
      Oracle Solaris 11.3 SPARC
 uname -a:
    SunOS m7-16-002c-ld3 5.11 11.3 sun4v sparc sun4v

 disk: df -h /cpu2017/rc3
 Filesystem             Size   Used  Available Capacity  Mounted on
 spec/cpu2017/rc3       2.4T   1.2G       1.7T     1%    /cpu2017/rc3

 (End of data from sysinfo program)

Compiler Version Notes

==============================================================================
C               | 519.lbm_r(base, peak) 538.imagick_r(base, peak)
                | 544.nab_r(base, peak)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++             | 508.namd_r(base, peak) 510.parest_r(base, peak)
------------------------------------------------------------------------------
CC: Studio 12.5 Sun C++ 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C          | 507.cactuBSSN_r(base pass 0, peak pass 0) 511.povray_r(base
                | pass 0, base pass 0, peak pass 1, peak pass 1, peak pass 2,
                | peak pass 2) 526.blender_r(base pass 0, base pass 0, peak
                | pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
CC: Studio 12.5 Sun C++ 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C          | 511.povray_r(base pass 0, base pass 0, peak pass 1, peak
                | pass 1, peak pass 2, peak pass 2) 526.blender_r(base pass
                | 0, base pass 0, peak pass 1, peak pass 1, peak pass 2, peak
                | pass 2)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Compiler Version Notes (Continued)

==============================================================================
C++, C          | 507.cactuBSSN_r(base pass 0, peak pass 0) 511.povray_r(base
                | pass 0, base pass 0, peak pass 1, peak pass 1, peak pass 2,
                | peak pass 2) 526.blender_r(base pass 0, base pass 0, peak
                | pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
CC: Studio 12.5 Sun C++ 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C          | 511.povray_r(base pass 0, base pass 0, peak pass 1, peak
                | pass 1, peak pass 2, peak pass 2) 526.blender_r(base pass
                | 0, base pass 0, peak pass 1, peak pass 1, peak pass 2, peak
                | pass 2)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
f90: Studio 12.5 Fortran 95 8.8 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
f90: Studio 12.5 Fortran 95 8.8 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
Fortran         | 503.bwaves_r(base, peak) 549.fotonik3d_r(base, peak)
                | 554.roms_r(base, peak)
------------------------------------------------------------------------------
f90: Studio 12.5 Fortran 95 8.8 SunOS_sparc 2016/05/31

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Compiler Version Notes (Continued)

------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
f90: Studio 12.5 Fortran 95 8.8 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
cc: Studio 12.5 Sun C 5.14 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
f90: Studio 12.5 Fortran 95 8.8 SunOS_sparc 2016/05/31
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f95

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Base Compiler Invocation (Continued)

Benchmarks using both Fortran and C:

f95 cc

Benchmarks using both C and C++:

CC cc

Benchmarks using Fortran, C, and C++:

CC cc f95

Base Portability Flags

503.bwaves_r: -D_FILE_OFFSET_BITS=64 507.cactuBSSN_r: -DSPEC_NO_C99_MATH_IN_CXX -D_FILE_OFFSET_BITS=64 508.namd_r: -D_FILE_OFFSET_BITS=64 510.parest_r: -D_FILE_OFFSET_BITS=64 511.povray_r: -D_FILE_OFFSET_BITS=64 519.lbm_r: -D_FILE_OFFSET_BITS=64 521.wrf_r: -D_FILE_OFFSET_BITS=64 526.blender_r: -xchar=u -DSPEC_NO_ISFINITE -D_FILE_OFFSET_BITS=64 527.cam4_r: -D_FILE_OFFSET_BITS=64 538.imagick_r: -D_FILE_OFFSET_BITS=64 544.nab_r: -D_FILE_OFFSET_BITS=64 549.fotonik3d_r: -D_FILE_OFFSET_BITS=64 554.roms_r: -D_FILE_OFFSET_BITS=64

Base Optimization Flags

C benchmarks:

-m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast -xipo=2
-xthroughput=yes -xalias_level=std -g1 -lfast

C++ benchmarks:

-m32 -xpagesize=4M -std=c++03 -DSPEC_SUPPRESS_OPENMP -fast -xipo=2
-xthroughput=yes -xalias_level=compatible -g -lfast

Fortran benchmarks:

-m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast -xipo=2
-xthroughput=yes -g1 -lfast

Benchmarks using both Fortran and C:

-m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast(cc) -fast(f95)
-xipo=2 -xthroughput=yes -xalias_level=std -g1 -lfast

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Base Optimization Flags (Continued)

Benchmarks using both C and C++:

-m32 -std=c++03 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast(CC)
-fast(cc) -xipo=2 -xthroughput=yes -xalias_level=std
-xalias_level=compatible -g1 -g -lfast

Benchmarks using Fortran, C, and C++:

-m32 -xpagesize=4M -std=c++03 -DSPEC_SUPPRESS_OPENMP -fast(CC)
-fast(cc) -fast(f95) -xipo=2 -xthroughput=yes -xalias_level=std
-xalias_level=compatible -g1 -g -lfast

Base Other Flags

C benchmarks:

-xjobs=64 -errfmt

C++ benchmarks:

-xjobs=64

Fortran benchmarks:

-xjobs=64

Benchmarks using both Fortran and C:

-xjobs=64 -errfmt

Benchmarks using both C and C++:

-xjobs=64 -errfmt

Benchmarks using Fortran, C, and C++:

-xjobs=64 -errfmt

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f95

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Peak Compiler Invocation (Continued)

Benchmarks using both Fortran and C:

f95 cc

Benchmarks using both C and C++:

CC cc

Benchmarks using Fortran, C, and C++:

CC cc f95

Peak Portability Flags

Same as Base Portability Flags

Peak Optimization Flags

C benchmarks:

519.lbm_r: -m32 -xpagesize=256M -DSPEC_SUPPRESS_OPENMP -fast

-xipo=2 -xthroughput=yes -xprefetch_level=2
-xprefetch=latx:3 -xalias_level=std -g1

538.imagick_r: -m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast

-xthroughput=yes -xprefetch_level=2 -xalias_level=std
-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1 -lfast

544.nab_r: -m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast -xipo=2

-xthroughput=yes -xalias_level=std
-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1

C++ benchmarks:

508.namd_r: -m32 -xpagesize=4M -std=c++03 -DSPEC_SUPPRESS_OPENMP

-fast -xipo=1 -xthroughput=yes -xalias_level=compatible
-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g

510.parest_r: -m32 -xpagesize=256M -std=c++03 -DSPEC_SUPPRESS_OPENMP

-fast -xipo=2 -xprefetch=no%auto -xalias_level=compatible

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Peak Optimization Flags (Continued)

510.parest_r (continued):

-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g

Fortran benchmarks:

503.bwaves_r: basepeak = yes

549.fotonik3d_r: basepeak = yes

554.roms_r: -m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast

-xprefetch_level=2 -xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1

Benchmarks using both Fortran and C:

521.wrf_r: -m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast(cc)

-fast(f95) -xthroughput=yes -xprefetch_level=3
-xalias_level=std -xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1

527.cam4_r: -m32 -xpagesize=4M -DSPEC_SUPPRESS_OPENMP -fast(cc)

-fast(f95) -xthroughput=yes -xprefetch_level=2
-xalias_level=std -xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1 -lfast

Benchmarks using both C and C++:

511.povray_r: -library=stdcxx4 -xpagesize_heap=256M -m32

-xpagesize_stack=4M -template=extdef -std=sun03
-DSPEC_SUPPRESS_OPENMP -fast(CC) -fast(cc) -xipo=1
-xthroughput=yes -xalias_level=std
-xalias_level=compatible
-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1 -g

526.blender_r: -library=stlport4 -std=sun03 -m32 -xpagesize=256M

-DSPEC_SUPPRESS_OPENMP -fast(CC) -fast(cc) -xipo=2
-xprofile=collect:./feedback(pass 1)
-xprofile=use:./feedback(pass 2) -g1 -g

Benchmarks using Fortran, C, and C++:

-m32 -xpagesize=256M -std=c++03 -DSPEC_SUPPRESS_OPENMP -fast(CC)
-fast(cc) -fast(f95) -xipo=2 -g1 -g

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

Oracle Corporation 1-Chip VM with SPARC M7 SPECrate^®2017_fp_peak = 118

SPECrate^®2017_fp_base = 111

CPU2017 License: 6 Test Date: Oct-2016 Test Sponsor: Oracle Corporation Hardware Availability: Oct-2015 Tested by: Oracle Corporation Software Availability: Jul-2016

Peak Other Flags

C benchmarks:

-xjobs=64 -errfmt

C++ benchmarks:

-xjobs=64

Fortran benchmarks:

-xjobs=64

Benchmarks using both Fortran and C:

-xjobs=64 -errfmt

Benchmarks using both C and C++:

-xjobs=64 -errfmt

Benchmarks using Fortran, C, and C++:

-xjobs=64 -errfmt

The flags files that were used to format this result can be browsed at

http://www.spec.org/cpu2017/flags/Oracle-Solaris-Studio12.5.html
http://www.spec.org/cpu2017/flags/Oracle-SPARC.html

You can also download the XML flags sources by saving the following links:

http://www.spec.org/cpu2017/flags/Oracle-Solaris-Studio12.5.xml
http://www.spec.org/cpu2017/flags/Oracle-SPARC.xml

Originally published on 2017-06-19.

Report generated on 2020-01-15 19:45:03 by CPU2017 PS formatter v6255.

Tested with SPEC CPU^®2017 v0.903.0 on 2016-10-19 15:37:10-0400.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

names appearing in this result are trademarks or registered trademarks of their respective holders.

SPEC CPU and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and product