Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

503.bwaves_r 507.cactuBSSN_r

508.namd_r 510.parest_r 511.povray_r 519.lbm_r 521.wrf_r 526.blender_r 527.cam4_r 538.imagick_r

544.nab_r 549.fotonik3d_r

554.roms_r

Copies

(501)

SPECrate^®2017_fp_base

0 1200

50.0 100 150 200 250 300 350 400 450 500 550 600 650 700 750 800 850 900 950 1050

256^{1150} 256^{518} 256^{620} 256^{304} 256^{1020} 256^{137} 256^{494} 256^{824} 256^{456} 256^{953} 256^{559} 256^{331} 256^{246}

Hardware

CPU Name: Huawei Kunpeng 920 7260 Max MHz: 2600 Nominal: 2600 Enabled: 256 cores, 4 chips Orderable: 1,2,3,4 chips Cache L1: 64 KB I + 64 KB D on chip per core L2: 512 KB I+D on chip per core L3: 64 MB I+D on chip per chip Other: None Memory: 1 TB (32 x 32 GB 2Rx4 PC4-2933Y-R) Storage: 1 x 960 GB SAS SSD Other: None

Software

OS: kylin release 10 (Azalea) 4.19.90-5.ky10.aarch64 Compiler: C/C++/Fortran: Version 9.1.0 of GCC, the GNU Compiler Collection Parallel: No Firmware: Huawei Corp. Version 1.20 released Apr-2020 File System: xfs System State: Run level 5 (multi-user graphical) Base Pointers: 64-bit Peak Pointers: Not Applicable Other: None Power Management:^{BIOS set to prefer performance at the cost of additional power usage}

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

503.bwaves_r 256 2258 1140 2225 1150 2235 1150 507.cactuBSSN_r 256 638 508 626 518 623 521 508.namd_r 256 392 621 392 620 393 618 510.parest_r 256 2204 304 2202 304 2202 304 511.povray_r 256 586 1020 588 1020 590 1010 519.lbm_r 256 1970 137 1970 137 1971 137 521.wrf_r 256 1165 492 1161 494 1160 494 526.blender_r 256 473 824 473 824 473 824 527.cam4_r 256 964 464 1002 447 981 456 538.imagick_r 256 665 957 668 953 668 953 544.nab_r 256 769 560 771 559 772 558 549.fotonik3d_r 256 3017 331 3045 328 2878 347 554.roms_r 256 1655 246 1655 246 1679 242

SPECrate^®2017_fp_base = 501 SPECrate^®2017_fp_peak = Not Run

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

 The taskset mechanism was used to bind copies to processors. The config file option ’submit’
 was used to generate taskset commands to bind each copy to a specific processor.
 For details, please see the config file.

Operating System Notes

 Stack size set to unlimited using "ulimit -s unlimited"

Environment Variables Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH =
     "/usr/local/gcc-9.1.0/lib64/:/usr/local/gcc-9.1.0/lib/:/lib64:"

General Notes

Transparent Huge Pages enabled by default
Prior to runcpu invocation
Filesystem page cache synced and cleared with:
sync; echo 3>       /proc/sys/vm/drop_caches
NA: The test sponsor attests, as of date of publication, that CVE-2017-5754 (Meltdown)

(Continued on next page)

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

General Notes (Continued)

is mitigated in the system as tested and documented.
Yes: The test sponsor attests, as of date of publication, that CVE-2017-5753 (Spectre variant 1)
is mitigated in the system as tested and documented.
NA: The test sponsor attests, as of date of publication, that CVE-2017-5715 (Spectre variant 2)
is mitigated in the system as tested and documented.

Platform Notes

 BIOS configuration:
 Power Policy Set to Performance
 Custom Refresh Rate Set to 64ms
 CPU Prefetcher Set to Enabled
 L3 Cache Model Set to in :private out:private

 Sysinfo program /home/cpu2017/bin/sysinfo
 Rev: r6365 of 2019-08-21 295195f888a3d7edb1e6e46a485a0011
 running on localhost.localdomain Sun Jun 21 10:31:05 2020

 SUT (System Under Test) info as seen by some common utilities.
 For more information on this section, see
    https://www.spec.org/cpu2017/Docs/config.html#sysinfo

 From /proc/cpuinfo
 *
 * Did not identify cpu model.  If you would
 * like to write your own sysinfo program, see
 * www.spec.org/cpu2017/config.html#sysinfo
 *
 *
 * 0 "physical id" tags found.  Perhaps this is an older system,
 * or a virtualized system.  Not attempting to guess how to
 * count chips/cores for this system.
 *
       256 "processors"
    cores, siblings (Caution: counting these is hw and system dependent. The following
    excerpts from /proc/cpuinfo might not be reliable.  Use with caution.)

 From lscpu:
      Architecture:                    aarch64
      CPU op-mode(s):                  64-bit
      Byte Order:                      Little Endian
      CPU(s):                          256
      On-line CPU(s) list:             0-255
      Thread(s) per core:              1
      Core(s) per socket:              64
      Socket(s):                       4

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Platform Notes (Continued)

      NUMA node(s):                    8
      Vendor ID:                       HiSilicon
      Model:                           0
      Model name:                      Kunpeng-920
      Stepping:                        0x1
      BogoMIPS:                        200.00
      L1d cache:                       16 MiB
      L1i cache:                       16 MiB
      L2 cache:                        128 MiB
      L3 cache:                        512 MiB
      NUMA node0 CPU(s):               0-31
      NUMA node1 CPU(s):               32-63
      NUMA node2 CPU(s):               64-95
      NUMA node3 CPU(s):               96-127
      NUMA node4 CPU(s):               128-159
      NUMA node5 CPU(s):               160-191
      NUMA node6 CPU(s):               192-223
      NUMA node7 CPU(s):               224-255
      Vulnerability Itlb multihit:     Not affected
      Vulnerability L1tf:              Not affected
      Vulnerability Mds:               Not affected
      Vulnerability Meltdown:          Not affected
      Vulnerability Spec store bypass: Mitigation; Speculative Store Bypass disabled via
      prctl
      Vulnerability Spectre v1:        Mitigation; __user pointer sanitization
      Vulnerability Spectre v2:        Not affected
      Vulnerability Tsx async abort:   Not affected
      Flags:                           fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics
      fphp asimdhp cpuid asimdrdm jscvt fcma dcpop asimddp asimdfhm ssbs

 From numactl --hardware  WARNING: a numactl ’node’ might or might not correspond to a
 physical chip.

 From /proc/meminfo
    MemTotal:       1071619840 kB
    HugePages_Total:   100000
    Hugepagesize:       2048 kB

 From /etc/*release* /etc/*version*
    kylin-release: kylin release 10 (Azalea)
    os-release:
       NAME="kylin"
       VERSION="10 (Azalea)"
       ID="kylin"
       VERSION_ID="10"
       PRETTY_NAME="kylin 10 (Azalea)"
       ANSI_COLOR="0;31"

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Platform Notes (Continued)

    system-release: kylin release 10 (Azalea)
    system-release-cpe: cpe:/o:kylin:kylin:10:ga:server

 uname -a:
    Linux localhost.localdomain 4.19.90-5.ky10.aarch64 #1 SMP Wed Apr 8 09:34:13 CST 2020
    aarch64 aarch64 aarch64 GNU/Linux

 Kernel self-reported vulnerability status:

 itlb_multihit:                            Not affected
 CVE-2018-3620 (L1 Terminal Fault):        Not affected
 Microarchitectural Data Sampling:         Not affected
 CVE-2017-5754 (Meltdown):                 Not affected
 CVE-2018-3639 (Speculative Store Bypass): Mitigation: Speculative Store Bypass disabled
                                           via prctl
 CVE-2017-5753 (Spectre variant 1):        Mitigation: __user pointer sanitization
 CVE-2017-5715 (Spectre variant 2):        Not affected
 tsx_async_abort:                          Not affected

 run-level 5 Jun 19 18:13

 SPEC is set to: /home/cpu2017
    Filesystem              Type  Size  Used Avail Use% Mounted on
    /dev/mapper/klas00-home xfs   838G   18G  821G   3% /home

 From /sys/devices/virtual/dmi/id
     BIOS:    Huawei Corp. 1.20 04/14/2020
     Vendor:  Huawei
     Product: TaiShan 200 (Model 2480)
     Serial:  2102312UXX10KC000007

 Additional information from dmidecode follows.  WARNING: Use caution when you interpret
 this section. The ’dmidecode’ program reads system data which is "intended to allow
 hardware to be accurately determined", but the intent may not be met, as there are
 frequent changes to hardware, firmware, and the "DMTF SMBIOS" standard.
   Memory:
     32x Hynix HMA84GR7CJR4N-WM 32 GB 2 rank 2933

 (End of data from sysinfo program)
The sysinfo is missing the cpu name, the processor under test is Huawei Kunpeng 920 7260.
The L3 capacity is 64MB per processor for Huawei Kunpeng 920 7260 processor for a SUT
total of 256 MiB.

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Compiler Version Notes

==============================================================================
C               | 519.lbm_r(base) 538.imagick_r(base) 544.nab_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gcc
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

==============================================================================
C++             | 508.namd_r(base) 510.parest_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/g++
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

==============================================================================
C++, C          | 511.povray_r(base) 526.blender_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/g++
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gcc
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Compiler Version Notes (Continued)

Thread model: posix
gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/g++
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gcc
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gfortran
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

==============================================================================
Fortran         | 503.bwaves_r(base) 549.fotonik3d_r(base) 554.roms_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gfortran
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Compiler Version Notes (Continued)

gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base) 527.cam4_r(base)
------------------------------------------------------------------------------
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gfortran
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
Using built-in specs.
COLLECT_GCC=/usr/local/gcc-9.1.0/bin/gcc
COLLECT_LTO_WRAPPER=/usr/local/gcc-9.1.0/libexec/gcc/aarch64-unknown-linux-gnu/9.1.0/lto-wrapper
Target: aarch64-unknown-linux-gnu
Configured with: ../configure --enable-checking=release
  --enable-languages=c,c++,fortran --disable-multilib
  --prefix=/usr/local/gcc-9.1.0
Thread model: posix
gcc version 9.1.0 (GCC)
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Fortran benchmarks:

gfortran

Benchmarks using both Fortran and C:

gfortran gcc

Benchmarks using both C and C++:

g++ gcc

Benchmarks using Fortran, C, and C++:

g++ gcc gfortran

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

Base Portability Flags

503.bwaves_r: -DSPEC_LP64 507.cactuBSSN_r: -DSPEC_LP64 508.namd_r: -DSPEC_LP64 510.parest_r: -DSPEC_LP64 511.povray_r: -DSPEC_LP64 519.lbm_r: -DSPEC_LP64 521.wrf_r: -DSPEC_CASE_FLAG -fconvert=big-endian -DSPEC_LP64 526.blender_r: -funsigned-char -DSPEC_LINUX -DSPEC_LP64 527.cam4_r: -DSPEC_CASE_FLAG -DSPEC_LP64 538.imagick_r: -DSPEC_LP64 544.nab_r: -DSPEC_LP64 549.fotonik3d_r: -DSPEC_LP64 554.roms_r: -DSPEC_LP64

Base Optimization Flags

C benchmarks:

-mabi=lp64 -std=c99 -O3 -g -pipe -flto -march=armv8.2-a+lse
-fno-PIE -fomit-frame-pointer -no-pie -funroll-loops

C++ benchmarks:

-mabi=lp64 -O3 -g -pipe -flto -march=armv8.2-a+lse -fno-PIE
-fomit-frame-pointer -no-pie -funroll-loops

Fortran benchmarks:

-mabi=lp64 -O3 -g -pipe -flto -march=armv8.2-a+lse -fno-PIE
-fomit-frame-pointer -no-pie -funroll-loops

Benchmarks using both Fortran and C:

-mabi=lp64 -std=c99 -O3 -g -pipe -flto -march=armv8.2-a+lse
-fno-PIE -fomit-frame-pointer -no-pie -funroll-loops

Benchmarks using both C and C++:

-mabi=lp64 -std=c99 -O3 -g -pipe -flto -march=armv8.2-a+lse
-fno-PIE -fomit-frame-pointer -no-pie -funroll-loops

Benchmarks using Fortran, C, and C++:

-mabi=lp64 -std=c99 -O3 -g -pipe -flto -march=armv8.2-a+lse
-fno-PIE -fomit-frame-pointer -no-pie -funroll-loops

The flags files that were used to format this result can be browsed at

http://www.spec.org/cpu2017/flags/gcc.2020-06-30.html
http://www.spec.org/cpu2017/flags/PCL-Platform-Settings-Kunpeng-V1.0-revF.html

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: Peng Cheng Laboratory)

Huawei

(2.6 GHz,Huawei Kunpeng 920 7260)

Huawei TaiShan 200 Server (Model 2480) SPECrate®2017_fp_peak = Not Run

SPECrate^®2017_fp_base = 501

CPU2017 License: 5036 Test Date: May-2020 Test Sponsor: Peng Cheng Laboratory Hardware Availability: Jan-2020 Tested by: Peng Cheng Laboratory Software Availability: Jul-2020

You can also download the XML flags sources by saving the following links:

http://www.spec.org/cpu2017/flags/gcc.2020-06-30.xml
http://www.spec.org/cpu2017/flags/PCL-Platform-Settings-Kunpeng-V1.0-revF.xml

Originally published on 2020-07-07.

Report generated on 2020-07-07 14:30:03 by CPU2017 PS formatter v6255.

Tested with SPEC CPU^®2017 v1.1.0 on 2020-06-20 22:31:04-0400.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

names appearing in this result are trademarks or registered trademarks of their respective holders.

SPEC CPU and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and product