Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

500.perlbench_r

502.gcc_r

505.mcf_r

520.omnetpp_r

523.xalancbmk_r

525.x264_r

531.deepsjeng_r

541.leela_r

548.exchange2_r

557.xz_r

Copies

(338)

SPECrate^®2017_int_energy_peak

(63.9)

SPECrate^®2017_int_peak

(323)

SPECrate^®2017_int_energy_base

(61.4)

SPECrate^®2017_int_base

0 890

40.0 80.0 120 160 200 240 280 320 360 400 440 480 520 560 600 640 680 720 760 800 840 32 55.0 274 63.6 312 32 48.4 267 51.1 288 32 34.7 195 32 34.3 198 36.6 216 32 41.7 211 41.8 216 32 106 619 32 72.1 380 75.7 394 32 75.8 407 81.6 437 32 227 877 32 43.8 245 44.2 252 Hardware

CPU Name: Ampere eMAG 8180 Max MHz: 3300 Nominal: 3000 Enabled: 32 cores, 1 chip Orderable: 1 chips Cache L1: 32 KB I + 32 KB D on chip per core L2: 4 MB I+D on chip per chip (256 KiB shared / 2 cores) L3: 32 MB I+D on chip per chip Other: None Memory: 128 GB (8 x 16 GB 2Rx4 PC4-2666V-R) Storage: 1 x 480 GB SATA SSD Other: CPU Cooling: Air

Software

OS: Ubuntu 24.04.1 LTS kernel 6.8.0 (64KB pages) Compiler: C/C++/Fortran: Version 15.2.0 of GCC Parallel: No Firmware: Version 1.12 released Nov-2019 File System: ext4 System State: Run level 5 (multi-user) Base Pointers: 64-bit Peak Pointers: 64-bit Other: jemalloc v5.3+, commit hash 1972241 Power Management: OS CPU governor set to "performance"

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Power

Max. Power (W): 296.14 Idle Power (W): 77.99 Min. Temperature (C): 20.75 Elevation (m): 60 Line Standard: 120 V / 60 Hz / 1 phase / 2 wire Provisioning: Line powered

Power Settings

Management FW: Version 11.05.111 of Falcon BMC Memory Mode: Normal

Power-Relevant Hardware

Power Supply: 1 x 550 W (non-redundant) Details:^{Lenovo 03LD785 550 Watt High Efficiency Platinum}

AC Power Supply

Backplane: N/A Other Storage: N/A Storage Model #s:^{1 x Lenovo 01PE965 (480GB SATA SSD) connected to}

on-board HBA

NICs Installed:^{1 x Lenovo 01PE857 @ 10 GbE (2 ports ethernet)} NICs Enabled (FW/OS): 2 / 1 NICs Connected/Speed: 1 @ 1 Gbps Other HW Model #s: --

Power Analyzer

Power Analyzer: cpu-reference-ptd:8000 Hardware Vendor: Yokogawa Model: YokogawaWT310E Serial Number: T11733385 Input Connection: Serial over USB Metrology Institute: NIST Calibration By: Yokogawa USA Calibration Label: T126622 Calibration Date: 18-Aug-2025 PTDaemon^® Version: 1.11.3 (0c074d7d; 2025-10-15) Setup Description: Directly connected Current Ranges Used: 5A Voltage Range Used: 150V

Temperature Meter

Temperature Meter: cpu-reference-ptd:9000 Hardware Vendor: PCSensor Model: USB9097+DS18B20 Serial Number: -- Input Connection: USB PTDaemon Version: 1.11.3 (0c074d7d; 2025-10-15) Setup Description: In front of SUT front panel primary air inlet

Base Results Table

Benchmark Copies Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum

500.perlbench_r 32 926 55.0 203 273 219 278 926 55.0 202 274 218 278 923 55.2 201 275 217 283 502.gcc_r 32 937 48.4 184 267 197 266 939 48.3 184 267 196 269 937 48.4 184 267 197 270 505.mcf_r 32 1491 34.7 290 195 194 271 1489 34.7 289 196 194 273 1509 34.3 293 193 194 272 520.omnetpp_r 32 1224 34.3 229 198 187 195 1225 34.3 229 198 187 198 1224 34.3 230 198 188 197 523.xalancbmk_r 32 810 41.7 172 213 212 286 809 41.7 174 211 214 289 807 41.9 171 214 212 291 525.x264_r 32 528 106 98.1 619 186 205 527 106 98.2 619 186 205 533 105 98.7 615 185 203 531.deepsjeng_r 32 509 72.1 104 385 204 267 509 72.1 104 382 205 255 509 72.1 105 380 206 269 541.leela_r 32 699 75.8 142 405 203 251 699 75.8 141 407 201 243 698 75.9 142 404 203 264 548.exchange2_r 32 370 227 104 873 281 293 370 227 104 877 280 294 370 227 103 880 279 293 557.xz_r 32 789 43.8 153 246 193 226 788 43.8 153 245 195 252 788 43.9 154 244 196 265 SPECrate^®2017_int_base = 61.4

SPECrate^®2017_int_energy_base = 323

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Peak Results Table

Benchmark Copies Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum

500.perlbench_r 32 817 62.4 184 301 225 283 801 63.6 177 312 222 285 800 63.7 179 309 224 284 502.gcc_r 32 889 51.0 172 287 193 250 880 51.5 171 288 194 248 886 51.1 171 288 193 239 505.mcf_r 32 1491 34.7 290 195 194 271 1489 34.7 289 196 194 273 1509 34.3 293 193 194 272 520.omnetpp_r 32 1152 36.4 212 215 184 195 1146 36.6 211 215 185 193 1146 36.6 211 216 184 192 523.xalancbmk_r 32 812 41.6 168 218 206 296 809 41.8 169 216 209 296 807 41.9 167 219 207 294 525.x264_r 32 528 106 98.1 619 186 205 527 106 98.2 619 186 205 533 105 98.7 615 185 203 531.deepsjeng_r 32 484 75.7 101 394 209 269 484 75.7 101 394 209 275 491 74.7 101 394 206 260 541.leela_r 32 650 81.6 131 437 202 237 650 81.5 131 438 202 245 649 81.7 134 427 207 255 548.exchange2_r 32 370 227 104 873 281 293 370 227 104 877 280 294 370 227 103 880 279 293 557.xz_r 32 782 44.2 149 252 191 248 783 44.2 149 252 191 243 783 44.2 149 252 191 239 SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_peak = 338

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

The config file option ’submit’ was used.

Environment Variables Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH = "/usr/lib64/:/usr/lib/:/lib64:/home/mjm/jemalloc/lib"

General Notes

jemalloc is a general purpose malloc(3) implementation that emphasizes
fragmentation avoidance and scalable concurrency support.
sources available from https://github.com/facebook/jemalloc/tree/1972241
and built via "./configure --with-lg-quantum=3" which used system gcc-14 -O3

This benchmark result is intended to provide perspective on
past power and/or performance using the historical hardware
and/or software described on this result page.

The system as described on this result page was formerly
generally available. At the time of this publication, it may
not be shipping, and/or may not be supported, and/or may fail
to meet other tests of General Availability described in the
SPEC OSG Policy document, http://www.spec.org/osg/policy.html

This measured result may not be representative of the result
that would be measured were this benchmark run with hardware
and software available as of the publication date.

Platform Notes

 Sysinfo program /home/mjm/cpu2017/bin/sysinfo

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Platform Notes (Continued)

 Rev: r6732 of 2022-11-07 fe91c89b7ed5c36ae2c92cc097bec197
 running on emag Fri Feb 27 18:49:45 2026

 SUT (System Under Test) info as seen by some common utilities.

 ------------------------------------------------------------
 Table of contents
 ------------------------------------------------------------
  1. uname -a
  2. w
  3. Username
  4. ulimit -a
  5. sysinfo process ancestry
  6. /proc/cpuinfo
  7. lscpu
  8. numactl --hardware
  9. /proc/meminfo
 10. who -r
 11. Systemd service manager version: systemd 255 (255.4-1ubuntu8.8)
 12. Services, from systemctl list-unit-files
 13. Linux kernel boot-time arguments, from /proc/cmdline
 14. sysctl
 15. /sys/kernel/mm/transparent_hugepage
 16. /sys/kernel/mm/transparent_hugepage/khugepaged
 17. OS release
 18. Disk information
 19. /sys/devices/virtual/dmi/id
 20. dmidecode
 21. BIOS
 ------------------------------------------------------------

 ------------------------------------------------------------
 1. uname -a
   Linux emag 6.8.0 #1 SMP PREEMPT_DYNAMIC Fri Feb 28 00:25:30 UTC 2025 aarch64 aarch64 aarch64 GNU/Linux

 ------------------------------------------------------------
 2. w
    18:49:45 up 70 days, 19:14,  2 users,  load average: 2.03, 9.95, 13.63
   USER     TTY      FROM             LOGIN@   IDLE   JCPU   PCPU WHAT
   mjm               10.13.114.186    28Jan26 36:39m  0.00s  0.02s sshd: mjm [priv]

 ------------------------------------------------------------
 3. Username
   From environment variable $USER:  mjm

 ------------------------------------------------------------
 4. ulimit -a
   time(seconds)        unlimited
   file(blocks)         unlimited
   data(kbytes)         unlimited
   stack(kbytes)        unlimited
   coredump(blocks)     0
   memory(kbytes)       unlimited
   locked memory(kbytes) 16691648
   process              128681
   nofiles              1024
   vmemory(kbytes)      unlimited

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Platform Notes (Continued)

   locks                unlimited
   rtprio               0

 ------------------------------------------------------------
 5. sysinfo process ancestry
  /usr/lib/systemd/systemd --system --deserialize=66
  SCREEN
  -bin/tcsh
  runcpu --flagsurl=$SPEC/gcc.2024-08-14.xml --reportable -c emag-Ofast-gcc15 --tune=base,peak -n 3 -C 32
    intrate
  runcpu --flagsurl $SPEC/gcc.2024-08-14.xml --reportable --configfile emag-Ofast-gcc15 --tune base,peak
    --iterations 3 --copies 32 --runmode rate --tune base:peak --size refrate intrate --nopreenv --note-preenv
    --logfile $SPEC/tmp/CPU2017.093/templogs/preenv.intrate.093.0.log --lognum 093.0 --from_runcpu 2
  specperl $SPEC/bin/sysinfo -f
 $SPEC = /home/mjm/cpu2017

 ------------------------------------------------------------
 6. /proc/cpuinfo
     CPU implementer : 0x50
     CPU architecture: 8
     CPU variant     : 0x3
     CPU part        : 0x000
     CPU revision    : 2
     Features        : fp asimd evtstrm aes pmull sha1 sha2 crc32 cpuid

 ------------------------------------------------------------
 7. lscpu

 From lscpu from util-linux 2.39.3:
   Architecture:                       aarch64
   CPU op-mode(s):                     32-bit, 64-bit
   Byte Order:                         Little Endian
   CPU(s):                             32
   On-line CPU(s) list:                0-31
   Vendor ID:                          APM
   Model name:                         -
   Model:                              2
   Thread(s) per core:                 1
   Core(s) per socket:                 32
   Socket(s):                          1
   Stepping:                           0x3
   Frequency boost:                    disabled
   CPU(s) scaling MHz:                 100%
   CPU max MHz:                        2911.7639
   CPU min MHz:                        363.9700
   BogoMIPS:                           80.00
   Flags:                              fp asimd evtstrm aes pmull sha1 sha2 crc32 cpuid
   L1d cache:                          1 MiB (32 instances)
   L1i cache:                          1 MiB (32 instances)
   L2 cache:                           4 MiB (16 instances)
   NUMA node(s):                       1
   NUMA node0 CPU(s):                  0-31
   Vulnerability Gather data sampling: Not affected
   Vulnerability Itlb multihit:        Not affected
   Vulnerability L1tf:                 Not affected
   Vulnerability Mds:                  Not affected
   Vulnerability Meltdown:             Mitigation; PTI

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Platform Notes (Continued)

   Vulnerability Mmio stale data:      Not affected
   Vulnerability Retbleed:             Not affected
   Vulnerability Spec rstack overflow: Not affected
   Vulnerability Spec store bypass:    Vulnerable
   Vulnerability Spectre v1:           Mitigation; __user pointer sanitization
   Vulnerability Spectre v2:           Vulnerable
   Vulnerability Srbds:                Not affected
   Vulnerability Tsx async abort:      Not affected

 From lscpu --cache:
      NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
      L1d       32K       1M    8 Data            1
      L1i       32K       1M    8 Instruction     1
      L2       256K       4M   32 Unified         2

 ------------------------------------------------------------
 8. numactl --hardware
 NOTE: a numactl ’node’ might or might not correspond to a physical chip.
   available: 1 nodes (0)
   node 0 cpus: 0-31
   node 0 size: 130403 MB
   node 0 free: 101255 MB
   node distances:
   node   0
     0:  10

 ------------------------------------------------------------
 9. /proc/meminfo
    MemTotal:       133533376 kB

 ------------------------------------------------------------
 10. who -r
   run-level 5 Dec 18 23:35

 ------------------------------------------------------------
 11. Systemd service manager version: systemd 255 (255.4-1ubuntu8.8)
   Default Target  Status
   graphical       running

 ------------------------------------------------------------
 12. Services, from systemctl list-unit-files
   STATE            UNIT FILES
   enabled          ModemManager apparmor apport blk-availability cloud-config cloud-final cloud-init
                    cloud-init-local console-setup cron dmesg e2scrub_reap finalrd getty@ grub-common
                    grub-initrd-fallback keyboard-setup lvm2-monitor multipathd networkd-dispatcher open-iscsi
                    open-vm-tools pollinate power-profiles-daemon rsyslog secureboot-db setvtrgb snapd sysstat
                    systemd-networkd systemd-networkd-wait-online systemd-pstore systemd-resolved
                    systemd-timesyncd ua-reboot-cmds ubuntu-advantage udisks2 ufw unattended-upgrades vgauth
   enabled-runtime  netplan-ovs-cleanup systemd-fsck-root systemd-remount-fs
   disabled         console-getty debug-shell ipmievd iscsid nftables rsync ssh systemd-boot-check-no-failures
                    systemd-confext systemd-network-generator systemd-networkd-wait-online@
                    systemd-pcrlock-file-system systemd-pcrlock-firmware-code systemd-pcrlock-firmware-config
                    systemd-pcrlock-machine-id systemd-pcrlock-make-policy
                    systemd-pcrlock-secureboot-authority systemd-pcrlock-secureboot-policy systemd-sysext
                    systemd-time-wait-sync
   generated        openipmi perlbal
   indirect         serial-getty@ systemd-sysupdate systemd-sysupdate-reboot uuidd

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Platform Notes (Continued)

   masked           cryptdisks cryptdisks-early hwclock multipath-tools-boot screen-cleanup sudo x11-common

 ------------------------------------------------------------
 13. Linux kernel boot-time arguments, from /proc/cmdline
   BOOT_IMAGE=/boot/vmlinuz-6.8.0
   root=UUID=16268541-06d0-4374-97ca-2d512d4db26f
   ro
   cma=1024M
   iommu.passthrough=1

 ------------------------------------------------------------
 14. sysctl
   kernel.numa_balancing               0
   kernel.randomize_va_space           2
   vm.compaction_proactiveness        20
   vm.dirty_background_bytes           0
   vm.dirty_background_ratio          10
   vm.dirty_bytes                      0
   vm.dirty_expire_centisecs        3000
   vm.dirty_ratio                     20
   vm.dirty_writeback_centisecs      500
   vm.dirtytime_expire_seconds     43200
   vm.extfrag_threshold              500
   vm.min_unmapped_ratio               1
   vm.nr_hugepages                     0
   vm.nr_hugepages_mempolicy           0
   vm.nr_overcommit_hugepages          0
   vm.swappiness                      60
   vm.watermark_boost_factor       15000
   vm.watermark_scale_factor          10
   vm.zone_reclaim_mode                0

 ------------------------------------------------------------
 15. /sys/kernel/mm/transparent_hugepage
   defrag          always defer defer+madvise [madvise] never
   enabled         always [madvise] never
   hpage_pmd_size  536870912
   shmem_enabled   always within_size advise [never] deny force

 ------------------------------------------------------------
 16. /sys/kernel/mm/transparent_hugepage/khugepaged
   alloc_sleep_millisecs   60000
   defrag                      1
   max_ptes_none            8191
   max_ptes_shared          4096
   max_ptes_swap            1024
   pages_to_scan           65536
   scan_sleep_millisecs    10000

 ------------------------------------------------------------
 17. OS release
   From /etc/*-release /etc/*-version
   os-release Ubuntu 24.04.1 LTS

 ------------------------------------------------------------
 18. Disk information
 SPEC is set to: /home/mjm/cpu2017

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Platform Notes (Continued)

   Filesystem     Type  Size  Used Avail Use% Mounted on
   /dev/sda2      ext4  439G  292G  124G  71% /

 ------------------------------------------------------------
 19. /sys/devices/virtual/dmi/id
     Vendor:         Lenovo
     Product:        HR330A            7X33CTO1WW
     Product Family: Lenovo ThinkSystem HR330A/HR350A

 ------------------------------------------------------------
 20. dmidecode
   Additional information from dmidecode 3.5 follows.  WARNING: Use caution when you interpret this section.
   The ’dmidecode’ program reads system data which is "intended to allow hardware to be accurately
   determined", but the intent may not be met, as there are frequent changes to hardware, firmware, and the
   "DMTF SMBIOS" standard.
   Memory:
     8x Samsung M393A2K43CB2-CTD 16 GB 2 rank 2667

 ------------------------------------------------------------
 21. BIOS
 (This section combines info from /sys/devices and dmidecode.)
    BIOS Vendor:       LENOVO
    BIOS Version:      HVE104N-1.12
    BIOS Date:         11/29/2019
    BIOS Revision:     1.12
    Firmware Revision: 1.7

Power Settings Notes

OS CPU governor was set using the command:
echo performance | tee /sys/devices/system/cpu/cpu*/cpufreq/scaling_governor

Compiler Version Notes

============================================================================================================
C       | 500.perlbench_r(base, peak) 502.gcc_r(base, peak) 505.mcf_r(base, peak) 525.x264_r(base, peak)
        | 557.xz_r(base, peak)
------------------------------------------------------------------------------------------------------------
gcc (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------------------------------------

============================================================================================================
C++     | 520.omnetpp_r(base, peak) 523.xalancbmk_r(base, peak) 531.deepsjeng_r(base, peak)
        | 541.leela_r(base, peak)
------------------------------------------------------------------------------------------------------------
g++ (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------------------------------------

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Compiler Version Notes (Continued)

============================================================================================================
Fortran | 548.exchange2_r(base, peak)
------------------------------------------------------------------------------------------------------------
GNU Fortran (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Fortran benchmarks:

gfortran

Base Portability Flags

500.perlbench_r: -DSPEC_LINUX_AARCH64 -DSPEC_LP64 502.gcc_r: -DSPEC_LP64 505.mcf_r: -DSPEC_LP64 520.omnetpp_r: -DSPEC_LP64 523.xalancbmk_r: -DSPEC_LINUX -DSPEC_LP64 525.x264_r: -DSPEC_LP64 531.deepsjeng_r: -DSPEC_LP64 541.leela_r: -DSPEC_LP64 548.exchange2_r: -DSPEC_LP64 557.xz_r: -DSPEC_LP64

Base Optimization Flags

C benchmarks:

-mabi=lp64 -std=c99 -g -Ofast -mcpu=native -flto=16
-fno-strict-aliasing -fno-unsafe-math-optimizations
-fno-finite-math-only -fgnu89-inline -L/home/mjm/jemalloc/lib
-ljemalloc

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Base Optimization Flags (Continued)

C++ benchmarks:

-mabi=lp64 -std=c++03 -g -Ofast -mcpu=native -flto=16
-L/home/mjm/jemalloc/lib -ljemalloc

Fortran benchmarks:

-mabi=lp64 -g -Ofast -mcpu=native -flto=16 -L/home/mjm/jemalloc/lib
-ljemalloc

Base Other Flags

C benchmarks:

-fcommon

C++ benchmarks:

-Wno-error=template-body

Peak Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Fortran benchmarks:

gfortran

Peak Portability Flags

Same as Base Portability Flags

Peak Optimization Flags

C benchmarks:

(Continued on next page)

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

Peak Optimization Flags (Continued)

500.perlbench_r: -mabi=lp64 -std=c99 -fprofile-generate -fprofile-use -g

-Ofast -mcpu=native -flto=16 -fno-strict-aliasing
-fno-unsafe-math-optimizations -fno-finite-math-only
-L/home/mjm/jemalloc/lib -ljemalloc

502.gcc_r: -mabi=lp64 -std=c99 -fprofile-generate -fprofile-use -g

-Ofast -mcpu=native -flto=16 -fno-strict-aliasing
-fgnu89-inline -L/home/mjm/jemalloc/lib -ljemalloc

505.mcf_r: basepeak = yes

525.x264_r: basepeak = yes

557.xz_r: -mabi=lp64 -std=c99 -fprofile-generate -fprofile-use -g

-Ofast -mcpu=native -flto=16 -L/home/mjm/jemalloc/lib
-ljemalloc

C++ benchmarks:

-mabi=lp64 -std=c++03 -fprofile-generate -fprofile-use -g -Ofast
-mcpu=native -flto=16 -L/home/mjm/jemalloc/lib -ljemalloc

Fortran benchmarks:

548.exchange2_r: basepeak = yes

Peak Other Flags

C benchmarks:

505.mcf_r: -fcommon

525.x264_r: -fcommon

C++ benchmarks:

523.xalancbmk_r: -Wno-error=template-body

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2017/flags/gcc.2026-04-28.00.html

Page 12 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Integer Rate Result

Copyright 2017-2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Lenovo Global Technology

(3.00 GHz Ampere eMAG 8180)

ThinkSystem HR330A_{SPECrate®2017_int_energy_peak = 338}

SPECrate^®2017_int_peak = 63.9

SPECrate^®2017_int_energy_base = 323

SPECrate^®2017_int_base = 61.4

CPU2017 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Apr-2019 Tested by: Ampere Computing, Inc. Software Availability: Aug-2025

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2017/flags/gcc.2026-04-28.00.xml

Originally published on 2026-04-28.

Report generated on 2026-04-28 13:16:51 by CPU2017 PS formatter v6716.

Tested with SPEC CPU^®2017 v1.1.9 on 2026-02-27 13:49:44-0500.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

product names appearing in this result are trademarks or registered trademarks of their respective holders.

PTDaemon, SPEC CPU, and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and