Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD. (3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

709.cactus_r

722.palm_r

731.astcenc_r

736.ocio_r

737.gmsh_r

748.flightdm_r

749.fotonik3d_r

765.roms_r

766.femflow_r

767.nest_r

772.marian_r

782.lbm_r

Copies 0 680

30.0 60.0 90.0 120 150 180 210 240 270 300 330 360 390 420 450 480 510 540 570 600 630 192 567 63.6 192 321 41.9 321 42.2 192 547 86.2 192 381 57.5 192 326 48.7 342 51.3 192 640 95.1 670 105 192 106 17.0 106 17.0 192 132 20.3 132 20.2 192 668 72.8 675 73.4 192 428 59.9 435 61.1 192 590 81.2 600 82.3 192 42.7 6.96

42.6 7.01

Hardware

CPU Name: AmpereOneM A192-32M Max MHz: 3200 Nominal: 3200 Enabled: 192 cores, 1 chip Orderable: 1 chip Cache L1: 16 KB I + 64 KB D on chip per core L2: 2 MB I+D on chip per core L3: 64 MB I+D on chip per chip

Software

OS: Fedora Linux 43 (Server Edition) 6.17.5-200.64K_PS.fc42.aarch64 Compiler: C/C++/Fortran: Version 15.2.0 of GCC Compiler Category: Community Firmware: Version 5.4.5.1 released Oct-2025 File System: xfs System State: Run level 3 (multi-user) Base Pointers: 64-bit

(Continued on next page) (Continued on next page)

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Hardware (Continued)

Other: None Memory: 768 GB (12 x 64 GB 2Rx4 PC5-5600B-R) Storage: 1 x 960 GB Samsung M.2 (MZ1L2960HCJR-00A07) Cooling: Air Other: None

Software (Continued)

Peak Pointers: 64-bit Other: Jemalloc memory allocator library v5.3.0 Power Management: OS CPU governor set to "performance"

Power

Max. Power (W): 838.2 Idle Power (W): 234.7 Min. Temperature (C): 20.44 Elevation (m): 60 Line Standard: 120 V / 60 Hz / 1 phase / 2 wire Provisioning: Line powered

Power Settings

Management FW: Version 4.06 of MegaRAC BMC Memory Mode: Normal

Power-Relevant Hardware

Power Supply: 1 x 1600 W (non-redundant) Details: 1+1 1600W 80 PLUS Titanium redundant power

supplies AC Power Supply

Backplane: PCIe Gen5 x4 Other Storage: Embedded SATA Controller Storage Model #s: R2A3-T40-AAV1 NICs Installed:^{1 x Mellanox Technologies MT27710 Family @ 25 GbE}

(2 ports ethernet)

NICs Enabled (FW/OS): 2 / 1 NICs Connected/Speed: 1 @ 25 Gbps Other HW Model #s: Fan configuration is 4 x 80x80x38mm

Power Analyzer

Power Analyzer: cpu-reference-ptd:8000 Hardware Vendor: Yokogawa Model: WT-310 Serial Number: T11733285 Input Connection: Serial over USB Metrology Institute: NIST Calibration By: Yokogawa USA Calibration Label: T126622 Calibration Date: 13-Aug-2025 PTDaemon^® Version: 1.11.3 (0c074d7d; 2025-10-15) Setup Description: Directly Connected to PSU 1 Current Ranges Used: 10A Voltage Range Used: 150V

Temperature Meter

Temperature Meter: cpu-reference-ptd:9000 Hardware Vendor: PCSensor Model: USB9097+DS18B20 Serial Number: N/A Input Connection: USB PTDaemon Version: 1.11.3 (0c074d7d; 2025-10-15) Setup Description: In front of SUT front panel primary air inlet

Base Results Table

Benchmark Copies Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy

Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum

709.cactus_r 192 288 572 218 64.2 758 834 291 565 220 63.7 754 831 290 567 220 63.6 758 835 Table continues on next page. Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Base Results Table (Continued)

Benchmark Copies Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum

722.palm_r 192 790 321 513 41.9 650 725 790 321 514 41.9 650 724 790 321 513 41.9 650 724 731.astcenc_r 192 295 547 156 86.2 529 553 295 547 156 86.2 529 552 297 542 156 86.0 526 553 736.ocio_r 192 444 378 246 57.2 554 668 441 381 244 57.5 554 660 439 382 245 57.5 557 667 737.gmsh_r 192 270 326 152 48.7 562 664 270 327 152 48.5 565 662 270 326 153 48.3 566 660 748.flightdm_r 192 214 643 121 95.3 567 598 215 640 121 95.1 565 598 215 638 122 94.8 566 598 749.fotonik3d_r 192 2101 106 1110 17.0 531 554 2104 105 1120 17.0 530 552 2102 106 1120 17.0 532 554 765.roms_r 192 2281 133 1300 20.3 571 594 2288 132 1300 20.3 570 597 2292 132 1310 20.2 570 597 766.femflow_r 192 423 666 327 73.0 772 821 422 668 328 72.8 777 821 421 670 325 73.3 774 819 767.nest_r 192 355 428 212 59.9 595 729 356 428 212 59.9 595 718 356 427 212 59.9 594 719 772.marian_r 192 514 590 314 81.2 610 691 515 588 313 81.3 608 682 514 590 314 81.1 611 693 782.lbm_r 192 2574 42.7 1410 6.96 547 559 2579 42.7 1410 6.95 546 559 2578 42.7 1410 6.96 546 560 SPECrate^®2026_fp_base = 310 SPECrate^®2026_fp_energy_base = 43.9

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Peak Results Table

Benchmark Copies Seconds Ratio (kJ)

Energy

Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum Seconds Ratio (kJ)

Energy Ratio

Energy Power

Average Power

Maximum

709.cactus_r 192 288 572 218 64.2 758 834 291 565 220 63.7 754 831 290 567 220 63.6 758 835 722.palm_r 192 789 321 511 42.1 647 733 793 320 511 42.1 644 731 789 321 510 42.2 646 718 731.astcenc_r 192 295 547 156 86.2 529 553 295 547 156 86.2 529 552 297 542 156 86.0 526 553 736.ocio_r 192 444 378 246 57.2 554 668 441 381 244 57.5 554 660 439 382 245 57.5 557 667 737.gmsh_r 192 258 342 144 51.3 559 663 257 342 144 51.4 558 663 258 342 144 51.4 557 663 748.flightdm_r 192 204 675 110 105 538 560 205 669 110 105 536 560 205 670 110 105 538 560 749.fotonik3d_r 192 2100 106 1120 17.0 532 553 2104 105 1120 17.0 531 553 2101 106 1120 17.0 531 553 765.roms_r 192 2289 132 1310 20.2 570 595 2290 132 1310 20.2 570 596 2288 132 1310 20.2 571 593 766.femflow_r 192 417 675 325 73.4 779 820 416 677 324 73.6 778 822 418 674 325 73.4 778 819 767.nest_r 192 349 436 208 61.1 594 729 350 435 208 61.1 593 736 352 433 209 60.7 593 730 772.marian_r 192 504 602 309 82.5 613 696 506 599 310 82.2 612 695 505 600 310 82.3 613 694 782.lbm_r 192 2583 42.6 1390 7.03 540 555 2586 42.5 1390 7.03 539 555 2585 42.6 1400 7.01 540 555 SPECrate^®2026_fp_peak = 314 SPECrate^®2026_fp_energy_peak = 44.7

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Notes

 Binaries were compiled on a system with 1x AmpereOneM CPU
 chip + 768 GB Memory using Fedora Linux 42

Submit Notes

 The config file option ’submit’ was used.
 ’numactl’ was used to bind copies to the cores.

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Operating System Notes

 ’ulimit -s unlimited’ was used to set environment stack size
 Set dirty_ratio=8 to limit dirty cache to 8% of memory
      echo 8 | sudo tee /proc/sys/vm/dirty_ratio
 Set swappiness=1 to swap only if necessary
      echo 1 | sudo tee /proc/sys/vm/swappiness
 Set zone_reclaim_mode=1 to free local node memory and avoid remote memory
      echo 1 | sudo tee /proc/sys/vm/zone_reclaim_mode
 Set drop_caches=3 to reset caches before invoking runcpu
      echo 3 | sudo tee /proc/sys/vm/drop_caches
 Set numa_balancing=0 to disable automatic numa balancing
      echo 0 | sudo tee /proc/sys/kernel/numa_balancing
 Switch off all ktune and tuned settings
      sudo tuned-adm off
 Transparent huge pages set to ’never’
      sudo bash -c "echo never > /sys/kernel/mm/transparent_hugepage/enabled"

 runcpu command invoked through numactl i.e.
 numactl --interleave=all runcpu <etc>

Environment Variables Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH =
     "/home/amptest/workspace/sir2026_pkg_verify/ampere_spec2026/spec2026/jem
     alloc/install/lib:/home/amptest/workspace/sir2026_pkg_verify/ampere_spec
     2026/spec2026/gcc/install/lib64:/home/amptest/ampere_spec2026/spec2026/j
     emalloc/install/lib:/home/amptest/ampere_spec2026/spec2026/gcc/install/l
     ib64"
MALLOC_CONF = "thp:never,dirty_decay_ms:-1,muzzy_decay_ms:-1,retain:true"

General Notes

 Jemalloc v5.3.0 is available via
 https://github.com/jemalloc/jemalloc/releases/download/5.3.0/jemalloc-5.3.0.tar.bz2
 It was built on Fedora Linux 42 using Version 15.2.0 of GCC
 The configure options are
 "--with-lg-page=16" for building libjemalloc.so, and
 "--with-lg-quantum=3 --with-lg-page=16" for building libjemalloc_ext.so
 Tuned MALLOC_CONF in terms of https://jemalloc.net/jemalloc.3.html

  NA: The test sponsor attests, as of date of publication, that CVE-2017-5754 (Meltdown)
  is mitigated in the system as tested and documented.

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

General Notes (Continued)

  Yes: The test sponsor attests, as of date of publication, that CVE-2017-5753 (Spectre variant 1)
  is mitigated in the system as tested and documented.
  Yes: The test sponsor attests, as of date of publication, that CVE-2017-5715 (Spectre variant 2)
  is mitigated in the system as tested and documented.

Platform Notes

 Note: lscpu is not able to detect the SLC.
 SLC is defined at https://developer.arm.com/documentation/100180/0103/bry1436285730281

 Sysinfo program /home/amptest/workspace/sir2026_pkg_verify/ampere_spec2026/spec2026/bin/sysinfo
 Rev: 069f95da7e7f5d81b2ce48a82150e54f
 running on ampereone Wed Feb  4 18:20:32 2026

 SUT (System Under Test) info as seen by some common utilities.

 ------------------------------------------------------------
 Table of contents
 ------------------------------------------------------------
  1. uname -srvm
  2. w
  3. Username
  4. ulimit -a
  5. sysinfo process ancestry
  6. /proc/cpuinfo
  7. lscpu
  8. numactl --hardware
  9. /proc/meminfo
 10. Systemd service manager version: systemd 258 (258-1.fc43)
 11. Services, from systemctl list-unit-files
 12. Linux kernel boot-time arguments, from /proc/cmdline
 13. cpupower frequency-info
 14. tuned-adm active
 15. sysctl
 16. /sys/kernel/mm/transparent_hugepage
 17. /sys/kernel/mm/transparent_hugepage/khugepaged
 18. OS release
 19. Disk information
 20. /sys/devices/virtual/dmi/id
 21. dmidecode
 22. BIOS
 ------------------------------------------------------------

 ------------------------------------------------------------

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

 1. uname -srvm
   Linux 6.17.5-200.64K_PS.fc42.aarch64 #1 SMP PREEMPT_DYNAMIC Wed Jan 21 08:54:52 EST 2026 aarch64

 ------------------------------------------------------------
 2. w
    18:20:32 up 10:33,  2 users,  load average: 103.85, 38.22, 63.21
   USER     TTY        LOGIN@   IDLE   JCPU   PCPU WHAT
   amptest            07:47   10:33m  0.00s  0.02s sshd-session: amptest [priv]
   amptest            07:47   10:33m  0.00s  0.17s /usr/lib/systemd/systemd --user

 ------------------------------------------------------------
 3. Username
   From environment variable $USER:  root
   From the command ’logname’:       amptest

 ------------------------------------------------------------
 4. ulimit -a
   real-time non-blocking time  (microseconds, -R) unlimited
   core file size              (blocks, -c) 0
   data seg size               (kbytes, -d) unlimited
   scheduling priority                 (-e) 0
   file size                   (blocks, -f) unlimited
   pending signals                     (-i) 784991
   max locked memory           (kbytes, -l) 8192
   max memory size             (kbytes, -m) unlimited
   open files                          (-n) 524288
   pipe size                (512 bytes, -p) 8
   POSIX message queues         (bytes, -q) 819200
   real-time priority                  (-r) 0
   stack size                  (kbytes, -s) unlimited
   cpu time                   (seconds, -t) unlimited
   max user processes                  (-u) 784991
   virtual memory              (kbytes, -v) unlimited
   file locks                          (-x) unlimited

 ------------------------------------------------------------
 5. sysinfo process ancestry
  /usr/lib/systemd/systemd --switched-root --system --deserialize=57
  sshd: /usr/sbin/sshd -D [listener] 0 of 10-100 startups
  sshd-session: amptest [priv]
  sshd-session: amptest@notty
  java -jar remoting.jar -workDir /home/amptest -jar-cache /home/amptest/remoting/jarCache
  /bin/bash /tmp/jenkins10316276322400487163.sh
  sudo -S -E UPDATE_UTIL=false /home/amptest/util/jenkins/speccpu_pkg_verify.sh
    GreenSIR2026/without_report/spec2026_fprate_gcc15_Ofast_static_ampereonem_power_110.tgz

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

  /bin/bash /home/amptest/util/jenkins/speccpu_pkg_verify.sh
    GreenSIR2026/without_report/spec2026_fprate_gcc15_Ofast_static_ampereonem_power_110.tgz
  /bin/bash /home/amptest/workspace/sir2026_pkg_verify/ampere_spec2026/run_spec2026.sh --iterations 3

    --nobuild --action run --copies 192 --reportable --tune=base,peak fprate
  runcpu --config=ampere_aarch64 --define numasize=48 --define
    gcc_dir=/home/amptest/ampere_spec2026/spec2026/gcc/install --define
    llvm_dir=/home/amptest/ampere_spec2026/spec2026/llvm/install --define

    jemalloc_dir=/home/amptest/ampere_spec2026/spec2026/jemalloc/install --define glibc_dir=/ --iterations 3

    --nobuild --action run --copies 192 --reportable --tune=base,peak fprate
  runcpu --configfile ampere_aarch64 --define numasize=48 --define
    gcc_dir=/home/amptest/ampere_spec2026/spec2026/gcc/install --define
    llvm_dir=/home/amptest/ampere_spec2026/spec2026/llvm/install --define

    jemalloc_dir=/home/amptest/ampere_spec2026/spec2026/jemalloc/install --define glibc_dir=/ --iterations 3
    --nobuild --action run --copies 192 --reportable --tune base,peak --runmode rate --tune base:peak --size
    refrate fprate --nopreenv --note-preenv --logfile $SPEC/tmp/CPU2026.003/templogs/preenv.fprate.003.0.log

    --lognum 003.0 --from_runcpu 2
  specperl $SPEC/bin/sysinfo -f
 $SPEC = /home/amptest/workspace/sir2026_pkg_verify/ampere_spec2026/spec2026

 ------------------------------------------------------------
 6. /proc/cpuinfo
     CPU implementer : 0xc0
     CPU architecture: 8
     CPU variant     : 0x0
     CPU part        : 0xac4
     CPU revision    : 0

     Features        : fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp cpuid asimdrdm jscvt
                       fcma lrcpc dcpop sha3 sm3 sm4 asimddp sha512 asimdfhm dit uscat ilrcpc flagm ssbs sb

                       paca pacg dcpodp flagm2 frint i8mm bf16 rng bti ecv

 ------------------------------------------------------------
 7. lscpu

 From lscpu from util-linux 2.41.3:
   Architecture:                            aarch64
   CPU op-mode(s):                          64-bit
   Byte Order:                              Little Endian
   CPU(s):                                  192
   On-line CPU(s) list:                     0-191
   Vendor ID:                               Ampere
   BIOS Vendor ID:                          Ampere (R)
   Model name:                              Ampere-1a
   BIOS Model name:                         AmpereOne (R) A192-32M CPU @ 3.2GHz
   BIOS CPU family:                         257
   Model:                                   0

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

   Thread(s) per core:                      1
   Core(s) per socket:                      192
   Socket(s):                               1
   Stepping:                                0x0
   Frequency boost:                         disabled
   CPU(s) scaling MHz:                      100%
   CPU max MHz:                             3200.0000
   CPU min MHz:                             1000.0000
   BogoMIPS:                                2000.00

   Flags:                                   fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp
                                            cpuid asimdrdm jscvt fcma lrcpc dcpop sha3 sm3 sm4 asimddp sha512
                                            asimdfhm dit uscat ilrcpc flagm ssbs sb paca pacg dcpodp flagm2

                                            frint i8mm bf16 rng bti ecv
   L1d cache:                               12 MiB (192 instances)
   L1i cache:                               3 MiB (192 instances)
   L2 cache:                                384 MiB (192 instances)
   NUMA node(s):                            4
   NUMA node0 CPU(s):                       0-47
   NUMA node1 CPU(s):                       48-95
   NUMA node2 CPU(s):                       96-143
   NUMA node3 CPU(s):                       144-191
   Vulnerability Gather data sampling:      Not affected
   Vulnerability Ghostwrite:                Not affected
   Vulnerability Indirect target selection: Not affected
   Vulnerability Itlb multihit:             Not affected
   Vulnerability L1tf:                      Not affected
   Vulnerability Mds:                       Not affected
   Vulnerability Meltdown:                  Not affected
   Vulnerability Mmio stale data:           Not affected
   Vulnerability Old microcode:             Not affected
   Vulnerability Reg file data sampling:    Not affected
   Vulnerability Retbleed:                  Not affected
   Vulnerability Spec rstack overflow:      Not affected
   Vulnerability Spec store bypass:         Mitigation; Speculative Store Bypass disabled via prctl
   Vulnerability Spectre v1:                Mitigation; __user pointer sanitization
   Vulnerability Spectre v2:                Not affected
   Vulnerability Srbds:                     Not affected
   Vulnerability Tsa:                       Not affected
   Vulnerability Tsx async abort:           Not affected
   Vulnerability Vmscape:                   Not affected

 From lscpu --cache:
      NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
      L1d       64K      12M    4 Data            1  256                      64
      L1i       16K       3M    4 Instruction     1   64                      64

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

      L2         2M     384M    8 Unified         2 4096                      64

 ------------------------------------------------------------
 8. numactl --hardware
 NOTE: a numactl ’node’ might or might not correspond to a physical chip.
   available: 4 nodes (0-3)
   node 0 cpus: 0-47
   node 0 size: 195947 MB
   node 0 free: 147239 MB
   node 1 cpus: 48-95
   node 1 size: 196403 MB
   node 1 free: 145340 MB
   node 2 cpus: 96-143
   node 2 size: 196403 MB
   node 2 free: 147555 MB
   node 3 cpus: 144-191
   node 3 size: 196211 MB
   node 3 free: 148464 MB
   node distances:
   node     0    1    2    3
      0:   10   11   11   12
      1:   11   10   12   11
      2:   11   12   10   11
      3:   12   11   11   10

 ------------------------------------------------------------
 9. /proc/meminfo
    MemTotal:       803806272 kB

 ’who -r’ did not return a run level

 ------------------------------------------------------------
 10. Systemd service manager version: systemd 258 (258-1.fc43)
   Default Target  Status
   multi-user      running

 ------------------------------------------------------------
 11. Services, from systemctl list-unit-files
   STATE            UNIT FILES

   enabled          ModemManager NetworkManager NetworkManager-dispatcher abrt-journal-core abrt-oops
                    abrt-vmcore abrt-xorg abrtd atd audit-rules auditd authselect-apply-changes bluetooth
                    crond dbus-broker fips-crypto-policy-overlay firewalld getty@ irqbalance iscsi-onboot
                    iscsi-starter lm_sensors lvm2-monitor mdmonitor multipathd rpmdb-rebuild rsyslog
                    rtkit-daemon selinux-autorelabel-mark smartd sshd sssd systemd-boot-clear-sysfail
                    systemd-confext systemd-resolved systemd-sysext systemd-tpm2-clear tuned udisks2 upower

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

   enabled-runtime  systemd-remount-fs
   disabled         NetworkManager-wait-online abrt-pstoreoops arp-ethers blk-availability
                    canberra-system-bootup canberra-system-shutdown canberra-system-shutdown-reboot
                    chrony-wait chronyd chronyd-restricted console-getty containerd cpupower debug-shell
                    dnf-system-upgrade dnf5-offline-transaction dnsmasq docker fancontrol fsidd gssproxy
                    iscsi-init iscsid iscsiuio kvm_stat lastlog2-import low-memory-monitor lvm-devices-import

                    man-db-restart-cache-update netavark-dhcp-proxy netavark-firewalld-reload
                    netavark-nftables-reload nfs-blkmap nfs-server nftables nis-domainname
                    nvmefc-boot-connections nvmf-autoconnect openhpid podman podman-auto-update
                    podman-clean-transient podman-kube@ podman-restart psacct rmtfs rpcbind
                    selinux-check-proper-disable ssh-host-keys-migration sshd-keygen@ svnserve
                    systemd-boot-check-no-failures systemd-boot-update systemd-homed systemd-homed-activate
                    systemd-homed-firstboot systemd-network-generator systemd-oomd systemd-pcrlock-file-system
                    systemd-pcrlock-firmware-code systemd-pcrlock-firmware-config systemd-pcrlock-machine-id

                    systemd-pcrlock-make-policy systemd-pcrlock-secureboot-authority

                    systemd-pcrlock-secureboot-policy systemd-pstore systemd-time-wait-sync systemd-timesyncd
                    systemd-udev-load-credentials systemd-userdb-load-credentials wpa_supplicant zvbid
   indirect         iscsi pcscd serial-getty@ sshd@ sssd-autofs sssd-kcm sssd-nss sssd-pac sssd-pam sssd-ssh

                    sssd-sudo systemd-sysupdate systemd-sysupdate-reboot systemd-userdbd

 ------------------------------------------------------------
 12. Linux kernel boot-time arguments, from /proc/cmdline
   BOOT_IMAGE=(hd5,gpt2)/vmlinuz-6.17.5-200.64K_PS.fc42.aarch64
   root=/dev/mapper/fedora-root
   ro
   rd.lvm.lv=fedora/root
   nokaslr
   kaslr.disabled=1
   nohz=on
   nohz_full=0-191

 ------------------------------------------------------------
 13. cpupower frequency-info
   analyzing CPU 60:
     current policy: frequency should be within 1000 MHz and 3.20 GHz.
                     The governor "performance" may decide which speed to use
                     within this range.

 ------------------------------------------------------------
 14. tuned-adm active
   No current active profile.

 ------------------------------------------------------------
 15. sysctl
   kernel.numa_balancing               0

(Continued on next page)

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

   kernel.randomize_va_space           2
   vm.compaction_proactiveness        20
   vm.dirty_background_bytes           0
   vm.dirty_background_ratio          10
   vm.dirty_bytes                      0
   vm.dirty_expire_centisecs        3000
   vm.dirty_ratio                      8
   vm.dirty_writeback_centisecs      500
   vm.dirtytime_expire_seconds     43200
   vm.extfrag_threshold              500
   vm.min_unmapped_ratio               1
   vm.nr_hugepages                     0
   vm.nr_hugepages_mempolicy           0
   vm.nr_overcommit_hugepages          0
   vm.swappiness                       1
   vm.watermark_boost_factor       15000
   vm.watermark_scale_factor          10
   vm.zone_reclaim_mode                1

 ------------------------------------------------------------
 16. /sys/kernel/mm/transparent_hugepage
   defrag          always defer defer+madvise madvise [never]
   enabled         always madvise [never]
   hpage_pmd_size  536870912
   shmem_enabled   always within_size advise [never] deny force

 ------------------------------------------------------------
 17. /sys/kernel/mm/transparent_hugepage/khugepaged
   alloc_sleep_millisecs   60000
   defrag                      1
   max_ptes_none            8191
   max_ptes_shared          4096
   max_ptes_swap            1024
   pages_to_scan           65536
   scan_sleep_millisecs    10000

 ------------------------------------------------------------
 18. OS release
   From /etc/*-release /etc/*-version
   os-release     Fedora Linux 43 (Server Edition)
   fedora-release Fedora release 43 (Forty Three)
   redhat-release Fedora release 43 (Forty Three)
   system-release Fedora release 43 (Forty Three)

 ------------------------------------------------------------

(Continued on next page)

Page 12 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Platform Notes (Continued)

 19. Disk information
 SPEC is set to: /home/amptest/workspace/sir2026_pkg_verify/ampere_spec2026/spec2026
   Filesystem              Type  Size  Used Avail Use% Mounted on
   /dev/mapper/fedora-root xfs   891G  245G  646G  28% /

 ------------------------------------------------------------
 20. /sys/devices/virtual/dmi/id
     Vendor:         GIGACOMPUTING
     Product:        R2A3-T40-AAV1
     Product Family: R2A3-T40-AAV1
     Serial:         0000000000000000000000000001

 ------------------------------------------------------------
 21. dmidecode

   Additional information from dmidecode 3.6 follows.  WARNING: Use caution when you interpret this section.
   The ’dmidecode’ program reads system data which is "intended to allow hardware to be accurately
   determined", but the intent may not be met, as there are frequent changes to hardware, firmware, and the

   "DMTF SMBIOS" standard.
   Memory:
     12x Micron Technology MTC40F2046S1RC56BD2 MLCC 64 GB 2 rank 5600

 ------------------------------------------------------------
 22. BIOS
 (This section combines info from /sys/devices and dmidecode.)
    BIOS Vendor:       Ampere Computing LLC
    BIOS Version:      5.4.5.1
    BIOS Date:         10/22/2025
    BIOS Revision:     5.37

Compiler Version Notes

==============================================================================
C       | 782.lbm_r(base, peak)
------------------------------------------------------------------------------
gcc (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++     | 731.astcenc_r(base, peak) 736.ocio_r(base, peak)
        | 748.flightdm_r(base, peak) 766.femflow_r(base, peak)

(Continued on next page)

Page 13 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Compiler Version Notes (Continued)

        | 767.nest_r(base, peak) 772.marian_r(base, peak)
------------------------------------------------------------------------------
g++ (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C  | 709.cactus_r(base pass 0, peak pass 0) 737.gmsh_r(base pass 0, peak
        | pass 1, peak pass 2)
------------------------------------------------------------------------------
g++ (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C  | 709.cactus_r(base pass 0, peak pass 0) 737.gmsh_r(base pass 0, peak
        | pass 1, peak pass 2)
------------------------------------------------------------------------------
gcc (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C  | 709.cactus_r(base pass 0, peak pass 0) 737.gmsh_r(base pass 0, peak
        | pass 1, peak pass 2)
------------------------------------------------------------------------------
g++ (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C  | 709.cactus_r(base pass 0, peak pass 0) 737.gmsh_r(base pass 0, peak
        | pass 1, peak pass 2)
------------------------------------------------------------------------------
gcc (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO

(Continued on next page)

Page 14 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Compiler Version Notes (Continued)

warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
Fortran | 722.palm_r(base, peak) 749.fotonik3d_r(base, peak) 765.roms_r(base,
        | peak)
------------------------------------------------------------------------------
GNU Fortran (GCC) 15.2.0
Copyright (C) 2025 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Fortran benchmarks:

gfortran

Benchmarks using both C and C++:

g++ gcc

Base Portability Flags

736.ocio_r: -fno-finite-math-only 737.gmsh_r: -fno-fast-math 767.nest_r: -fno-finite-math-only

Base Optimization Flags

C benchmarks:

-mabi=lp64 -std=c18 -Wl,-allow-multiple-definition -static
-fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64

(Continued on next page)

Page 15 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Base Optimization Flags (Continued)

C benchmarks (continued):

-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib -g -Ofast
-mcpu=ampere1a -flto=32 -funroll-loops --param early-inlining-insns=96
--param max-inline-insns-auto=64 --param inline-unit-growth=96
-u malloc -ljemalloc

C++ benchmarks:

731.astcenc_r: -mabi=lp64 -std=c++17 -Wl,-allow-multiple-definition

-static -fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-g -Ofast -mcpu=ampere1a -flto=32 -funroll-loops
--param early-inlining-insns=256
--param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -u malloc
-ljemalloc_ext

736.ocio_r: Same as 731.astcenc_r

748.flightdm_r: Same as 731.astcenc_r

766.femflow_r: -mabi=lp64 -std=c++17 -Wl,-allow-multiple-definition

-static -fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-g -Ofast -mcpu=ampere1a -flto=32 -funroll-loops
--param early-inlining-insns=256
--param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -pthread
-u malloc -ljemalloc_ext

767.nest_r: Same as 731.astcenc_r

772.marian_r: Same as 766.femflow_r

Fortran benchmarks:

-mabi=lp64 -std=f2008 -Wl,-allow-multiple-definition -static
-fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib

(Continued on next page)

Page 16 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Base Optimization Flags (Continued)

Fortran benchmarks (continued):

-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib -g -Ofast
-mcpu=ampere1a -flto=32 -funroll-loops -fallow-argument-mismatch
-u malloc -ljemalloc

Benchmarks using both C and C++:

-mabi=lp64 -std=c++17 -std=c18 -Wl,-allow-multiple-definition -static
-fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib -g -Ofast
-mcpu=ampere1a -flto=32 -funroll-loops --param early-inlining-insns=96
--param max-inline-insns-auto=64 --param inline-unit-growth=96
--param early-inlining-insns=256 --param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -u malloc -ljemalloc_ext

Base Other Flags

C benchmarks:

-w -Wl,-Map,mapfile

C++ benchmarks:

-Wl,-Map,mapfile

Fortran benchmarks:

-Wl,-Map,mapfile

Benchmarks using both C and C++:

-w -Wl,-Map,mapfile

Peak Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

(Continued on next page)

Page 17 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Peak Compiler Invocation (Continued)

Fortran benchmarks:

gfortran

Benchmarks using both C and C++:

g++ gcc

Peak Portability Flags

736.ocio_r: -fno-finite-math-only 737.gmsh_r: -fno-fast-math 767.nest_r: -fno-finite-math-only

Peak Optimization Flags

C benchmarks:

-mabi=lp64 -std=c18 -Wl,-allow-multiple-definition -static
-fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-fprofile-generate -fprofile-use -fprofile-partial-training -g -Ofast
-mcpu=ampere1a -flto=32 -funroll-loops --param early-inlining-insns=96
--param max-inline-insns-auto=64 --param inline-unit-growth=96
-u malloc -ljemalloc

C++ benchmarks:

731.astcenc_r: basepeak = yes

736.ocio_r: basepeak = yes

748.flightdm_r: -mabi=lp64 -std=c++17 -Wl,-allow-multiple-definition

-static -fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-fprofile-generate -fprofile-use
-fprofile-partial-training -g -Ofast -mcpu=ampere1a
-flto=32 -funroll-loops --param early-inlining-insns=256

(Continued on next page)

Page 18 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Peak Optimization Flags (Continued)

748.flightdm_r (continued):

--param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -u malloc
-ljemalloc_ext

766.femflow_r: -mabi=lp64 -std=c++17 -Wl,-allow-multiple-definition

-static -fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-fprofile-generate -fprofile-use
-fprofile-partial-training -g -Ofast -mcpu=ampere1a
-flto=32 -funroll-loops --param early-inlining-insns=256
--param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -pthread
-u malloc -ljemalloc_ext

767.nest_r: Same as 748.flightdm_r

772.marian_r: Same as 766.femflow_r

Fortran benchmarks:

-mabi=lp64 -std=f2008 -Wl,-allow-multiple-definition -static
-fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-fprofile-generate -fprofile-use -fprofile-partial-training -g -Ofast
-mcpu=ampere1a -flto=32 -funroll-loops -fallow-argument-mismatch
-u malloc -ljemalloc

Benchmarks using both C and C++:

709.cactus_r: basepeak = yes

737.gmsh_r: -mabi=lp64 -std=c++17 -std=c18

-Wl,-allow-multiple-definition -static -fwhole-program
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib64
-L/home/amptest/ampere_spec2026/spec2026/gcc/install/lib
-L/home/amptest/ampere_spec2026/spec2026/jemalloc/install/lib
-fprofile-generate -fprofile-use
-fprofile-partial-training -g -Ofast -mcpu=ampere1a
-flto=32 -funroll-loops --param early-inlining-insns=96
--param max-inline-insns-auto=64

(Continued on next page)

Page 19 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Floating Point Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

GIGA-BYTE TECHNOLOGY CO., LTD.

(3.20 GHz AmpereOneM A192-32M)

R2A3-T40-AAV1_{SPECrate®2026_fp_energy_peak = 44.7}

SPECrate^®2026_fp_peak = 314

SPECrate^®2026_fp_energy_base = 43.9

SPECrate^®2026_fp_base = 310

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Nov-2025 Tested by: Ampere Computing, Inc. Software Availability: Oct-2025

Peak Optimization Flags (Continued)

737.gmsh_r (continued):

--param inline-unit-growth=96
--param early-inlining-insns=256
--param max-inline-insns-auto=128
--param inline-unit-growth=256 -ffinite-loops -u malloc
-ljemalloc_ext

Peak Other Flags

C benchmarks:

-w -Wl,-Map,mapfile

C++ benchmarks:

-Wl,-Map,mapfile

Fortran benchmarks:

-Wl,-Map,mapfile

Benchmarks using both C and C++:

-w -Wl,-Map,mapfile

The flags files that were used to format this result can be browsed at

http://www.spec.org/cpu2026/results/flags/gcc-rev-A2.html
http://www.spec.org/cpu2026/results/flags/GIGA-BYTE-platform-settings-AmpereOneM-rev.1.html

You can also download the XML flags sources by saving the following links:

http://www.spec.org/cpu2026/results/flags/gcc-rev-A2.xml
http://www.spec.org/cpu2026/results/flags/GIGA-BYTE-platform-settings-AmpereOneM-rev.1.xml

Originally published on 2026-05-05.

Report generated on 2026-05-04 23:26:31 by CPU2026 PS formatter (86729d3b).

Tested with SPEC CPU^®2026 v0.902.0 on 2026-02-04 21:20:31-0500.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

product names appearing in this result are trademarks or registered trademarks of their respective holders.

PTDaemon, SPEC CPU, and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and