Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

706.stockfish_r

707.ntest_r

708.sqlite_r

710.omnetpp_r

714.cpython_r

721.gcc_r

723.llvm_r

727.cppcheck_r

729.abc_r

734.vpr_r

735.gem5_r

750.sealcrypto_r

753.ns3_r

777.zstd_r

Copies 0 9.00

1.00 2.00 3.00 4.00 5.00 6.00 7.00 8.00 4 6.84 7.65 4 6.17

4 4.68 4.71 4 4.94 4.98 4 8.01 8.10 4 3.45 3.50 4 4.59 4.67 4 3.93 3.99 4 4.38

4 3.38 3.43 4 5.46 5.53 4 4.68 4.75 4 6.56 6.57 4 2.88 2.92

Hardware

CPU Name: Broadcom BCM2712 Max MHz: 2400 Nominal: 2400 Enabled: 4 cores, 1 chip Orderable: 1 board Cache L1: 64 KB I + 64 KB D on chip per core L2: 2 MB I+D on chip per core 512 KB L3: 2 MB I+D on chip per chip Other: None Memory: 16 GB Storage: 1 x 128 GB Samsung PRO Endurance MicroSD Cooling: Air Other: Adafruit Raspberry Pi 5 case (ID 6307; no fan); veakson Portable Desk Fan (UPC 669936718801)

Software

OS: DietPi v9.19.2 (kernel 6.12.47+rpt-rpi-2712) Compiler: C/C++/Fortran: Version 14.2.0 of GCC, the GNU Compiler Collection (Debian 14.2.0-19) Compiler Category: Community Firmware: Version 57db150d released Nov-2025 File System: ext4 System State: Run level 3 (multi-user; no GUI) Base Pointers: 64-bit Peak Pointers: 64-bit Other: None Power Management: All settings left at default.

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

706.stockfish_r 4 736 6.84 731 6.89 4 659 7.65 657 7.67 707.ntest_r 4 384 6.17 381 6.21 4 384 6.17 381 6.21 708.sqlite_r 4 452 4.68 451 4.68 4 447 4.73 448 4.71 710.omnetpp_r 4 393 4.94 393 4.94 4 391 4.98 388 5.01 714.cpython_r 4 238 8.05 239 8.01 4 237 8.10 235 8.16 721.gcc_r 4 796 3.45 795 3.45 4 782 3.51 784 3.50 723.llvm_r 4 442 4.59 439 4.62 4 435 4.67 433 4.69 727.cppcheck_r 4 361 3.98 365 3.93 4 359 3.99 360 3.99 729.abc_r 4 419 4.38 418 4.39 4 419 4.38 418 4.39 734.vpr_r 4 540 3.41 546 3.38 4 538 3.43 532 3.47 735.gem5_r 4 356 5.48 357 5.46 4 351 5.55 353 5.53 750.sealcrypto_r 4 458 4.68 457 4.69 4 451 4.75 450 4.77 753.ns3_r 4 373 6.58 374 6.56 4 371 6.61 373 6.57 777.zstd_r 4 896 2.88 883 2.92 4 882 2.92 883 2.92 SPECrate^®2026_int_base = 4.80 SPECrate^®2026_int_peak = 4.89

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 ’ulimit -s unlimited’ was used to set environment stack size limit

Environment Variables Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH = "/usr/lib64/:/usr/lib/:/lib64"

Platform Notes

 System powered via USB-C from Apple 45W USB-C power supply.
 HDMI display and keyboard were disconnected during the run.

 Sysinfo program /spec/cpu2026-0.902.0/bin/sysinfo
 Rev: 069f95da7e7f5d81b2ce48a82150e54f
 running on ci-pi5 Sat Feb  7 14:42:23 2026

 SUT (System Under Test) info as seen by some common utilities.

 ------------------------------------------------------------
 Table of contents

(Continued on next page)

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Platform Notes (Continued)

 ------------------------------------------------------------
  1. uname -srvm
  2. w
  3. Username
  4. ulimit -a
  5. sysinfo process ancestry
  6. /proc/cpuinfo
  7. lscpu
  8. numactl warning
  9. /proc/meminfo
 10. Systemd service manager version: systemd 257 (257.9-1~deb13u1)
 11. Services, from systemctl list-unit-files
 12. Linux kernel boot-time arguments, from /proc/cmdline
 13. sysctl
 14. OS release
 15. Disk information
 16. dmidecode warning
 ------------------------------------------------------------

 ------------------------------------------------------------
 1. uname -srvm
   Linux 6.12.47+rpt-rpi-2712 #1 SMP PREEMPT Debian 1:6.12.47-1+rpt1 (2025-09-16) aarch64

 ------------------------------------------------------------
 2. w
    14:42:23 up 4 min,  0 users,  load average: 0.08, 0.02, 0.01
   USER     TTY      FROM             LOGIN@   IDLE   JCPU   PCPU  WHAT

 ------------------------------------------------------------
 3. Username
   From environment variable $USER:  cloyce

 ------------------------------------------------------------
 4. ulimit -a
   time(seconds)        unlimited
   file(blocks)         unlimited
   data(kbytes)         unlimited
   stack(kbytes)        unlimited
   coredump(blocks)     0
   memory(kbytes)       unlimited
   locked memory(kbytes) 8192
   process              64597
   nofiles              1024
   vmemory(kbytes)      unlimited
   locks                unlimited
   rtprio               0

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Platform Notes (Continued)

 ------------------------------------------------------------
 5. sysinfo process ancestry
  /sbin/init
  tmux a
  zsh
  runcpu --reportable -c rpi-gcc intrate

  runcpu --reportable --configfile rpi-gcc --nopower --runmode rate --tune base:peak --size refrate intrate
    --nopreenv --note-preenv --logfile $SPEC/tmp/CPU2026.011/templogs/preenv.intrate.011.0.log --lognum 011.0

    --from_runcpu 2
  specperl $SPEC/bin/sysinfo -f
 $SPEC = /spec/cpu2026-0.902.0

 ------------------------------------------------------------
 6. /proc/cpuinfo
     CPU implementer : 0x41
     CPU architecture: 8
     CPU variant     : 0x4
     CPU part        : 0xd0b
     CPU revision    : 1

     Features        : fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp cpuid asimdrdm lrcpc

                       dcpop asimddp

    WARNING: the number of "processors" from /proc/cpuinfo does not seem to match the number of hardware

    threads as reported by lscpu.   Please verify counts independently.

 ------------------------------------------------------------
 7. lscpu

 From lscpu from util-linux 2.41:
   Architecture:                            aarch64
   CPU op-mode(s):                          32-bit, 64-bit
   Byte Order:                              Little Endian
   CPU(s):                                  4
   On-line CPU(s) list:                     0-3
   Vendor ID:                               ARM
   Model name:                              Cortex-A76
   Model:                                   1
   Thread(s) per core:                      1
   Core(s) per cluster:                     4
   Socket(s):                               -
   Cluster(s):                              1
   Stepping:                                r4p1
   CPU(s) scaling MHz:                      71%
   CPU max MHz:                             2400.0000
   CPU min MHz:                             1500.0000
   BogoMIPS:                                108.00

   Flags:                                   fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp

                                            cpuid asimdrdm lrcpc dcpop asimddp

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Platform Notes (Continued)

   L1d cache:                               256 KiB (4 instances)
   L1i cache:                               256 KiB (4 instances)
   L2 cache:                                2 MiB (4 instances)
   L3 cache:                                2 MiB (1 instance)
   NUMA node(s):                            8
   NUMA node0 CPU(s):                       0-3
   NUMA node1 CPU(s):                       0-3
   NUMA node2 CPU(s):                       0-3
   NUMA node3 CPU(s):                       0-3
   NUMA node4 CPU(s):                       0-3
   NUMA node5 CPU(s):                       0-3
   NUMA node6 CPU(s):                       0-3
   NUMA node7 CPU(s):                       0-3
   Vulnerability Gather data sampling:      Not affected
   Vulnerability Indirect target selection: Not affected
   Vulnerability Itlb multihit:             Not affected
   Vulnerability L1tf:                      Not affected
   Vulnerability Mds:                       Not affected
   Vulnerability Meltdown:                  Not affected
   Vulnerability Mmio stale data:           Not affected
   Vulnerability Reg file data sampling:    Not affected
   Vulnerability Retbleed:                  Not affected
   Vulnerability Spec rstack overflow:      Not affected
   Vulnerability Spec store bypass:         Mitigation; Speculative Store Bypass disabled via prctl
   Vulnerability Spectre v1:                Mitigation; __user pointer sanitization
   Vulnerability Spectre v2:                Mitigation; CSV2, BHB
   Vulnerability Srbds:                     Not affected
   Vulnerability Tsa:                       Not affected
   Vulnerability Tsx async abort:           Not affected
   Vulnerability Vmscape:                   Not affected

 From lscpu --cache:
      NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
      L1d       64K     256K    4 Data            1  256                      64
      L1i       64K     256K    4 Instruction     1  256                      64
      L2       512K       2M    8 Unified         2 1024                      64
      L3         2M       2M   16 Unified         3 2048                      64

 ------------------------------------------------------------
 8. numactl warning

 Unable to get information from ’numactl --hardware’.  Please consider installing numactl.

 ------------------------------------------------------------
 9. /proc/meminfo
    MemTotal:       16604176 kB

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Platform Notes (Continued)

 ’who -r’ did not return a run level

 ------------------------------------------------------------
 10. Systemd service manager version: systemd 257 (257.9-1~deb13u1)
   Default Target  Status
   graphical       running

 ------------------------------------------------------------
 11. Services, from systemctl list-unit-files
   STATE            UNIT FILES
   enabled          console-setup cron dietpi-kill_ssh dietpi-postboot dietpi-preboot dietpi-ramlog
                    fake-hwclock-load fake-hwclock-save getty@ keyboard-setup networking rpi-eeprom-update ssh

                    sshd-keygen systemd-pstore systemd-timesyncd
   enabled-runtime  systemd-fsck-root systemd-remount-fs

   disabled         console-getty debug-shell dietpi-cloudshell dietpi-firstboot dietpi-fs_partition_resize
                    dietpi-vpn dietpi-wifi-monitor e2scrub_reap ifupdown-wait-online rsync sysstat
                    systemd-boot-check-no-failures systemd-confext systemd-network-generator systemd-networkd
                    systemd-networkd-wait-online systemd-networkd-wait-online@ systemd-pcrlock-file-system
                    systemd-pcrlock-firmware-code systemd-pcrlock-firmware-config systemd-pcrlock-machine-id

                    systemd-pcrlock-make-policy systemd-pcrlock-secureboot-authority
                    systemd-pcrlock-secureboot-policy systemd-sysext systemd-time-wait-sync

                    systemd-udev-load-credentials wpa_supplicant wpa_supplicant-nl80211@ wpa_supplicant-wired@

                    wpa_supplicant@
   indirect         serial-getty@ sshd@

   masked           apt-daily apt-daily-upgrade cryptdisks cryptdisks-early fake-hwclock getty-static hwclock

                    serial-getty@ttyAMA0 serial-getty@ttyS0 sudo systemd-logind x11-common

 ------------------------------------------------------------
 12. Linux kernel boot-time arguments, from /proc/cmdline
   reboot=w
   coherent_pool=1M
   8250.nr_uarts=1
   pci=pcie_bus_safe
   cgroup_disable=memory
   numa_policy=interleave
   nvme.max_host_mem_size_mb=0
   bcm2708_fb.fbwidth=1920
   bcm2708_fb.fbheight=1080
   bcm2708_fb.fbdepth=16
   bcm2708_fb.fbswap=1
   numa=fake=8
   system_heap.max_order=0
   iommu_dma_numa_policy=interleave
   smsc95xx.macaddr=88:A2:9E:03:6B:8B
   vc_mem.mem_base=0x3fc00000
   vc_mem.mem_size=0x40000000
   root=PARTUUID=b06e45c0-02

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Platform Notes (Continued)

   rootfstype=ext4
   rootwait
   fsck.repair=yes
   net.ifnames=0
   logo.nologo
   console=ttyAMA10,115200
   console=tty1

 ------------------------------------------------------------
 13. sysctl
   kernel.randomize_va_space           2
   vm.compaction_proactiveness        20
   vm.dirty_background_bytes           0
   vm.dirty_background_ratio          10
   vm.dirty_bytes                      0
   vm.dirty_expire_centisecs        3000
   vm.dirty_ratio                     20
   vm.dirty_writeback_centisecs      500
   vm.dirtytime_expire_seconds     43200
   vm.extfrag_threshold              500
   vm.min_unmapped_ratio               1
   vm.swappiness                       1
   vm.watermark_boost_factor       15000
   vm.watermark_scale_factor          10
   vm.zone_reclaim_mode                0

 ------------------------------------------------------------
 14. OS release
   From /etc/*-release /etc/*-version
   os-release Debian GNU/Linux 13 (trixie)

 ------------------------------------------------------------
 15. Disk information
 SPEC is set to: /spec/cpu2026-0.902.0
   Filesystem     Type  Size  Used Avail Use% Mounted on
   /dev/root      ext4  117G   22G   91G  20% /

 ------------------------------------------------------------
 16. dmidecode warning
   Could not find dmidecode

 BIOS: (could not find information)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Compiler Version Notes

==============================================================================
C      | 708.sqlite_r(base, peak) 714.cpython_r(base, peak) 777.zstd_r(base,
       | peak)
------------------------------------------------------------------------------
gcc (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++    | 706.stockfish_r(base, peak) 707.ntest_r(base, peak)
       | 727.cppcheck_r(base, peak) 753.ns3_r(base, peak)
------------------------------------------------------------------------------
g++ (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C | 710.omnetpp_r(base pass 0, peak pass 0) 721.gcc_r(base pass 0, peak
       | pass 0) 723.llvm_r(base pass 0, peak pass 0) 729.abc_r(base pass 0,
       | peak pass 0) 734.vpr_r(base pass 0, peak pass 0) 735.gem5_r(base
       | pass 0, peak pass 0) 750.sealcrypto_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
g++ (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C | 710.omnetpp_r(base pass 0, peak pass 0) 721.gcc_r(base pass 0, peak
       | pass 0) 723.llvm_r(base pass 0, peak pass 0) 729.abc_r(base pass 0,
       | peak pass 0) 734.vpr_r(base pass 0, peak pass 0) 735.gem5_r(base
       | pass 0, peak pass 0) 750.sealcrypto_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
gcc (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C | 710.omnetpp_r(base pass 0, peak pass 0) 721.gcc_r(base pass 0, peak
       | pass 0) 723.llvm_r(base pass 0, peak pass 0) 729.abc_r(base pass 0,

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Compiler Version Notes (Continued)

       | peak pass 0) 734.vpr_r(base pass 0, peak pass 0) 735.gem5_r(base
       | pass 0, peak pass 0) 750.sealcrypto_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
g++ (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

==============================================================================
C++, C | 710.omnetpp_r(base pass 0, peak pass 0) 721.gcc_r(base pass 0, peak
       | pass 0) 723.llvm_r(base pass 0, peak pass 0) 729.abc_r(base pass 0,
       | peak pass 0) 734.vpr_r(base pass 0, peak pass 0) 735.gem5_r(base
       | pass 0, peak pass 0) 750.sealcrypto_r(base pass 0, peak pass 0)
------------------------------------------------------------------------------
gcc (Debian 14.2.0-19) 14.2.0
Copyright (C) 2024 Free Software Foundation, Inc.
This is free software; see the source for copying conditions.  There is NO
warranty; not even for MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Benchmarks using both C and C++:

g++ gcc

Base Portability Flags

706.stockfish_r: -DSPEC_LP64 707.ntest_r: -DSPEC_LP64 708.sqlite_r: -DSPEC_LP64 710.omnetpp_r: -DSPEC_LP64 714.cpython_r: -DSPEC_LP64 721.gcc_r: -DSPEC_LP64 723.llvm_r: -DSPEC_LP64 727.cppcheck_r: -DSPEC_LP64 729.abc_r: -DSPEC_LP64

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Base Portability Flags (Continued)

734.vpr_r: -DSPEC_LP64 735.gem5_r: -DSPEC_LP64 750.sealcrypto_r: -DSPEC_LP64 753.ns3_r: -DSPEC_LP64 777.zstd_r: -DSPEC_LP64

Base Optimization Flags

C benchmarks:

-mabi=lp64 -std=c18 -g -O3 -flto

C++ benchmarks:

-mabi=lp64 -std=c++17 -g -O3 -flto

Benchmarks using both C and C++:

-mabi=lp64 -std=c++17 -std=c18 -g -O3 -flto

Peak Compiler Invocation

C benchmarks:

gcc

C++ benchmarks:

g++

Benchmarks using both C and C++:

g++ gcc

Peak Portability Flags

706.stockfish_r: -DSPEC_LP64 707.ntest_r: -DSPEC_LP64 708.sqlite_r: -DSPEC_LP64 710.omnetpp_r: -fno-finite-math-only(*) -DSPEC_LP64 714.cpython_r: -DSPEC_LP64 721.gcc_r: -DSPEC_LP64 723.llvm_r: -DSPEC_LP64 727.cppcheck_r: -DSPEC_LP64 729.abc_r: -DSPEC_LP64

(Continued on next page)

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

Peak Portability Flags (Continued)

734.vpr_r: -fno-finite-math-only(*) -DSPEC_LP64 735.gem5_r: -fno-finite-math-only(*) -DSPEC_LP64 750.sealcrypto_r: -DSPEC_LP64 753.ns3_r: -fno-finite-math-only(*) -DSPEC_LP64 777.zstd_r: -DSPEC_LP64 (*) Indicates a portability flag that was found in a non-portability variable.

Peak Optimization Flags

C benchmarks:

-mabi=lp64 -std=c18 -Ofast -mcpu=native -flto

C++ benchmarks: 706.stockfish_r: -mabi=lp64 -std=c++17 -Ofast -mcpu=native -flto 707.ntest_r: basepeak = yes 727.cppcheck_r: Same as 706.stockfish_r 753.ns3_r: Same as 706.stockfish_r Benchmarks using both C and C++: 710.omnetpp_r: -mabi=lp64 -std=c++17 -std=c18 -Ofast -mcpu=native

-flto

721.gcc_r: Same as 710.omnetpp_r 723.llvm_r: Same as 710.omnetpp_r 729.abc_r: basepeak = yes 734.vpr_r: Same as 710.omnetpp_r 735.gem5_r: Same as 710.omnetpp_r 750.sealcrypto_r: Same as 710.omnetpp_r

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2026/results/flags/gcc-rev-A2.html

Page 12 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Ampere Computing, Inc.)

Raspberry Pi

Raspberry Pi 5 Model B Rev 1.1 (16 GB) SPECrate^®2026_int_peak = 4.89

SPECrate^®2026_int_base = 4.80

CPU2026 License: 6412 Test Date: Feb-2026 Test Sponsor: Ampere Computing, Inc. Hardware Availability: Jan-2025 Tested by: Ampere Computing, Inc. Software Availability: Nov-2025

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2026/results/flags/gcc-rev-A2.xml

Originally published on 2026-05-05.

Report generated on 2026-05-11 16:35:52 by CPU2026 PS formatter (86729d3b).

Tested with SPEC CPU^®2026 v0.902.0 on 2026-02-07 17:42:21-0500.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

names appearing in this result are trademarks or registered trademarks of their respective holders.

SPEC CPU and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and product