Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

706.stockfish_r

707.ntest_r

708.sqlite_r

710.omnetpp_r

714.cpython_r

721.gcc_r

723.llvm_r

727.cppcheck_r

729.abc_r

734.vpr_r

735.gem5_r

750.sealcrypto_r

753.ns3_r

777.zstd_r

Copies 0 13.0

1.00 2.00 3.00 4.00 5.00 6.00 7.00 8.00 9.00 10.0 11.0 12.0

1^{12.5}

1^{4.96}

1^{3.93}

1^{5.88}

1^{6.84}

1^{5.52}

1^{5.27}

1^{5.37}

1^{4.39}

1^{5.30}

1^{5.91}

1^{11.9}

1^{7.56}

1^{3.88}

Hardware

CPU Name: NVIDIA GB10 Max MHz: 4004 Nominal: 3900 Enabled: 20 (10x Cortex-X925, 10x Cortex-A725) cores, 1 chip Orderable: 1 chips Cache L1: 64 KB I + 64 KB D on chip per core L2: 2 MB I+D on chip per core; 512 KB I+D on chip per core L3: 16 MB I+D on chip per 10 core cluster (Cluster 1); 8 MB I+D on chip per 10 core cluster (Cluster 0) Other: None Memory: 128 GB (LPDDR5X-8533 MT/s) Storage: 1 x 3.7 TB NVMe SSD Cooling: Air Other: None

Software

OS: Ubuntu 24.04.3 LTS 6.14.0-1013-nvidia Compiler: C/C++/Fortran: Version 22.1.0 of LLVM Compiler Category: Community Firmware: Version 5.36_0ACUM018 released Aug-2025 File System: ext4 System State: Run level 5 (graphical multi-user) Base Pointers: 64-bit Peak Pointers: Not Applicable Other: None Power Management: OS set to prefer performance at the cost of additional power usage

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

706.stockfish_r 1 100 12.6 101 12.5 102 12.4 707.ntest_r 1 121 4.91 117 5.05 119 4.96 708.sqlite_r 1 134 3.93 137 3.86 129 4.09 710.omnetpp_r 1 82.6 5.88 82.6 5.88 82.8 5.87 714.cpython_r 1 70.0 6.84 70.6 6.79 69.4 6.90 721.gcc_r 1 124 5.52 125 5.47 118 5.84 723.llvm_r 1 96.0 5.28 97.7 5.19 96.3 5.27 727.cppcheck_r 1 66.8 5.38 66.8 5.37 67.0 5.36 729.abc_r 1 105 4.39 104 4.43 105 4.39 734.vpr_r 1 87.0 5.30 86.7 5.32 87.8 5.25 735.gem5_r 1 82.4 5.91 82.9 5.88 82.3 5.92 750.sealcrypto_r 1 45.3 11.8 43.3 12.4 45.2 11.9 753.ns3_r 1 81.1 7.56 81.0 7.57 81.2 7.55 777.zstd_r 1 166 3.88 166 3.88 144 4.48

SPECrate^®2026_int_base = 5.97 SPECrate^®2026_int_peak = Not Run

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Notes

 The compiler used was release candidate 2 of llvm 22.1.0,
 downloaded from github.com/llvm/llvm-project/releases/download/llvmorg-22.1.0-rc2
 built locally with GCC14 with default flags and clang, flang and lld projects
 following the instructions detailed here: https://llvm.org/docs/CMake.html

Operating System Notes

 ’ulimit -s unlimited’ was used to set environment stack size limit
 THP was enabled by running $echo always | sudo tee /sys/kernel/mm/transparent_hugepage/enabled

Environment Variables Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH =
     "/opt/llvm/llvm-22.1.0-rc2/lib64/:/opt/llvm/llvm-22.1.0-rc2/lib/:/lib64"

General Notes

 CPU consists of 2 heterogeneous clusters: with L3 of 8MB and 16MB respectively.
 Each CPU cluster is made up of 5 e-cores and 5 p-cores

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes

 Sysinfo program /opt/builds/spec2026/bin/sysinfo
 Rev: 069f95da7e7f5d81b2ce48a82150e54f
 running on spark-ca5f Fri Feb  6 10:24:39 2026

 SUT (System Under Test) info as seen by some common utilities.

 ------------------------------------------------------------
 Table of contents
 ------------------------------------------------------------
  1. uname -srvm
  2. w
  3. Username
  4. ulimit -a
  5. sysinfo process ancestry
  6. /proc/cpuinfo
  7. lscpu
  8. numactl --hardware
  9. /proc/meminfo
 10. who -r
 11. Systemd service manager version: systemd 255 (255.4-1ubuntu8.11)
 12. Services, from systemctl list-unit-files
 13. Linux kernel boot-time arguments, from /proc/cmdline
 14. cpupower frequency-info
 15. sysctl
 16. /sys/kernel/mm/transparent_hugepage
 17. /sys/kernel/mm/transparent_hugepage/khugepaged
 18. OS release
 19. Disk information
 20. /sys/devices/virtual/dmi/id
 21. dmidecode
 22. BIOS
 ------------------------------------------------------------

 ------------------------------------------------------------
 1. uname -srvm
   Linux 6.14.0-1013-nvidia #13-Ubuntu SMP PREEMPT_DYNAMIC Wed Oct 29 06:01:19 UTC 2025 aarch64

 ------------------------------------------------------------
 2. w
    10:24:39 up 2 days,  1:59,  2 users,  load average: 0.94, 0.99, 1.00
   USER     TTY      FROM             LOGIN@   IDLE   JCPU   PCPU  WHAT
   fralov01          10.34.125.5      08:02    1:18m  0.00s  0.03s sshd: fralov01 [priv]
   gdm      tty1     -                Wed08    2days  1:28   0.04s /usr/bin/gjs -m
   /usr/share/gnome-shell/org.gnome.ScreenSaver

 ------------------------------------------------------------

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

 3. Username
   From environment variable $USER:  root
   From the command ’logname’:       fralov01

 ------------------------------------------------------------
 4. ulimit -a
   time(seconds)        unlimited
   file(blocks)         unlimited
   data(kbytes)         unlimited
   stack(kbytes)        unlimited
   coredump(blocks)     0
   memory(kbytes)       unlimited
   locked memory(kbytes) 15688996
   process              511872
   nofiles              1024
   vmemory(kbytes)      unlimited
   locks                unlimited
   rtprio               0

 ------------------------------------------------------------
 5. sysinfo process ancestry
  /sbin/init splash
  sshd: /usr/sbin/sshd -D [listener] 0 of 10-100 startups
  sshd: fralov01 [priv]
  sshd: fralov01@pts/0
  -bash
  sudo bash
  sudo bash
  bash

  runcpu --config=llvm-rc-linux-aarch64-dgx-spark.cfg --action=run fprate intrate --iterations=4 --reportable
  runcpu --configfile llvm-rc-linux-aarch64-dgx-spark.cfg --action run --iterations 4 --reportable --nopower

    --runmode rate --tune base --size refrate intrate --nopreenv --note-preenv --logfile
    $SPEC/tmp/CPU2026.001/templogs/preenv.intrate.001.1.log --lognum 001.1 --from_runcpu 2
  specperl $SPEC/bin/sysinfo -f
 $SPEC = /opt/builds/spec2026

 ------------------------------------------------------------
 6. /proc/cpuinfo
     CPU implementer : 0x41
     CPU architecture: 8
     CPU variant     : 0x0
     CPU part        : 0xd85
     CPU part        : 0xd87
     CPU revision    : 1

     Features        : fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp cpuid asimdrdm jscvt
                       fcma lrcpc dcpop sha3 sm3 sm4 asimddp sha512 sve asimdfhm dit uscat ilrcpc flagm sb
                       paca pacg dcpodp sve2 sveaes svepmull svebitperm svesha3 svesm4 flagm2 frint svei8mm

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

                       svebf16 i8mm bf16 dgh bti ecv afp wfxt

    WARNING: the number of "processors" from /proc/cpuinfo does not seem to match the number of hardware

    threads as reported by lscpu.   Please verify counts independently.

 ------------------------------------------------------------
 7. lscpu

 From lscpu from util-linux 2.39.3:
   Architecture:                            aarch64
   CPU op-mode(s):                          64-bit
   Byte Order:                              Little Endian
   CPU(s):                                  20
   On-line CPU(s) list:                     0-19
   Vendor ID:                               ARM
   BIOS Vendor ID:                          NVIDIA
   Model name:                              Cortex-X925
   BIOS Model name:                         GB10 Spark CPU @ 3.9GHz
   BIOS CPU family:                         258
   Model:                                   1
   Thread(s) per core:                      1
   Core(s) per socket:                      10
   Socket(s):                               1
   Stepping:                                r0p1
   CPU(s) scaling MHz:                      116%
   CPU max MHz:                             4004.0000
   CPU min MHz:                             1378.0000
   BogoMIPS:                                2000.00

   Flags:                                   fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp
                                            cpuid asimdrdm jscvt fcma lrcpc dcpop sha3 sm3 sm4 asimddp sha512
                                            sve asimdfhm dit uscat ilrcpc flagm sb paca pacg dcpodp sve2
                                            sveaes svepmull svebitperm svesha3 svesm4 flagm2 frint svei8mm

                                            svebf16 i8mm bf16 dgh bti ecv afp wfxt
   Model name:                              Cortex-A725
   BIOS Model name:                         GB10 Spark CPU @ 3.9GHz
   BIOS CPU family:                         258
   Model:                                   1
   Thread(s) per core:                      1
   Core(s) per socket:                      10
   Socket(s):                               1
   Stepping:                                r0p1
   CPU(s) scaling MHz:                      83%
   CPU max MHz:                             2860.0000
   CPU min MHz:                             338.0000
   BogoMIPS:                                2000.00

   Flags:                                   fp asimd evtstrm aes pmull sha1 sha2 crc32 atomics fphp asimdhp
                                            cpuid asimdrdm jscvt fcma lrcpc dcpop sha3 sm3 sm4 asimddp sha512
                                            sve asimdfhm dit uscat ilrcpc flagm sb paca pacg dcpodp sve2

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

                                            sveaes svepmull svebitperm svesha3 svesm4 flagm2 frint svei8mm

                                            svebf16 i8mm bf16 dgh bti ecv afp wfxt
   L1d cache:                               1.3 MiB (20 instances)
   L1i cache:                               1.3 MiB (20 instances)
   L2 cache:                                25 MiB (20 instances)
   L3 cache:                                24 MiB (2 instances)
   NUMA node(s):                            1
   NUMA node0 CPU(s):                       0-19
   Vulnerability Gather data sampling:      Not affected
   Vulnerability Ghostwrite:                Not affected
   Vulnerability Indirect target selection: Not affected
   Vulnerability Itlb multihit:             Not affected
   Vulnerability L1tf:                      Not affected
   Vulnerability Mds:                       Not affected
   Vulnerability Meltdown:                  Not affected
   Vulnerability Mmio stale data:           Not affected
   Vulnerability Reg file data sampling:    Not affected
   Vulnerability Retbleed:                  Not affected
   Vulnerability Spec rstack overflow:      Not affected
   Vulnerability Spec store bypass:         Mitigation; Speculative Store Bypass disabled via prctl
   Vulnerability Spectre v1:                Mitigation; __user pointer sanitization
   Vulnerability Spectre v2:                Mitigation; CSV2, BHB
   Vulnerability Srbds:                     Not affected
   Vulnerability Tsa:                       Not affected
   Vulnerability Tsx async abort:           Not affected
   Vulnerability Vmscape:                   Not affected

 From lscpu --cache:
      NAME ONE-SIZE ALL-SIZE WAYS TYPE        LEVEL SETS PHY-LINE COHERENCY-SIZE
      L1d       64K     1.3M    4 Data            1  256                      64
      L1i       64K     1.3M    4 Instruction     1  256                      64
      L2       512K      25M    8 Unified         2 1024                      64
      L3         8M      24M   16 Unified         3 8192                      64

 ------------------------------------------------------------
 8. numactl --hardware
 NOTE: a numactl ’node’ might or might not correspond to a physical chip.
   available: 1 nodes (0)
   node 0 cpus: 0-19
   node 0 size: 122570 MB
   node 0 free: 42736 MB
   node distances:
   node   0
     0:  10

 ------------------------------------------------------------
 9. /proc/meminfo

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

    MemTotal:       125511968 kB

 ------------------------------------------------------------
 10. who -r
   run-level 5 Feb 4 08:25

 ------------------------------------------------------------
 11. Systemd service manager version: systemd 255 (255.4-1ubuntu8.11)
   Default Target  Status
   graphical       running

 ------------------------------------------------------------
 12. Services, from systemctl list-unit-files
   STATE            UNIT FILES

   enabled          ModemManager NetworkManager NetworkManager-dispatcher accounts-daemon anacron apparmor
                    apport avahi-daemon blk-availability bluetooth cfg-iommu cloud-config cloud-final
                    cloud-init cloud-init-local console-setup containerd cron cups cups-browsed dgx-dashboard
                    dgx-dashboard-admin dgx-release dgxstation-desktop dmesg docker e2scrub_reap finalrd
                    getty@ gnome-remote-desktop grub-common grub-initrd-fallback kdump-tools keyboard-setup
                    lvm2-monitor multipathd networkd-dispatcher nv-cpu-governor nv-docker-gpus
                    nvidia-cdi-refresh nvidia-conf-xconfig nvidia-console-settings nvidia-disable-aqc-nic
                    nvidia-disable-init-on-alloc nvidia-disable-numa-balancing nvidia-earlycon
                    nvidia-enable-power-meter-cap nvidia-grubserial nvidia-hibernate

                    nvidia-nvme-interrupt-coalescing nvidia-pci-realloc nvidia-persistenced nvidia-raid-config
                    nvidia-redfish-config nvidia-resume nvidia-spark-run-apt-upgrade-once nvidia-suspend
                    nvmefc-boot-connections nvmf-autoconnect open-iscsi open-vm-tools openvpn pollinate
                    ras-mc-ctl rasdaemon restart-resolved rsyslog samba-ad-dc secureboot-db setvtrgb
                    smartmontools snapd srp_daemon ssl-cert switcheroo-control sysstat systemd-pstore
                    systemd-resolved systemd-timesyncd ua-reboot-cmds ubuntu-advantage udisks2 ufw vgauth

                    wpa_supplicant
   enabled-runtime  netplan-ovs-cleanup systemd-fsck-root systemd-remount-fs

   disabled         NetworkManager-wait-online brltty console-getty debug-shell dgx-oobe dgx-oobe-admin
                    dgx-oobe-hostname dgx-oobe-hotspot dgx-oobe-hotspot-watchdog dgx-oobe-ubuntu-pro-activate
                    dnsmasq dnsmasq@ iperf3 ipmievd iscsid nftables nmbd nvidia-desktop-default-snaps
                    nvidia-dgx-sol nvidia-dgx-telemetry nvidia-remove-gnome-software-once

                    nvidia-spark-mlnx-firmware-manager nvidia-spark-remove-once nvidia-suspend-then-hibernate
                    openvpn-client@ openvpn-server@ openvpn@ quota quotarpc rpcbind rsync rtkit-daemon
                    setup-oem-config-override smbd speech-dispatcherd srp_daemon_port@ ssh

                    systemd-boot-check-no-failures systemd-confext systemd-network-generator systemd-networkd
                    systemd-networkd-wait-online systemd-networkd-wait-online@ systemd-pcrlock-file-system
                    systemd-pcrlock-firmware-code systemd-pcrlock-firmware-config systemd-pcrlock-machine-id

                    systemd-pcrlock-make-policy systemd-pcrlock-secureboot-authority
                    systemd-pcrlock-secureboot-policy systemd-sysext systemd-time-wait-sync upower
                    wpa_supplicant-nl80211@ wpa_supplicant-wired@ wpa_supplicant@
   generated        speech-dispatcher

   indirect         saned@ serial-getty@ spice-vdagentd systemd-sysupdate systemd-sysupdate-reboot uuidd
   masked           alsa-utils cryptdisks cryptdisks-early hwclock multipath-tools-boot nfs-common nvsm

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

                    nvsm-api-gateway nvsm-core nvsm-exporter nvsm-mqtt nvsm-notifier saned screen-cleanup sudo

                    x11-common

 ------------------------------------------------------------
 13. Linux kernel boot-time arguments, from /proc/cmdline
   BOOT_IMAGE=/boot/vmlinuz-6.14.0-1013-nvidia
   root=UUID=d27bfd26-ff30-400e-9eca-9cdf73de9406
   ro
   init_on_alloc=0
   console=tty0
   plymouth.ignore-serial-consoles
   plymouth.use-simpledrm
   earlycon=uart,mmio32,0x16A00000
   console=tty0
   console=ttyS0,921600
   crashkernel=1G-:0M
   quiet
   splash
   pci=pcie_bus_safe
   vt.handoff=7

 ------------------------------------------------------------
 14. cpupower frequency-info
   analyzing CPU 19:
     current policy: frequency should be within 1.38 GHz and 4.00 GHz.
                     The governor "performance" may decide which speed to use
                     within this range.

 ------------------------------------------------------------
 15. sysctl
   kernel.numa_balancing               0
   kernel.randomize_va_space           2
   vm.compaction_proactiveness        20
   vm.dirty_background_bytes           0
   vm.dirty_background_ratio          10
   vm.dirty_bytes                      0
   vm.dirty_expire_centisecs        3000
   vm.dirty_ratio                     20
   vm.dirty_writeback_centisecs      500
   vm.dirtytime_expire_seconds     43200
   vm.extfrag_threshold              500
   vm.min_unmapped_ratio               1
   vm.nr_hugepages                     0
   vm.nr_hugepages_mempolicy           0
   vm.nr_overcommit_hugepages          0
   vm.swappiness                      60
   vm.watermark_boost_factor       15000

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

   vm.watermark_scale_factor          10
   vm.zone_reclaim_mode                0

 ------------------------------------------------------------
 16. /sys/kernel/mm/transparent_hugepage
   defrag          always defer defer+madvise [madvise] never
   enabled         [always] madvise never
   hpage_pmd_size  2097152
   shmem_enabled   always within_size advise [never] deny force

 ------------------------------------------------------------
 17. /sys/kernel/mm/transparent_hugepage/khugepaged
   alloc_sleep_millisecs   60000
   defrag                      1
   max_ptes_none             511
   max_ptes_shared           256
   max_ptes_swap              64
   pages_to_scan            4096
   scan_sleep_millisecs    10000

 ------------------------------------------------------------
 18. OS release
   From /etc/*-release /etc/*-version
   os-release  Ubuntu 24.04.3 LTS
   dgx-release DGX_NAME="DGX Spark"

 ------------------------------------------------------------
 19. Disk information
 SPEC is set to: /opt/builds/spec2026
   Filesystem     Type  Size  Used Avail Use% Mounted on
   /dev/nvme0n1p2 ext4  3.7T  493G  3.0T  14% /

 ------------------------------------------------------------
 20. /sys/devices/virtual/dmi/id
     Vendor:         NVIDIA
     Product:        NVIDIA_DGX_Spark
     Product Family: DGX Spark
     Serial:         1984025007657

 ------------------------------------------------------------
 21. dmidecode

   Additional information from dmidecode 3.5 follows.  WARNING: Use caution when you interpret this section.
   The ’dmidecode’ program reads system data which is "intended to allow hardware to be accurately
   determined", but the intent may not be met, as there are frequent changes to hardware, firmware, and the

   "DMTF SMBIOS" standard.
   Memory:
     1x SK Hynix None 128 GB 8533

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Platform Notes (Continued)

 ------------------------------------------------------------
 22. BIOS
 (This section combines info from /sys/devices and dmidecode.)
    BIOS Vendor:       American Megatrends International, LLC.
    BIOS Version:      5.36_0ACUM018
    BIOS Date:         08/06/2025
    BIOS Revision:     5.36

Compiler Version Notes

==============================================================================
C      | 708.sqlite_r(base) 714.cpython_r(base) 777.zstd_r(base)
------------------------------------------------------------------------------
clang version 22.1.0-rc2
Target: aarch64-unknown-linux-gnu
Thread model: posix
InstalledDir: /opt/llvm/llvm-22.1.0-rc2/bin
------------------------------------------------------------------------------

==============================================================================
C++    | 706.stockfish_r(base) 707.ntest_r(base) 727.cppcheck_r(base)
       | 753.ns3_r(base)
------------------------------------------------------------------------------
clang version 22.1.0-rc2
Target: aarch64-unknown-linux-gnu
Thread model: posix
InstalledDir: /opt/llvm/llvm-22.1.0-rc2/bin
------------------------------------------------------------------------------

==============================================================================
C++, C | 710.omnetpp_r(base) 721.gcc_r(base) 723.llvm_r(base) 729.abc_r(base)
       | 734.vpr_r(base) 735.gem5_r(base) 750.sealcrypto_r(base)
------------------------------------------------------------------------------
clang version 22.1.0-rc2
Target: aarch64-unknown-linux-gnu
Thread model: posix
InstalledDir: /opt/llvm/llvm-22.1.0-rc2/bin
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

clang

(Continued on next page)

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Base Compiler Invocation (Continued)

C++ benchmarks:

clang++

Benchmarks using both C and C++:

clang++ clang

Base Portability Flags

706.stockfish_r: -DSPEC_LP64 707.ntest_r: -DSPEC_LP64 708.sqlite_r: -DSPEC_LP64 710.omnetpp_r: -fno-finite-math-only -DSPEC_LP64 714.cpython_r: -DSPEC_LP64 721.gcc_r: -DSPEC_LP64 723.llvm_r: -DSPEC_LP64 727.cppcheck_r: -DSPEC_LP64 729.abc_r: -DSPEC_LP64 734.vpr_r: -fno-finite-math-only -DSPEC_LP64 735.gem5_r: -fno-finite-math-only -DSPEC_LP64 750.sealcrypto_r: -DSPEC_LP64 753.ns3_r: -fno-finite-math-only -DSPEC_LP64 777.zstd_r: -DSPEC_LP64

Base Optimization Flags

C benchmarks:

-fuse-ld=lld -std=c18 -g -O3 -mcpu=native -ffast-math -flto=thin
-fomit-frame-pointer

C++ benchmarks:

706.stockfish_r: -fuse-ld=lld -std=c++17 -g -O3 -mcpu=native

-ffast-math -flto=thin -fomit-frame-pointer -pthread

707.ntest_r: -fuse-ld=lld -std=c++17 -g -O3 -mcpu=native

-ffast-math -flto=thin -fomit-frame-pointer

727.cppcheck_r: Same as 707.ntest_r

(Continued on next page)

Page 12 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/

SPEC CPU^®2026 Integer Rate Result

Copyright 2026 Standard Performance Evaluation Corporation

(Test Sponsor: Arm)

NVIDIA

(3.9 GHz NVIDIA GB10 CPU)

NVIDIA DGX Spark SPECrate®2026_int_peak = Not Run

SPECrate^®2026_int_base = 5.97

CPU2026 License: 9044 Test Date: Feb-2026 Test Sponsor: Arm Hardware Availability: Oct-2025 Tested by: Arm Software Availability: Feb-2026

Base Optimization Flags (Continued)

753.ns3_r: Same as 707.ntest_r Benchmarks using both C and C++: 710.omnetpp_r: -fuse-ld=lld -std=c++17 -std=c18 -g -O3 -mcpu=native

-ffast-math -flto=thin -fomit-frame-pointer

721.gcc_r: Same as 710.omnetpp_r 723.llvm_r: -fuse-ld=lld -std=c++17 -std=c18 -g -O3 -mcpu=native

-ffast-math -flto=thin -fomit-frame-pointer -pthread

729.abc_r: Same as 710.omnetpp_r 734.vpr_r: Same as 710.omnetpp_r 735.gem5_r: Same as 723.llvm_r 750.sealcrypto_r: Same as 710.omnetpp_r

The flags files that were used to format this result can be browsed at

http://www.spec.org/cpu2026/results/flags/llvm-rev-A2.html
http://www.spec.org/cpu2026/results/flags/Nvidia-Platform-Settings.html

You can also download the XML flags sources by saving the following links:

http://www.spec.org/cpu2026/results/flags/llvm-rev-A2.xml
http://www.spec.org/cpu2026/results/flags/Nvidia-Platform-Settings.xml

Originally published on 2026-05-05.

Report generated on 2026-05-04 23:30:37 by CPU2026 PS formatter (86729d3b).

Tested with SPEC CPU^®2026 v0.902.0 on 2026-02-06 05:24:39-0500.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

names appearing in this result are trademarks or registered trademarks of their respective holders.

SPEC CPU and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and product