Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Fujitsu Limited

PRIMEPOWER HPC2500 ( 2.08GHz )

SPECompMpeak2001 = SPECompMbase2001 =

53901 50609

SPEC license #:HPG0003 Tested by: Fujitsu Limited Test site: Numazu, Japan Test date: Aug-2004 Hardware Avail:Jun-2004 Software Avail:Sep-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 100000 200000 300000

310.wupwise_m 6000 82.1 73045 80.6 74400

312.swim_m 6000 138 43563 137 43761

314.mgrid_m 7300 166 44023 166 44023

316.applu_m 4000 26.7 150067 26.8 149311

318.galgel_m 5100 204 24987 201 25324

320.equake_m 2600 76.1 34170 52.0 49960

324.apsi_m 3400 34.5 98409 34.2 99372

326.gafort_m 8700 151 57577 144 60278

328.fma3d_m 4600 153 29985 137 33657

330.art_m 6400 57.6 111077 57.6 111077

332.ammp_m 7000 425 16468 380 18401

Hardware

CPU: SPARC64 V CPU MHz: 2080 FPU: Integrated CPU(s) enabled: 64 cores, 64 chips, 1 core/chip CPU(s) orderable: 8 to 128 Primary Cache: 128KBI+128KBD on chip Secondary Cache: 4MB(I+D) on chip, per core L3 Cache: None Other Cache: None Memory: 256GB Disk Subsystem: 1x 73GB Ultra SCSI Other Hardware: None

Software

OpenMP Threads: 63 Parallel: OpenMP Operating System: Solaris 8_{Fujitsu Parallelnavi 2.3 (NQS, CPU scheduler, largepage)}

Compiler: Fujitsu Parallelnavi 2.4 (C & F90) File System: ufs System State: Multi-user

Notes/Tuning Information

 Baseline flags:
     C:    -KOMP,fast_GP2=2,V9,hardbarrier,largepage=1,prefetch=2
            preex,a8,mfunc,ilfunc -O5 -x-
     F90:  -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=4,
            prefetch_cache_level=3,mfunc=2 -O5 -Nautoobjstack

 Base User Environment:
     ENV_OMP_NUM_THREADS = 62

 Portability Flags:
     318.galgel_m:  -Am -Fixed -w
     328.fma3d_m:   -Am

 Extra Flags:
      330.art_m:    -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Peak Optimization Flags:

  310.wupwise_m:
      F90: -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=7,
           prefetch_cache_level=3,mfunc=2,ilfunc -O5 -Nautoobjstack

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Fujitsu Limited

PRIMEPOWER HPC2500 ( 2.08GHz )

SPECompMpeak2001 = SPECompMbase2001 =

53901 50609

SPEC license #:HPG0003 Tested by: Fujitsu Limited Test site: Numazu, Japan Test date: Aug-2004 Hardware Avail:Jun-2004 Software Avail:Sep-2004

Notes/Tuning Information (Continued)

  312.swim_m:
      F90: -KOMP,fast_GP2=2,V9,hardbarrier,largepage=1,prefetch_line=7,
           prefetch_cache_level=3,mfunc=2 -O5 -Nautoobjstack
  316.applu_m:
      F90: -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=4,
           prefetch_cache_level=3,mfunc=2,bcopy -O5 -Nautoobjstack
  318.galgel_m:
      F90: -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=4,
           prefetch_cache_level=3,mfunc=2 -x70 -O5 -Nautoobjstack
  326.gafort_m:
      F90: -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=4,
           prefetch_cache_level=3,mfunc=2 -O5 -Nautoobjstack
           -Kunroll=4
  328.fma3d_m:
      F90: -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch_line=6,
           prefetch_cache_level=3,mfunc=2 -O5 -Nautoobjstack
           -Kcommonpad=8,prefetch_infer
  332.ammp_m:
      C:   -KOMP,fast_GP2=2,V8PLUS,hardbarrier,largepage=1,prefetch=2,preex

 Alternate sources:

 Add critical region around update of linked list in parallel loop.
 Compulsory src.alt available as ompm-purdue1-20040324.tar.gz
 Used for 330.art_m base and peak.

 Peak sources:

 SPEC OMPL2001 source for 32bit systems modified for SPEC OMPM2001.
 Available as ompl src.alt in the SPEC OMP v3.0 release.
 Used for 316.applu_m, 320.equake_m, 324.apsi_m, 326.gafort_m, and 328.fma3d_m.

 System tunables:
     /etc/system:
         set shmsys:shminfo_shmmax=2147483648
         set shmsys:shminfo_shmmni=256
         set shmsys:shminfo_shmseg=256
         set autoup=172800
         set memscrub_period_sec=345600
     /etc/opt/FJSVpnrm/lpg.conf:
         JOB=192G,SHMSEGSIZE=2048M
     /etc/opt/FJSVpnrm/cpursc.conf:
         CPU_USE=0:0
     NQS:
         Per-process data size limit = UNLIMITED
         Per-process permanent file size limit = UNLIMITED
         Per-process memory size limit = 128 gigabytes
         Per-request memory size limit = 128 gigabytes
         Per-process number of cpus limit = 63
         Per-process stack size limit = 4 gigabytes
         Per-process CPU time limit = 2147483646.000
         Execution mode = SImplex
         Jobclass = 0

 Submitting the runspec to NQS:
     Run the qsub command with the following sh script.

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Fujitsu Limited

PRIMEPOWER HPC2500 ( 2.08GHz )

SPECompMpeak2001 = SPECompMbase2001 =

53901 50609

SPEC license #:HPG0003 Tested by: Fujitsu Limited Test site: Numazu, Japan Test date: Aug-2004 Hardware Avail:Jun-2004 Software Avail:Sep-2004

Notes/Tuning Information (Continued)

         cd /spec/omp2001
         . ./shrc
         OMP_NUM_THREADS=63
         export OMP_NUM_THREADS
         runspec --config=Fujitsu --reportable --tune=all medium