Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer GS1280 7/1300

SPECompMpeak2001 = SPECompMbase2001 =

42044 32727

SPEC license #:HPG0009 Tested by: Hewlett-Packard Company Test site: Marlborough, MA Test date: Sep-2004 Hardware Avail:Aug-2004 Software Avail: Jul-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 100000 200000 300000

310.wupwise_m 6000 176 34090 93.7 64004

312.swim_m 6000 58.0 103379 35.1 171122

314.mgrid_m 7300 136 53637 117 62370

316.applu_m 4000 53.9 74216 44.9 89175

318.galgel_m 5100 268 19044 265 19269

320.equake_m 2600 277 9391 141 18423

324.apsi_m 3400 80.4 42296 65.8 51702

326.gafort_m 8700 260 33510 229 38007

328.fma3d_m 4600 247 18604 180 25546

330.art_m 6400 119 53808 125 51238

332.ammp_m 7000 540 12959 537 13047

Hardware

CPU: Alpha 21364 CPU MHz: 1300 FPU: Integrated CPU(s) enabled: 32 cores, 32 chips, 1 core/chip CPU(s) orderable: 2 to 64 Primary Cache: 64KB(I)+64KB(D) on chip Secondary Cache: 1.75MB on chip per CPU L3 Cache: None Other Cache: None Memory: 2GB per core; 256MB RIMMs; 64GB total Disk Subsystem: 36GB Ultra 160 10KRPM Other Hardware: None

Software

OpenMP Threads: 32 Parallel: OpenMP Operating System: Tru64 UNIX V5.1B-1 + Patch Kit 4 Compiler: HP Fortran V5.5A-3548-48D88 Compaq C V6.5-011-48C5K File System: UFS System State: Multi-user

Notes/Tuning Information

 MP_STACK_SIZE=10000000
 4Mb pages used (sysconfigtab)
 no processor sets used

 Tuning pseudo-switches:
    +BPD - Big page disable
    +PFB - Post-link feedback for prefetches
    See the flags description or the configuration file
    for more details.

 Base:
    Fortran: f90 -arch ev7 -fast -omp -O5
    C: cc -arch ev7 -fast -omp -O4
    alternate source purdue1 for 330.art_m
 Peak:
 All use  -arch host -omp ONESTEP
   Individual benchmark tuning:
    310.wupwise_m: f90 -arch host -omp -call_shared
        -inline all -unroll 12 -align commons
        +PFB +BPD
    alternate source ompl.32

    312.swim_m: f90 -arch host -omp -fast -O5

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer GS1280 7/1300

SPECompMpeak2001 = SPECompMbase2001 =

42044 32727

SPEC license #:HPG0009 Tested by: Hewlett-Packard Company Test site: Marlborough, MA Test date: Sep-2004 Hardware Avail:Aug-2004 Software Avail: Jul-2004

Notes/Tuning Information (Continued)

        +PFB +BPD
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    314.mgrid_m: f90 -arch host -omp -O5 -transform_loops
        -tune ev7 -unroll 8
        +PFB +BPD
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    316.applu_m: f90 -arch host -omp -fast -O5 -unroll 14
        +PFB
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    318.galgel_m: f90 -arch host -omp -fast -unroll 5 -O5
        +PFB

    320.equake_m: cc -arch host -omp -fast -call_shared
        -O4 -ldensemalloc -assume restricted_pointers
        -inline speed -unroll 13
        +PFB +BPD
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    324.apsi_m: f90 -arch host -omp -O5 -transform_loops
        -unroll 8
        +PFB
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    326.gafort_m: f90 -arch host -omp -fast -O5
        -arch ev67 -tune ev67
    alternate source ompl.32

    328.fma3d: f90 -arch host -omp -fast -O4
        -transform_loops
        +PFB +BPD
    PTHREAD_CONFIG=feature=def-scs,d4-scs
    alternate source ompl.32

    330.art_m: cc -arch host -omp -assume whole_program
        -ldensemalloc -call_shared
        -assume restricted_pointers -fast -O4 -unroll 16
        -inline none
        +PFB +BPD
    alternate source purdue1

    332.ammp_m: cc -arch host -omp -O4 -ifo
        -assume nomath_errno
        -assume trusted_short_alignment -fp_reorder
        -readonly_strings -ldensemalloc
        -assume restricted_pointers -unroll 9
    PTHREAD_CONFIG=feature=def-scs,d4-scs

 Information on UNIX V5.1B Patches can be found at

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard Company AlphaServer GS1280 7/1300

SPECompMpeak2001 = SPECompMbase2001 =

42044 32727

SPEC license #:HPG0009 Tested by: Hewlett-Packard Company Test site: Marlborough, MA Test date: Sep-2004 Hardware Avail:Aug-2004 Software Avail: Jul-2004

Notes/Tuning Information (Continued)

 http://h30097.www3.hp.com/docs/patch/51B/bl25/ReleaseNotes.pdf

 The densemalloc library provides an alternate set of malloc
 routines that implement a "dense malloc" memory allocation
 strategy.  This can  improve run time performance by reducing
 bookkeeping overhead and rounding up padding attached to
 allocated chunks.
 File containing flag descriptions can be found at
 http://www.spec.org/omp/results/flags/HP-ALPHA-TRU64-F90-CompaqC.txt