Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder n6650w (S2915) (AMD Opteron 8220)

SPECompMpeak2001 = SPECompMbase2001 =

10085 9565

SPEC license #:HPG0017 Tested by: AMD Test site: Austin TX Test date: Nov-2006 Hardware Avail:Nov-2006 Software Avail:Oct-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 10000 20000 30000

310.wupwise_m 6000 547 10975 537 11163

312.swim_m 6000 602 9970 602 9970

314.mgrid_m 7300 699 10445 709 10303

316.applu_m 4000 426 9397 417 9587

318.galgel_m 5100 506 10074 579 8805

320.equake_m 2600 196 13289 189 13737

324.apsi_m 3400 402 8459 306 11102

326.gafort_m 8700 1374 6331 1374 6331

328.fma3d_m 4600 573 8027 571 8056

330.art_m 6400 368 17398 247 25935

332.ammp_m 7000 1228 5701 1245 5623

Hardware

CPU: AMD Opteron(tm) Processor 8220 CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 1,2 Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 8x512MB, PC2-5300 CL4 Disk Subsystem: 250GB 7200 rpm SATA Other Hardware: None

Software

OpenMP Threads: 4 Parallel: OpenMP + Auto Concurrentization Operating System: SLES9 SP3 64bit Compiler: PGI Fortran 6.2-4 File System: Linux/ext3 System State: Multi-User

Notes/Tuning Information

 Extra art Base Flags
   330.art_m (extra): -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Base tuning:
   C       : pgcc  -mp -tp=k8-64 -fastsse -O4 -Minline=levels:8 -mcmodel=medium
   Fortran : pgf90 -mp -tp=k8-64 -fastsse -O4 -Minline=levels:8 -mcmodel=medium
   ONESTEP=yes

 Peak tuning:
  ONESTEP=yes for all peak tests.

  310.wupwise_m   : -mp -tp=k8-64 -fastsse -Minline=level:8  -mcmodel=medium
  312.swim_m      : basepeak=yes
  314.mgrid_m     : -mp -tp=k8-64 -fastsse    -Mnofptrap -Mlongbranch

  316.applu_m     :  -mp -tp=k8-64 -fastsse -O4  -Minline=levels:8 -Mipa=fast,inline -Mfprelaxed=rsqrt -mcmodel=medium

                    srcalt = ompl.32

  318.galgel_m    : -mp -tp=k8-64 -fastsse -Mconcur -Mipa=fast,inline -Mfprelaxed=rsqrt -mcmodel=medium

                    -I/opt/acml3.5.0/pgi64/include -L/opt/acml3.5.0/pgi64/lib -lacml
                    RM_SOURCES=lapak.f90
  320.equake_m    : -mp -tp=k8-64 -fastsse -Mipa=fast,inline -Mfprelaxed=rsqrt -mcmodel=medium
                    srcalt = ompl.32
  324.apsi_m      : -mp -tp=k8-64 -fastsse -O4 -Minline=levels:8 -mcmodel=medium
                    srcalt = ompl.32

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder n6650w (S2915) (AMD Opteron 8220)

SPECompMpeak2001 = SPECompMbase2001 =

10085 9565

SPEC license #:HPG0017 Tested by: AMD Test site: Austin TX Test date: Nov-2006 Hardware Avail:Nov-2006 Software Avail:Oct-2006

Notes/Tuning Information (Continued)

  326.gafort_m    : basepeak=yes
  328.fma3d_m     : -mp -tp=k8-64 -fastsse -O4  -Mvect=assoc -Minline -mcmodel=medium

  330.art_m       : -mp -fast  -Mscalarsse -Mcache_align -Mflushz -Minline -Mpa=fast,inline -Mfprelaxed=rsqrt -mcmodel=medium

  332.ammp_m      : -mp -tp=k8-64 -fastsse  -O -Minline  -Mframe -Mipa=fast,inline -Mfprelaxed=rsqrt

 Portability flags:
  318.galgel_m    : -Mfixed -Mextend

 Base and Peak User Environment (bash):
   export OMP_NUM_THREADS=4
   export OMP_DYNAMIC=FALSE
   export PGI=/opt/pgi
   export LD_LIBRARY_PATH=/opt/acml3.5.0/pgi64/lib
   ulimit -s unlimited

 Default BIOS settings used.
 System can be built using a standard EATX case, Matrox Millennium G450 PCI
 graphics adapter and an Antec True550 EPS12V power supply.
 PGI compiler flags are in AMD-20061107-pgi62_flags.txt.