Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

IBM Corporation

IBM BladeCenter JS22 (4.0 GHz, 4 core)

SPECompMpeak2001 = SPECompMbase2001 =

19568 18218

SPEC license #:HPG0005 Tested by: IBM Test site: Austin, TX Test date: Oct-2007 Hardware Avail:Nov-2007 Software Avail:Nov-2007

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 20000 40000 60000

310.wupwise_m 6000 239 25120 239 25120

312.swim_m 6000 374 16057 355 16893

314.mgrid_m 7300 474 15410 380 19190

316.applu_m 4000 286 13976 263 15217

318.galgel_m 5100 291 17526 237 21490

320.equake_m 2600 137 18923 122 21380

324.apsi_m 3400 175 19476 163 20845

326.gafort_m 8700 539 16133 539 16133

328.fma3d_m 4600 377 12194 362 12709

330.art_m 6400 122 52331 122 52312

332.ammp_m 7000 551 12699 553 12652

Hardware

CPU: POWER6 CPU MHz: 4000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip, 2 threads/core CPU(s) orderable: 4 cores Primary Cache: 64 KB I + 64 KB D on chip per core Secondary Cache: 4 MB I+D on chip per core L3 Cache: None Other Cache: None Memory: 16 GB (4x4 GB) DDR2 667 MHz Disk Subsystem: 1x146 GB SAS 15K RPM Other Hardware: None

Software

OpenMP Threads: 8 Parallel: OpenMP Operating System: IBM AIX 5L V5.3 Compiler: XL C/C++ Enterprise Edition Version 9.0 for AIX

XL Fortran Enterprise Edition Version 11.1 for AIX Other Software: IBM Engineering and Scientific Subroutine Library (ESSL) version 4.3.0.2

File System: AIX/JFS2 System State: Multi-user

Notes/Tuning Information

      Portability Flags Variables
         -qfixed used in: 310.wupwise_m, 312.swim_m, 314.mgrid_m, 316.applu_m, 324.apsi_m
         -qfixed=80 used in: 318.galgel_m
         -qsuffix=f=f90 used in: 318.galgel_m, 326.gafort_m, 328.fma3d_m

     Base Flags
       FORTRAN: -qsmp=omp -qipa=partition=large -qmaxmem=-1 -qsuppress=cmpmsg
                -O5 -bmaxdata:0x80000000
       C:       -qsmp=omp -qipa=partition=large -qmaxmem=-1
                -O5 -bmaxdata:0x80000000

     Base & Peak User Environment:
       OMP_DYNAMIC=FALSE
       MALLOCOPTIONS=multiheap
       MEMORY_AFFINITY=MCM
       XLFRTEOPTS=intrinthds=1
       ENV_XLSMPOPTS=SPINS=0:YIELDS=0:STACK=8000000:SCHEDULE=STATIC:STARTPROC=0:STRIDE=1
       OMP_NUM_THREADS=8

      Peak sources:

         Approved SPEC OMPL2001 source for 32bit systems modified for SPEC OMPM2001 used with 320.equake_m.

     Peak Flags:

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

IBM Corporation

IBM BladeCenter JS22 (4.0 GHz, 4 core)

SPECompMpeak2001 = SPECompMbase2001 =

19568 18218

SPEC license #:HPG0005 Tested by: IBM Test site: Austin, TX Test date: Oct-2007 Hardware Avail:Nov-2007 Software Avail:Nov-2007

Notes/Tuning Information (Continued)

         310.wupwise_m:  basepeak=1
         312.swim_m:     -qsmp=omp -qipa=partition=large -qmaxmem=-1
                         -O5 -qenablevmx -qvecnvol -qessl

                         -bdatapsize:64K -bstackpsize:64K -btextpsize:64K -bmaxdata:0x80000000 -lesslsmp

         314.mgrid_m:    -qsmp=omp -qipa=partition=large -qmaxmem=-1 -qsuppress=cmpmsg
                         -pdf1/pdf2 -O5 -q64 -qalign=struct=natural
                         -bdatapsize:64K -bstackpsize:64K
                         ENV_OMP_NUM_THREADS=4

                         ENV_XLSMPOPTS=SPINS=0:YIELDS=0:STACK=8000000:SCHEDULE=STATIC:STARTPROC=0:STRIDE=2

         316.applu_m:    -qsmp=omp -qipa=partition=large -qmaxmem=-1
                         -O5 -qenablevmx -qvecnvol -qessl

                         -bdatapsize:64K -bstackpsize:64K -btextpsize:64K -bmaxdata:0x80000000 -lesslsmp

         318.galgel_m:   -qsmp=omp -qipa=partition=large -qmaxmem=-1 -qsuppress=cmpmsg
                         -O4 -q64 -qessl
                         -bdatapsize:64K -bstackpsize:64K -lesslsmp
         320.equake_m:   -qsmp=omp -qipa=partition=large -qmaxmem=-1
                         -pdf1/pdf2 -O5 -qhot=arraypad -Q
                         -btextpsize:64K -bdatapsize:64K -bmaxdata:0x80000000
         324.apsi_m:     -qsmp=omp -qipa=partition=large -qmaxmem=-1 -qsuppress=cmpmsg
                         -O5 -qenablevmx -qvecnvol -qessl

                         -bdatapsize:64K -bstackpsize:64K -btextpsize:64K -bmaxdata:0x80000000 -lesslsmp

         326.gafort_m:   basepeak=1
         328.fma3d_m:    -qsmp=omp -qipa=partition=large -qmaxmem=-1 -qsuppress=cmpmsg
                         -O5
                         -bmaxdata:0x80000000 -btextpsize:64K -bdatapsize:64K
         330.art_m:      -qsmp=omp -qipa=partition=large -qmaxmem=-1
                         -O5 -qenablevmx -qvecnvol -qessl
                         -bdatapsize:64K -bstackpsize:64K -btextpsize:64K -bmaxdata:0x80000000
         332.ammp_m:     -qsmp=omp -qipa=partition=large -qmaxmem=-1
                         -O5
                         -btextpsize:64K -bdatapsize:64K -bstackpsize:64K -bmaxdata:0x80000000

      The installed OS level is AIX 5L for POWER version 5.3 with the 5300-07 Technology Level.
      IBM XL Compilers updated to October 2007 PTF Level.
      C:              IBM XL C for AIX invoked as xlc_r
      Fortran:        IBM XL Fortran for AIX invoked as xlf90_r

      ulimits set to unlimited.
      User system privileges (capabilities) and Large Pages are set as follows:
          vmo -r -o lgpg_regions=256 -o lgpg_size=16777216
          chuser capabilities=CAP_BYPASS_RAC_VMM,CAP_PROPAGATE $USER
          bosboot -aD
          shutdown -rF

      Use flags-description file IBM-20070606-AIX.txt