Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Tyan Computer Corporation Tyan Thunder n425QE (S4985E)

SPECompMpeak2001 = SPECompMbase2001 =

28283 27001

SPEC license #:HPG0017 Tested by: Advanced Micro Devices Test site: Austin, TX Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Nov-2007

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 30000 60000 90000

310.wupwise_m 6000 146 41227 134 44895

312.swim_m 6000 251 23941 212 28351

314.mgrid_m 7300 239 30496 239 30496

316.applu_m 4000 260 15391 260 15391

318.galgel_m 5100 244 20928 244 20928

320.equake_m 2600 105 24748 87.3 29789

324.apsi_m 3400 96.1 35383 90.8 37452

326.gafort_m 8700 295 29469 295 29469

328.fma3d_m 4600 251 18314 251 18314

330.art_m 6400 82.7 77397 82.7 77397

332.ammp_m 7000 446 15684 440 15902

Hardware

CPU: AMD Opteron Processor 8356 CPU MHz: 2300 FPU: Integrated CPU(s) enabled: 16 cores, 4 chips, 4 cores/chip CPU(s) orderable: 1-4 Primary Cache: 64 KB I + 64 KB D on chip per core Secondary Cache: 512 KB I+D on chip per core L3 Cache: 2 MB I+D on chip per chip Other Cache: None Memory: 32GB (16x2GB, PC2-5300, CL5 dual-rank) Disk Subsystem: 250GB 7200 RPM SATA Other Hardware: None

Software

OpenMP Threads: 16 Parallel: OpenMP Operating System: SLES10 SP1 64bit Compiler: PathScale Compiler Suite ver. 3.1 File System: Linux/Ext3 System State: Multi-User

Notes/Tuning Information

 Extra art Base Flags
   330.art_m (extra): -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Base Tuning:
   C       : pathcc  -mp -Ofast -mcmodel=medium
   Fortran : pathf90 -mp -Ofast -OPT:early_mp=on -mcmodel=medium
   ONESTEP=yes
 Peak Tuning:
    310.wupwise_m: -mp -Ofast -msse3 -LNO:prefetch_ahead=5:prefetch=3
                   -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
                   -IPA:linear=on:plimit=50000:callee_limit=5000
    312.swim_m: -mp -O3 -OPT:Ofast -m3dnow -mcmodel=medium -LNO:simd=0
    314.mgrid_m: basepeak=yes
    316.applu_m: basepeak=yes
    318.galgel_m: basepeak=yes
    320.equake_m: -Ofast -mp -OPT:alias=disjoint
    324.apsi_m: -mp -O3 -OPT:Ofast -TENV:x=4 -LNO:fusion=2:prefetch=0
    326.gafort_m: basepeak=yes
    328.fma3d_m: basepeak=yes
    330.art_m: basepeak=yes
    332.ammp_m: -mp -Ofast -mcpu=opteron -mcmodel=medium

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2008, Standard Performance Evaluation Corporation

Tyan Computer Corporation Tyan Thunder n425QE (S4985E)

SPECompMpeak2001 = SPECompMbase2001 =

28283 27001

SPEC license #:HPG0017 Tested by: Advanced Micro Devices Test site: Austin, TX Test date: Mar-2008 Hardware Avail:Apr-2008 Software Avail:Nov-2007

Notes/Tuning Information (Continued)

 Portablility flags:
  318.galgel_m    : -fixedform -col80

 Base and Peak User Environment (bash):
   export OMP_NUM_THREADS=16
   export OMP_DYNAMIC=FALSE
   export PSC_OMP_AFFINITY_MAP=15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0
   export PSC_OMP_STATIC_FAIR=TRUE
   export PSC_OMP_THREAD_SPIN=1000000000
   ulimit -s unlimited
 For flag descriptions, see file AMD-Apr2008-psc31_flags.txt
 Phoenix BIOS v.2.02.
 Default BIOS settings used, except ECC was set to "basic" instead of none.