Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

IBM Corporation

IBM System X 3550 (1.86 GHz Xeon E5320, 8MB L2 Cache)

SPECfp2000 = SPECfp_base2000 = -- 1801

SPEC license #: 11 Tested by: IBM Corporation Test date: Nov-2006 Hardware Avail: Dec-2006 Software Avail: Mar-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 64.7 2473

171.swim 3100 148 2097

172.mgrid 1800 154 1166

173.applu 2100 156 1346

177.mesa 1400 78.6 1782

178.galgel 2900 64.3 4508

179.art 2600 40.1 6480

183.equake 1300 59.0 2203

187.facerec 1900 107 1778

188.ammp 2200 164 1338

189.lucas 2000 131 1524

191.fma3d 2100 157 1335

200.sixtrack 1100 147 747

301.apsi 2600 232 1120

Hardware

CPU: Intel Xeon processor E5320 ( 1.86 GHz, 1066 MHz bus) CPU MHz: 1866 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip CPU(s) orderable: 1, 2 chips Parallel: No Primary Cache: 32KB(I) + 32KB(D) on chip (per core) Secondary Cache: 8MB(I+D) on chip, per chip (4MB shared per 2 cores) L3 Cache: N/A Other Cache: N/A Memory: 8 x 1024 MB ECC PC2-5300F Disk Subsystem: 73GB SAS 10K RPM Other Hardware:

Software

Operating System: Windows Server 2003 Enterprise Edition (32-bit) Compiler: Intel C++ and Fortran Compiler 9.1 for 32-bit applications

Build 20060323Z Microsoft Visual Studio 2005(for libraries) SmartHeap Library Version 8.0 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning for Fortran programs:  -fast -Qansi_alias +FDO
 Base tuning for C programs:  -fast    +FDO shlW32M.lib
 Portability:
 178.galgel:   -FI /F32000000