For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Hewlett-Packard Co.: HP Netserver LP 2000r

Chromium Communications Corp.: Chromium X15 WebServer 1.0

SPECweb99 = 2365

Test Date: Tester:

May-2001 Hewlett-Packard Company

Hardware Avail: Jun-2001 OS Avail: Dec-2000 HTTP Software Avail: Aug-2001 Sup. Software Avail: Aug-2001 SPEC license #: 3

Hardware

Vendor: Hewlett-Packard Co. Model: HP Netserver LP 2000r Processor: Intel Pentium III at 1Ghz # Processors: 2 cores, 2 chips, 1 core/chip Primary Cache: 16KBI+16KBD on chip Secondary Cache: 256KB on chip Other Cache: none Memory: 4 GB Disk Subsystem: 6 18GB 15K Ultra3 SCSI Disk Controllers: Integrated Ultra3 SCSI Other Hardware: 2 Alteon ACEswitch 180

Software

Operating System: RedHat 6.2 Linux File System: ext2 Other Software: None

HTTP Software

Vendor: Chromium Communications Corp. HTTP Software: Chromium X15 WebServer 1.0 API: TUX API Server Cache: None Log Mode: Apache Quick Format

Test Sponsor

Test Date: May-2001 Tested By: Hewlett-Packard Company SPEC License: 3

Network

# of Controllers: 2 Network Controllers: Alteon AceNIC 1000SX # of Nets: 2 Type of Nets: Gigabit Ethernet Network Speed: 1 Gb/s MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 14 Model: HP Kayak XU Processor: Intel Pentium II at 550MHz # of Processors: 2 Memory: 256MB Network Controller: Alteon AceNIC 1000SX Operating System: Microsoft Windows 2000 Pro Compiler: Microsoft C++ Version 6

Notes/Tuning Information

SUT Notes

1 disk for OS 1 disk for Logs 4 disk software RAID0 for Data

Operating System Notes

net/ipv4/ip_forward = 0 net/ipv4/conf/all/rp_filter = 1 net/ipv4/tcp_timestamps = 1 net/ipv4/tcp_sack = 0 net/ipv4/tcp_window_scaling = 0 net/ipv4/tcp_max_tw_buckets = 2000000 net/ipv4/ip_local_port_range = 16384 65536 net/core/rmem_max = 10485760 net/core/wmem_max = 10485760 net/core/rmem_default = 10485760 net/core/wmem_default = 10485760 fs/file-max = 100000 Gigabit Tuning: tx_coal_tick=300, rx_coal_tick=300

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

HTTP Software Notes

mmap_static module enabled MaxKeepAliveRequests 0 MaxClients 1050 Cache On SingleListen On

HTTP API Notes

Tux API from Compaq-20010122-DL320-API.tar.gz

Other Notes

One NIC IRQs bound to first processor One NIC and Timer IRQs bound to second processor