For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Hewlett-Packard Company: Alphaserver ES45 68/1250

Zeus Ltd: Zeus 4.1r1

SPECweb99 = 5094

Test Date: Tested By:

Jun-2002 Hewlett-Packard Company

Hardware Avail: Aug-2002 OS Avail: Nov-2002 HTTP Software Avail: May-2002 Sup. Software Avail: Oct-2002 SPEC license #: 2

Hardware

Vendor: Hewlett-Packard Company Model: Alphaserver ES45 68/1250 Processor: 1.25 GHz 21264C # Processors: 4 Primary Cache: 64KBI+64KBD on chip Secondary Cache: 16MB off chip Other Cache: none Memory: 32 GB Disk Subsystem: 13 x(BB00912301 9GB SCSI) Disk Controllers: 2 x QLOGIC ISP1040B/V2 FW SCSI Other Hardware:^{3 x ALTEON ACEswitch 180 GbE Switch}

Software

Operating System: Tru64 UNIX T5.1B File System: UFS & AdvFS Other Software: none

HTTP Software

Vendor: Zeus Ltd HTTP Software: Zeus 4.1r1 API: ISAPI Server Cache: none Log Mode: Binary Log Format

Test Sponsor

Test Date: Jun-2002 Tested By: Hewlett-Packard Company SPEC License: 2

Network

# of Controllers: 3 Network Controllers: 3 x DEGPA-SA # of Nets: 3 Type of Nets: Gigabit Ethernet Network Speed: 1 Gb/s MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 12 Model: HP DS20E Processor: 667MHz 21264 # of Processors: 2 Memory: 1GB Network Controller: DEGPA-SA Operating System: Tru64 UNIX V5.1 Compiler: Compaq C V6.3-026

Notes/Tuning Information

Operating System Notes

OS Tuning parameters:

vm: swapdevice=/dev/disk/dsk8c

vm_swap_eager = 0

proc:

max_per_proc_address_space = 0x40000000000 max_per_proc_data_size = 0x40000000000 max_proc_per_user = 2048 max_threads_per_user = 0 per_proc_address_space = 0x40000000000 per_proc_data_size = 0x40000000000

inet:

ipqmaxlen = 2000 ipqs = 16 tcbhashnum = 16 tcbhashsize = 1024

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

Operating System Notes (Continued)

tcp_dont_winscale = 1048576 tcp_recvspace = 1048576 tcp_sendspace = 1048576

net:

netisrthreads=2 netisrwakeupthreshold = 96

socket:

somaxconn = 32765 sominconn = 32765 umc = 1

vfs:

name_cache_hash_size = 16384 namei_cache_valid_time = 86400

advfs:

AdvfsSyncMmapPages = 0

alt:

send_ticks = 31250 recv_ticks = 200 send_coal = 500 recv_coal = 32

HTTP Software Notes

Zeus Tuning

global.cfg:

tuning!bind_any yes tuning!cache_files 237911 tuning!cache_flush_interval 86400 tuning!cache_large_file 1048576 tuning!cache_max_bytes 0 tuning!cache_small_file 0 tuning!cache_stat_expire 86400 tuning!num_children 4 tuning!so_wbuff_size 1048576 tuning!softservers no tuning!unique_bind no tuning!use_poll no

tuning!cache_cooling_time 0 tuning!cbuff_size 65536 tuning!keepalive yes tuning!keepalive_max -1 tuning!modules!isapi!writeclient_limit 524288000

runningsites/&lt;host&gt;:

bindaddr text 10.76.76.76,11.76.76.76,12,76.76.76 modules!fastcgi!enabled yes modules!map!alias!/fast-cgi/!filepath /www/fast-cgi modules!isapi!enabled yes modules!map!alias!/isapi/!filepath /www/isapi

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

Hardware Notes

Disk Configuration:

disk1: OS (/, /usr) [Controller 1] disk2: URLroot (/www) [1] disk3, disk9: http logging (log_dmn#log_fs) [1,2] disk4-7, disk10-13 wwwdomain#file_set rw,noatimes [1,2]

disk8: swap [1]

Network Notes

Network Tuning: N/A

Client Notes

max-proc-per-user = 0 proc:

maxusers = 1024 max-threads-per-user = 1024 socket:

sominconn = 32765 somaxconn = 32765 inet:

ipport_userreserved = 65000 tcp_recvspace = 1048576

Other Notes

Other Notes Tuning Disclosure: HP-20020805-Alpha-Tru64-5.1b.txt Dynamic API: Compaq-ES45-20011115.tar.gz Client code built: ./configure --enable-posix-threads i --enable-safe-gethostbyname ; make