Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Bull NovaScale 5080 (1500MHz)

SPECfp_rate2000 = SPECfp_rate_base2000 = 125 124 SPEC license #: 20 Tested by: JFL Test date: Jul-2003 Hardware Avail: Sep-2003 Software Avail: Sep-2003

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 200 400 600 800 168.wupwise 8 144 103 8 144 103

171.swim 8 283 102 8 283 102

172.mgrid 8 232 72.1 8 232 72.0

173.applu 8 105 185 8 105 185

177.mesa 8 126 103 8 126 103

178.galgel 8 72.7 370 8 72.7 370

179.art 8 38.0 635 8 38.0 635

183.equake 8 140 86.1 8 140 86.1

187.facerec 8 135 131 8 135 131

188.ammp 8 196 104 8 196 104

189.lucas 8 274 67.6 8 275 67.6

191.fma3d 8 269 72.4 8 269 72.4

200.sixtrack 8 77.1 132 8 77.1 132

301.apsi 8 297 81.2 8 272 88.7

Hardware

CPU: Itanium 2 processor 1500 MHz CPU MHz: 1500 FPU: Integrated CPU(s) enabled: 8 cores, 8 chips, 1 core/chip CPU(s) orderable: 4 to 8 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: 6MB (I+D) off chip Other Cache: N/A Memory: 32 GB (2 * 16 * 1GB DIMMs) Disk Subsystem: 1 SJ0812 Disk drawer with 2 15krpm 36GB SCSI disks Other Hardware:

Software

Operating System: Linux 64 bit : Red Hat Advanced Server 2.1 + Bull expansion Pack Compiler: Intel(R) Fortran Compiler for Linux 7.1 (Build 20030605) Intel(R) C++ Compiler for Linux 7.1 (Build 20030605) File System: ext2 System State: multi User

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use

 Baseline optimization flags:
   C programs:       -ipo -O3 +FDO -ansi_alias
   Fortran programs: -ipo -O3 +FDO

 Portability Flags:
   178.galgel:  -FI

 Peak optimization flags:
   168.wupwise: basepeak=yes
   171.swim: basepeak=yes
   172.mgrid: -O3 -ipo
   173.applu: basepeak=yes
   177.mesa: basepeak=yes
   178.galgel: basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Bull NovaScale 5080 (1500MHz)

SPECfp_rate2000 = SPECfp_rate_base2000 = 125 124 SPEC license #: 20 Tested by: JFL Test date: Jul-2003 Hardware Avail: Sep-2003 Software Avail: Sep-2003

Notes/Tuning Information (Continued)

   179.art: basepeak=yes
   183.equake: basepeak=yes
   187.facerec: basepeak=yes
   188.ammp: basepeak=yes
   189.lucas: -O3 -ipo
   191.fma3d: basepeak=yes
   200.sixtrack: basepeak=yes
   301.apsi: -O3 -ipo