Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECint^®_rate2006 = --

SPECint_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate_base2006 = 1.00

0 1.05

0.0500 0.150 0.200 0.250 0.300 0.350 0.400 0.450 0.500 0.550 0.600 0.650 0.700 0.750 0.800 0.850 0.900 0.950 1 1.00 1 1.00 1 0.999 1 0.980 1 1.02 1 0.992 1 1.03 1 1.00 1 1.01 1 1.03 1 1.00 1 1.00

Hardware

CPU Name: UltraSPARC II CPU Characteristics: CPU MHz: 296 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1-2 chips Primary Cache: 16 KB I + 16 KB D on chip per chip Secondary Cache: 2 MB I+D off chip per chip L3 Cache: None Other Cache: None Memory: 2 GB Disk Subsystem: 2x36GB 10K RPM SCSI (1 sys disk, 1 for SPEC) Other Hardware: None

Software

Operating System: Solaris 10 3/05 Compiler: Sun Studio 11 Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: Not Applicable Other Software: None

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECint_rate2006 = -- SPECint_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 1 9922 0.985 9734 1.00 9766 1.00 401.bzip2 1 9656 0.999 9644 1.00 9644 1.00 403.gcc 1 8059 0.999 8058 0.999 8023 1.00 429.mcf 1 9358 0.975 9306 0.980 9303 0.980 445.gobmk 1 10257 1.02 10283 1.02 10449 1.00 456.hmmer 1 9408 0.992 9409 0.992 9338 0.999 458.sjeng 1 11780 1.03 11787 1.03 12419 0.974 462.libquantum 1 20708 1.00 20702 1.00 20704 1.00 464.h264ref 1 22015 1.01 21925 1.01 22334 0.991 471.omnetpp 1 6012 1.04 6087 1.03 6166 1.01 473.astar 1 7032 0.998 7006 1.00 7017 1.00 483.xalancbmk 1 6818 1.01 6869 1.00 6904 0.999

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 Stack limit set to 131072

Platform Notes

 Although two CPUs were enabled during testing,
 the SPEC CPU2006 benchmarks used only 1 CPU.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Base Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC 403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECint_rate2006 = -- SPECint_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

Base Optimization Flags

C benchmarks:

-g -fast -xpagesize=4M

C++ benchmarks:

-g0 -library=stlport4 -fast -xpagesize=4M

Base Other Flags

C benchmarks:

-V

C++ benchmarks:

-verbose=version

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/sun-studio.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/sun-studio.xml

Originally published on 24 August 2006.

Report generated on Tue Jul 22 10:01:53 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v89.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance