Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECfp^®_rate2006 = -- SPECfp_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

Copies

SPECfp_rate_base2006 = 1.00

0 1.05

0.0500 0.150 0.200 0.250 0.300 0.350 0.400 0.450 0.500 0.550 0.600 0.650 0.700 0.750 0.800 0.850 0.900 0.950 1 1.00 1 0.983 1 0.998 1 1.00 1 1.00 1 1.01 1 1.00 1 0.999 1 1.03 1 0.998 1 1.03 1 0.997 1 1.00 1 1.01 1 1.00 1 1.01 1 1.01

Hardware

CPU Name: UltraSPARC II CPU Characteristics: CPU MHz: 296 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1-2 chips Primary Cache: 16 KB I + 16 KB D on chip per chip Secondary Cache: 2 MB I+D off chip per chip

Software

Operating System: Solaris 10 3/05 Compiler: Sun Studio 11 Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: Not Applicable Other Software: None

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECfp_rate2006 = -- SPECfp_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005 L3 Cache: None Other Cache: None Memory: 2 GB Disk Subsystem: 2x36GB 10K RPM SCSI (1 sys disk, 1 for SPEC) Other Hardware: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 1 13579 1.00 13595 1.00 13592 1.00 416.gamess 1 19914 0.983 19523 1.00 20036 0.977 433.milc 1 9189 0.999 9200 0.998 9198 0.998 434.zeusmp 1 9096 1.00 9086 1.00 9134 0.996 435.gromacs 1 7132 1.00 7154 0.998 7088 1.01 436.cactusADM 1 11787 1.01 11878 1.01 11809 1.01 437.leslie3d 1 9353 1.01 9358 1.00 9376 1.00 444.namd 1 8027 0.999 8026 0.999 8010 1.00 447.dealII 1 11180 1.02 11151 1.03 11150 1.03 450.soplex 1 8356 0.998 8355 0.998 8339 1.00 453.povray 1 5190 1.03 5197 1.02 5076 1.05 454.calculix 1 8264 0.998 8294 0.995 8275 0.997 459.GemsFDTD 1 10585 1.00 10581 1.00 10583 1.00 465.tonto 1 9689 1.02 9927 0.991 9725 1.01 470.lbm 1 13736 1.00 13718 1.00 13707 1.00 481.wrf 1 11160 1.00 11104 1.01 11084 1.01 482.sphinx3 1 19335 1.01 19321 1.01 19368 1.01

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 Stack limit set to 131072

Platform Notes

 Although two CPUs were enabled during testing,
 the SPEC CPU2006 benchmarks used only 1 CPU.

Base Compiler Invocation

C benchmarks:

cc

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECfp_rate2006 = --

SPECfp_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

Base Compiler Invocation (Continued)

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Base Optimization Flags

C benchmarks:

-g -fast -xpagesize=4M

C++ benchmarks:

-g0 -library=stlport4 -fast -xpagesize=4M

Fortran benchmarks:

-g -fast -xpagesize=4M

Benchmarks using both Fortran and C:

-g -fast(cc) -fast(f90) -xpagesize=4M

Base Other Flags

C benchmarks:

-V

C++ benchmarks:

-verbose=version

Fortran benchmarks:

-V

Benchmarks using both Fortran and C:

-V

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/sun-studio.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/sun-studio.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECfp_rate2006 = -- SPECfp_rate_base2006 = 1.00

CPU2006 license: 6 Test date: Mar-2006 Test sponsor: Sun Microsystems Hardware Availability: Apr-1997 Tested by: Sun Microsystems Software Availability: Oct-2005

Originally published on 24 August 2006.

Report generated on Tue Jul 22 10:00:06 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v90.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance