Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp^®_rate2006 = 62.3

SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

Copies

SPECfp_rate2006 = 62.3

SPECfp_rate_base2006 = 57.9

0 105

5.00 10.0 15.0 20.0 25.0 30.0 35.0 40.0 45.0 50.0 55.0 60.0 65.0 70.0 75.0 80.0 85.0 90.0 95.0 100 63 83.7

63 51.7

63 53.2

63 78.9

63 54.2

63 54.3

63 51.4

63 52.7

63 52.7

63 53.3

63 54.4

48 57.0

63 58.8

63 59.5

63 92.2

63 66.8

63 78.1

63 103

63 39.2

63 49.7

63 54.2

56 58.3

63 22.9

8 46.8

63 66.4

63 67.3

63 75.3

63 77.0

Hardware

CPU Name: UltraSPARC T2 CPU Characteristics: CPU MHz: 1417 FPU: Integrated CPU(s) enabled: 8 cores, 1 chip, 8 cores/chip, 8 threads/core CPU(s) orderable: 1 chip Primary Cache: 16 KB I + 8 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip

Software

Operating System: Solaris 10 8/07 (build s10s_u4wos_10) Compiler: Sun Studio 12 (build 2007/05/20) Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp_rate2006 = 62.3 SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007 L3 Cache: None Other Cache: None Memory: 64 GB (16 x 4 GB) Disk Subsystem: 275 GB Solaris Volume Manager RAID 0, interlace 384KB, on 5 x SUN72G 10K RPM SAS disks; ufs fragment size 8192 bytes Other Hardware: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 63 10163 84.2 10226 83.7 10228 83.7 63 10163 84.2 10226 83.7 10228 83.7 416.gamess 63 23870 51.7 23865 51.7 23868 51.7 63 23183 53.2 23195 53.2 23185 53.2 433.milc 63 7347 78.7 7320 79.0 7333 78.9 63 7347 78.7 7320 79.0 7333 78.9 434.zeusmp 63 10611 54.0 10570 54.2 10568 54.3 63 10544 54.4 10554 54.3 10584 54.2 435.gromacs 63 8746 51.4 8743 51.4 8706 51.7 63 8527 52.8 8542 52.7 8534 52.7 436.cactusADM 63 14284 52.7 14295 52.7 14349 52.5 63 14122 53.3 14129 53.3 14100 53.4 437.leslie3d 63 10876 54.4 10876 54.4 10859 54.5 48 7919 57.0 7935 56.9 7921 57.0 444.namd 63 8577 58.9 8618 58.6 8596 58.8 63 8488 59.5 8485 59.5 8512 59.4 447.dealII 63 7816 92.2 7831 92.0 7806 92.3 63 7816 92.2 7831 92.0 7806 92.3 450.soplex 63 7913 66.4 7864 66.8 7864 66.8 63 7913 66.4 7864 66.8 7864 66.8 453.povray 63 4233 79.2 4302 77.9 4291 78.1 63 3266 103 3250 103 3244 103 454.calculix 63 13251 39.2 13286 39.1 13241 39.3 63 13251 39.2 13286 39.1 13241 39.3 459.GemsFDTD 63 13439 49.7 13429 49.8 13443 49.7 63 13439 49.7 13429 49.8 13443 49.7 465.tonto 63 11437 54.2 11439 54.2 11242 55.1 56 9439 58.4 9477 58.1 9453 58.3 470.lbm 63 37983 22.8 37632 23.0 37763 22.9 8 2345 46.9 2347 46.8 2357 46.6 481.wrf 63 10601 66.4 10603 66.4 10608 66.3 63 10449 67.3 10488 67.1 10453 67.3 482.sphinx3 63 16315 75.3 16305 75.3 16387 74.9 63 15972 76.9 15953 77.0 15946 77.0

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

Processes were bound to cores using "submit" and "pbind".
ulimit -s 131072 was used to limit the space
consumed by the stack (and therefore make more
space available to the heap).
 /etc/system parameters
    autoup=600
       Causes pages older than the listed number of seconds to
       be written by fsflush.

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp_rate2006 = 62.3

SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007

Operating System Notes (Continued)

    tune_t_fsflushr=10
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush.

 The "webconsole" service was turned off using
     svcadm disable webconsole

Platform Notes

This result was measured on a Sun SPARC Enterprise
T5220.  All of these are electronically equivalent:
  - Sun SPARC Enterprise T5120
  - Sun SPARC Enterprise T5220
  - Fujitsu SPARC Enterprise T5120
  - Fujitsu SPARC Enterprise T5220

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Base Optimization Flags

C benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2 -xalias_level=std
-xprefetch_level=3 -xprefetch_auto_type=indirect_array_access

C++ benchmarks:

-g0 -library=stlport4 -fast -xipo=2 -xpagesize=4M -xprefetch_level=2
-xdepend -xalias_level=compatible

Fortran benchmarks:

-g -fast -xipo=2 -xpagesize=4M -xprefetch_level=2

Benchmarks using both Fortran and C:

-g -fast(cc) -fast(f90) -xipo=2 -xpagesize=4M -xprefetch_level=2
-xalias_level=std -xprefetch_level=3
-xprefetch_auto_type=indirect_array_access

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp_rate2006 = 62.3

SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007

Base Other Flags

C benchmarks:

-xjobs=16 -V

C++ benchmarks:

-xjobs=16 -verbose=diags,version

Fortran benchmarks:

-xjobs=16 -V

Benchmarks using both Fortran and C:

-xjobs=16 -V

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Peak Optimization Flags

C benchmarks:

433.milc: basepeak = yes

470.lbm: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xprefetch_level=3 -xipo=2 -xrestrict

482.sphinx3: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xinline= -xprefetch_level=2 -Wc,-Qlp-ol=1 -xrestrict
-xalias_level=strong -fsimple=1 -xlinkopt=2 -lfast

C++ benchmarks:

444.namd: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xdepend -xalias_level=compatible -xprefetch_level=1
-xlinkopt=2

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp_rate2006 = 62.3 SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007

Peak Optimization Flags (Continued)

447.dealII: basepeak = yes

450.soplex: basepeak = yes

453.povray: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xdepend -xalias_level=compatible -xipo=2 -xrestrict
-xlinkopt=2

Fortran benchmarks:

410.bwaves: basepeak = yes

416.gamess: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xpagesize=4M
-xlinkopt=2

434.zeusmp: -g -fast -xpagesize=4M -xipo=1 -qoption cg -Qeps:enabled=1

-qoption cg -Qeps:ws=8 -lmopt

437.leslie3d: -g -fast -xpagesize_heap=4M -xpagesize_stack=64K

-xprefetch_level=3 -xprefetch=latx:1.6 -qoption cg -Qlp=1
-qoption cg -Qlp-fa=0 -qoption cg -Qlp-fl=1
-qoption cg -Qlp-av=448 -qoption cg -Qlp-t=4

459.GemsFDTD: basepeak = yes

465.tonto: -g -fast -xpagesize=4M -xipo=2 -lfast

Benchmarks using both Fortran and C:

435.gromacs: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -xipo=1 -xinline= -xarch=generic
-xchip=generic -fsimple=0

436.cactusADM: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -xipo=2 -fsimple=1 -xlinkopt=2

454.calculix: basepeak = yes

481.wrf: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast(cc) -fast(f90)
-xpagesize=4M -xlinkopt=2

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Limited Fujitsu SPARC Enterprise T5220

SPECfp_rate2006 = 62.3 SPECfp_rate_base2006 = 57.9

CPU2006 license: 19 Test date: Jul-2007 Test sponsor: Fujitsu Limited Hardware Availability: Oct-2007 Tested by: Sun Microsystems Software Availability: Sep-2007

Peak Other Flags

C benchmarks:

-xjobs=16 -V

C++ benchmarks:

-xjobs=16 -verbose=diags,version

Fortran benchmarks:

-xjobs=16 -V

Benchmarks using both Fortran and C:

-xjobs=16 -V

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12.20090714.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12.20090714.xml

Originally published on 1 November 2007.

Report generated on Tue Jul 22 14:08:42 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance