Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T3400 (Intel E8500, 3.16 GHz)

SPECint^®_rate2006 = 40.9

SPECint_rate_base2006 = 38.3

CPU2006 license: 55 Test date: Apr-2008 Test sponsor: Dell Inc. Hardware Availability: Jan-2008 Tested by: Dell Inc. Software Availability: Mar-2008

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 40.9

SPECint_rate_base2006 = 38.3

0 70.0

3.00 6.00 9.00 12.0 15.0 18.0 21.0 24.0 27.0 30.0 33.0 36.0 39.0 42.0 45.0 48.0 51.0 54.0 57.0 60.0 63.0 66.0 2 39.4

2 44.5

2 32.4

2 33.6

2 35.9

2 37.1

2 43.7

2 42.7

2 42.0

2 45.6

2 33.1

2 35.9

2 37.2

2 41.9

2 45.0

1 50.7

2 66.2

2 69.2

2 27.4

2 29.0

2 27.6

2 30.3

2 42.5

2 43.8

Hardware

CPU Name: Intel Core 2 Duo E8500 CPU Characteristics: 1333 MHz Bus Speed CPU MHz: 3166 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1 chip Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 6 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 8 GB (4x2 GB 800 MHz ECC CL6 DDR2) Disk Subsystem: 1 x 160 GB SATA 7200 RPM Other Hardware: None

Software

Operating System: Windows Vista Ultimate (64-bit) Compiler: Intel C++ Compiler for IA-32, Version 10.1

Build 20080312 Package ID: w_cc_p_10.1.021 Microsoft Visual Studio 2005 SP1

Auto Parallel: Yes File System: NTFS System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: MicroQuill SmartHeap Library 8.1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T3400 (Intel E8500, 3.16 GHz)

SPECint_rate2006 = 40.9 SPECint_rate_base2006 = 38.3

CPU2006 license: 55 Test date: Apr-2008 Test sponsor: Dell Inc. Hardware Availability: Jan-2008 Tested by: Dell Inc. Software Availability: Mar-2008

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 2 496 39.4 499 39.2 494 39.6 2 439 44.5 439 44.5 439 44.6 401.bzip2 2 596 32.4 613 31.5 595 32.4 2 575 33.6 591 32.7 573 33.7 403.gcc 2 445 36.2 449 35.9 454 35.5 2 432 37.3 433 37.1 440 36.6 429.mcf 2 416 43.8 417 43.7 417 43.7 2 427 42.7 428 42.6 427 42.8 445.gobmk 2 499 42.0 499 42.0 500 41.9 2 460 45.6 460 45.6 459 45.7 456.hmmer 2 563 33.1 563 33.1 563 33.1 2 520 35.9 519 35.9 519 35.9 458.sjeng 2 651 37.2 651 37.1 651 37.2 2 578 41.9 578 41.9 578 41.9 462.libquantum 2 909 45.6 922 45.0 922 44.9 1 409 50.7 410 50.6 408 50.8 464.h264ref 2 669 66.2 670 66.1 668 66.2 2 640 69.2 641 69.1 640 69.2 471.omnetpp 2 455 27.5 455 27.4 456 27.4 2 431 29.0 430 29.0 430 29.1 473.astar 2 508 27.6 508 27.6 508 27.6 2 464 30.2 464 30.3 464 30.3 483.xalancbmk 2 325 42.5 324 42.6 325 42.5 2 315 43.8 315 43.8 315 43.8

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Base Compiler Invocation

C benchmarks:

icl -Qstd=c99

C++ benchmarks:

icl

Base Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32 483.xalancbmk: -Qoption,cpp,--no_wchar_t_keyword

Base Optimization Flags

C benchmarks:

-fast -Qvec-guard-write /F512000000

C++ benchmarks:

-fast -Qcxx_features /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T3400 (Intel E8500, 3.16 GHz)

SPECint_rate2006 = 40.9 SPECint_rate_base2006 = 38.3

CPU2006 license: 55 Test date: Apr-2008 Test sponsor: Dell Inc. Hardware Availability: Jan-2008 Tested by: Dell Inc. Software Availability: Mar-2008

Base Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

Peak Compiler Invocation

C benchmarks:

icl -Qstd=c99

C++ benchmarks:

icl

Peak Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32 483.xalancbmk: -Qoption,cpp,--no_wchar_t_keyword

Peak Optimization Flags

C benchmarks:

400.perlbench: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias

-Qprefetch /F512000000

401.bzip2: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qprefetch

/F512000000

403.gcc: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast /F512000000

429.mcf: Same as 401.bzip2

445.gobmk: -Qprof_gen(pass 1) -Qprof_use(pass 2) -QxT -O2 -Qipo

-Qprec-div- -Qansi-alias /F512000000

456.hmmer: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll2

-Qansi-alias -Qopt-multi-version-aggressive /F512000000

458.sjeng: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll4

/F512000000

462.libquantum: -fast -Qunroll4 -Ob0 -Qprefetch

-Qopt-streaming-stores:always -Qparallel
-Qpar-runtime-control /F512000000 shlw32mt.lib

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T3400 (Intel E8500, 3.16 GHz)

SPECint_rate2006 = 40.9 SPECint_rate_base2006 = 38.3

CPU2006 license: 55 Test date: Apr-2008 Test sponsor: Dell Inc. Hardware Availability: Jan-2008 Tested by: Dell Inc. Software Availability: Mar-2008

Peak Optimization Flags (Continued)

464.h264ref: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qunroll2

-Qansi-alias /F512000000

C++ benchmarks:

471.omnetpp: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias

-Qopt-ra-region-strategy=block -Qcxx_features /F512000000
shlw32m.lib            -link /FORCE:MULTIPLE

473.astar: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias

-Qopt-ra-region-strategy=routine -Qcxx_features /F512000000
shlw32m.lib            -link /FORCE:MULTIPLE

483.xalancbmk: -Qprof_gen(pass 1) -Qprof_use(pass 2) -fast -Qansi-alias

-Qcxx_features /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

Peak Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/dell.ic10.1.windows.flags.20090714.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/dell.ic10.1.windows.flags.20090714.xml

Originally published on 13 May 2008.

Report generated on Tue Jul 22 17:09:08 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance