Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T7500 (Intel Xeon X5570, 2.93 GHz)

SPECint^®_rate2006 = 239

SPECint_rate_base2006 = 225

CPU2006 license: 55 Test date: Mar-2009 Test sponsor: Dell Inc. Hardware Availability: Apr-2009 Tested by: Dell Inc. Software Availability: Feb-2009

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 239

SPECint_rate_base2006 = 225

0 760

30.0 60.0 90.0 120 150 180 210 240 270 300 330 360 390 420 450 480 510 540 570 600 630 660 690 720 16 195 16 253

16 147 16 147

16 189 16 190

16 270 16 267

16 234 16 261

16 173 16 173

16 218 16 235

16 755

16 309 16 323

16 173 16 195

16 150 16 168

16 216

Hardware

CPU Name: Intel Xeon X5570 CPU Characteristics: Intel Turbo Boost Technology up to 3.33 GHz CPU MHz: 2933 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip, 2 threads/core CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 256 KB I+D on chip per core L3 Cache: 8 MB I+D on chip per chip Other Cache: None Memory: 24 GB (6x4 GB DDR3-1333R, ECC, CL9) Disk Subsystem: 1 x 146 GB SAS 15000 RPM Other Hardware: None

Software

Operating System: Windows Vista Business SP1 (64-bit) Compiler: Intel C++ Compiler for IA-32, Version 11.0

Build 20090131 Package ID: w_cproc_p_11.0.072 Microsoft Visual Studio 2008 SP1

Auto Parallel: No File System: NTFS System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: MicroQuill SmartHeap Library 8.1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T7500 (Intel Xeon X5570, 2.93 GHz)

SPECint_rate2006 = 239 SPECint_rate_base2006 = 225

CPU2006 license: 55 Test date: Mar-2009 Test sponsor: Dell Inc. Hardware Availability: Apr-2009 Tested by: Dell Inc. Software Availability: Feb-2009

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 16 785 198 805 194 801 195 16 621 251 616 254 618 253 401.bzip2 16 1048 147 1009 154 1060 146 16 1052 147 1028 150 1064 146 403.gcc 16 675 190 690 187 684 189 16 676 190 673 192 680 189 429.mcf 16 544 269 540 270 539 270 16 541 270 545 267 545 267 445.gobmk 16 712 235 719 234 721 232 16 645 261 645 261 646 261 456.hmmer 16 866 173 866 173 868 171 16 856 174 864 173 863 173 458.sjeng 16 884 219 893 216 891 218 16 822 235 822 235 820 237 462.libquantum 16 438 757 439 755 442 750 16 438 757 439 755 442 750 464.h264ref 16 1141 310 1149 309 1152 307 16 1093 323 1091 325 1097 323 471.omnetpp 16 580 173 581 173 580 173 16 514 195 514 195 513 195 473.astar 16 750 150 749 150 747 150 16 666 168 669 168 666 168 483.xalancbmk 16 509 216 510 216 505 219 16 509 216 510 216 505 219

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

The config file option ’submit’ was used.

Platform Notes

 BIOS Settings
   Memory Node Interleaving set to NUMA.
   Hyper-Threading Technology set to ON.

General Notes

 Binaries were built on Windows Vista Business (64-bit)

Base Compiler Invocation

C benchmarks:

icl -Qvc9 -Qstd=c99

C++ benchmarks:

icl -Qvc9

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T7500 (Intel Xeon X5570, 2.93 GHz)

SPECint_rate2006 = 239

SPECint_rate_base2006 = 225

CPU2006 license: 55 Test date: Mar-2009 Test sponsor: Dell Inc. Hardware Availability: Apr-2009 Tested by: Dell Inc. Software Availability: Feb-2009

Base Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32 483.xalancbmk: -Qoption,cpp,--no_wchar_t_keyword

Base Optimization Flags

C benchmarks:

-QxSSE4.2 -Qipo -O3 -Qprec-div- -Qopt-prefetch /F512000000

C++ benchmarks:

-QxSSE4.2 -Qipo -O3 -Qprec-div- -Qopt-prefetch -Qcxx_features
/F512000000 shlw32m.lib            -link /FORCE:MULTIPLE

Base Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

Peak Compiler Invocation

C benchmarks:

icl -Qvc9 -Qstd=c99

C++ benchmarks:

icl -Qvc9

Peak Portability Flags

403.gcc: -DSPEC_CPU_WIN32 464.h264ref: -DSPEC_CPU_NO_INTTYPES -DWIN32 483.xalancbmk: -Qoption,cpp,--no_wchar_t_keyword

Peak Optimization Flags

C benchmarks:

400.perlbench: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qansi-alias -Qopt-prefetch
/F512000000 shlw32m.lib            -link /FORCE:MULTIPLE

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T7500 (Intel Xeon X5570, 2.93 GHz)

SPECint_rate2006 = 239 SPECint_rate_base2006 = 225

CPU2006 license: 55 Test date: Mar-2009 Test sponsor: Dell Inc. Hardware Availability: Apr-2009 Tested by: Dell Inc. Software Availability: Feb-2009

Peak Optimization Flags (Continued)

401.bzip2: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qansi-alias -Qopt-prefetch
/F512000000

403.gcc: -Qprof_gen(pass 1) -QxSSE4.2 -Qprof_use(pass 2) -Qipo -O3

-Qprec-div- -Qopt-prefetch /F512000000

429.mcf: -QxSSE4.2 -Qipo -O3 -Qprec-div- -Qopt-prefetch

/F512000000

445.gobmk: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O2 -Qprec-div- -Qansi-alias /F512000000

456.hmmer: -QxSSE4.2 -Qipo -O3 -Qprec-div- -Qunroll2 -Qansi-alias

/F512000000

458.sjeng: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qunroll4 /F512000000

462.libquantum: basepeak = yes

464.h264ref: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qunroll2 -Qansi-alias /F512000000

C++ benchmarks:

471.omnetpp: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qansi-alias
-Qopt-ra-region-strategy=block /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

473.astar: -Qprof_gen(pass 1) -QxSSE4.2(pass 2) -Qprof_use(pass 2)

-Qipo -O3 -Qprec-div- -Qansi-alias
-Qopt-ra-region-strategy=routine /F512000000 shlw32m.lib
           -link /FORCE:MULTIPLE

483.xalancbmk: basepeak = yes

Peak Other Flags

C benchmarks:

403.gcc: -Dalloca=_alloca

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/dell.ic11.0.windows.flags.20090710.html

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Dell Inc.

Dell Precision T7500 (Intel Xeon X5570, 2.93 GHz)

SPECint_rate2006 = 239 SPECint_rate_base2006 = 225

CPU2006 license: 55 Test date: Mar-2009 Test sponsor: Dell Inc. Hardware Availability: Apr-2009 Tested by: Dell Inc. Software Availability: Feb-2009

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/dell.ic11.0.windows.flags.20090710.xml

Originally published on 2 April 2009.

Report generated on Tue Jul 22 23:58:33 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance