Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems

Sun Blade X6270 (Sun Studio no autopar, base only)

SPECfp^®2006 = Not Run SPECfp_base2006 = 29.1

CPU2006 license: 6 Test date: May-2009 Test sponsor: Sun Microsystems Hardware Availability: Apr-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

410.bwaves

416.gamess

433.milc

434.zeusmp

435.gromacs

436.cactusADM

437.leslie3d

444.namd

447.dealII

450.soplex

453.povray

454.calculix

459.GemsFDTD

465.tonto

470.lbm

481.wrf

482.sphinx3

SPECfp_base2006 = 29.1

0 45.0

2.00 4.00 6.00 8.00 10.0 12.0 14.0 16.0 18.0 20.0 22.0 24.0 26.0 28.0 30.0 32.0 34.0 36.0 38.0 40.0 42.0 43.5

21.2

24.0

31.0

19.9

29.1

31.1

17.0

31.3

31.1

26.5

23.6

33.9

25.8

44.6

37.8

41.5

Hardware

CPU Name: Intel Xeon X5570 CPU Characteristics: Intel Turbo Boost Technology up to 3.33 GHz CPU MHz: 2933 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip, 2 threads/core CPU(s) orderable: 1 or 2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 256 KB I+D on chip per core

Software

Operating System: OpenSolaris 2008.11 Compiler: Sun Studio 12 Update 1 (internal build 43) Auto Parallel: No File System: zfs with gzip compression System State: Default Base Pointers: 64-bit Peak Pointers: Not Applicable

Continued on next page Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems

Sun Blade X6270 (Sun Studio no autopar, base only)

SPECfp2006 = Not Run SPECfp_base2006 = 29.1

CPU2006 license: 6 Test date: May-2009 Test sponsor: Sun Microsystems Hardware Availability: Apr-2009 Tested by: Sun Microsystems Software Availability: Jun-2009 L3 Cache: 8 MB I+D on chip per chip Other Cache: None Memory: 24 GB (6 x 4 GB DDR3-1333) Disk Subsystem: 1 x 146 GB Sun 10,000 RPM SAS Other Hardware: None

Other Software: none

Results Table

Benchmark Seconds Ratio Seconds Ratio Seconds Ratio

Base Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 312 43.5 312 43.6 313 43.4 416.gamess 922 21.2 923 21.2 923 21.2 433.milc 383 24.0 383 24.0 383 24.0 434.zeusmp 293 31.1 293 31.0 293 31.0 435.gromacs 359 19.9 359 19.9 359 19.9 436.cactusADM 411 29.1 410 29.1 409 29.2 437.leslie3d 301 31.2 302 31.1 302 31.1 444.namd 471 17.0 471 17.0 471 17.0 447.dealII 366 31.3 366 31.3 366 31.3 450.soplex 268 31.1 267 31.2 268 31.1 453.povray 201 26.5 201 26.5 200 26.5 454.calculix 350 23.6 350 23.6 350 23.6 459.GemsFDTD 313 33.9 313 33.9 313 33.9 465.tonto 382 25.8 382 25.8 382 25.8 470.lbm 308 44.6 308 44.6 308 44.6 481.wrf 296 37.8 295 37.8 295 37.8 482.sphinx3 470 41.4 470 41.5 470 41.5

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

 The config file option ’submit’ was used, along with ’pbind’, to
 run each benchmark on a specific core.

Operating System Notes

 ulimit -s 131072  (shell): increases stack
 For more information on shell/tuning paramaters, please
 see the "Platform settings" section of the flags file.
 /etc/system parameters
    tune_t_fsflushr=10
    autoup=900
    set lpg_alloc_prefer=1
    set zfs:zfs_arc_max = 0x10000000

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems

Sun Blade X6270 (Sun Studio no autopar, base only)

SPECfp2006 = Not Run

SPECfp_base2006 = 29.1

CPU2006 license: 6 Test date: May-2009 Test sponsor: Sun Microsystems Hardware Availability: Apr-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Platform Notes

 AMIBIOS Build Date 1/26/09 ID 07.01.36.00
   Default BIOS settings used except:
   Intel VT-d: Disabled.  VT-d, if enabled, supports
   remapping of I/O DMA transfers for virtualization.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Fortran benchmarks:

f90

Benchmarks using both Fortran and C:

cc f90

Base Portability Flags

410.bwaves: -DSPEC_CPU_LP64 416.gamess: -DSPEC_CPU_LP64

433.milc: -DSPEC_CPU_LP64 434.zeusmp: -DSPEC_CPU_LP64 435.gromacs: -DSPEC_CPU_LP64 436.cactusADM: -DSPEC_CPU_LP64

437.leslie3d: -DSPEC_CPU_LP64

444.namd: -DSPEC_CPU_LP64 447.dealII: -DSPEC_CPU_LP64 450.soplex: -DSPEC_CPU_LP64 453.povray: -DSPEC_CPU_LP64 454.calculix: -DSPEC_CPU_LP64 459.GemsFDTD: -DSPEC_CPU_LP64

465.tonto: -DSPEC_CPU_LP64 470.lbm: -DSPEC_CPU_LP64 481.wrf: -DSPEC_CPU_LP64 -DSPEC_CPU_WORDS_LITTLEENDIAN 482.sphinx3: -DSPEC_CPU_LP64

Base Optimization Flags

C benchmarks:

-fast -xipo=2 -m64 -xvector=simd -xpagesize=2M

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems

Sun Blade X6270 (Sun Studio no autopar, base only)

SPECfp2006 = Not Run SPECfp_base2006 = 29.1

CPU2006 license: 6 Test date: May-2009 Test sponsor: Sun Microsystems Hardware Availability: Apr-2009 Tested by: Sun Microsystems Software Availability: Jun-2009

Base Optimization Flags (Continued)

C++ benchmarks:

-fast -xipo=2 -m64 -xvector=simd -xpagesize=2M -library=stlport4

Fortran benchmarks:

-fast -xipo=2 -m64 -xvector=simd -xpagesize=2M

Benchmarks using both Fortran and C:

-fast(cc) -xipo=2 -m64 -xvector=simd -xpagesize=2M -fast(f90)

Base Other Flags

C benchmarks:

-V -# -xjobs=16

C++ benchmarks:

-verbose=diags,version -xjobs=16

Fortran benchmarks:

-V -v -xjobs=16

Benchmarks using both Fortran and C:

-V -# -xjobs=16 -v

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-OpenSolaris-Studio-x86_64.20090710.01.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-OpenSolaris-Studio-x86_64.20090710.01.xml

Originally published on 23 June 2009.

Report generated on Wed Jul 23 01:34:36 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance