Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2001, Standard Performance Evaluation Corporation SGI SGI Origin 3800 64X 500MHz R14k

SPECompMpeak2001 = SPECompMbase2001 =

17826 15758

SPEC license #:HPG0014 Tested by: SGI Test site: Test date: Jun-2001 Hardware Avail:Jun-2001 Software Avail:Mar-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 20000 40000 60000

310.wupwise_m 6000 218 27572 211 28475

312.swim_m 6000 258 23268 252 23843

314.mgrid_m 7300 281 25964 280 26046

316.applu_m 4000 184 21730 131 30440

318.galgel_m 5100 661 7712 553 9222

320.equake_m 2600 275 9461 179 14512

324.apsi_m 3400 216 15720 156 21821

326.gafort_m 8700 601 14465 590 14750

328.fma3d_m 4600 339 13560 343 13425

330.art_m 6400 343 18667 346 18471

332.ammp_m 7000 715 9789 697 10045

Hardware

CPU: R14000 CPU MHz: 500 FPU: Integrated CPU(s) enabled: 64 CPU(s) orderable: 2-512 Primary Cache: 32KBI + 32KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: N/A Other Cache: N/A Memory: 64 GB Disk Subsystem: 1 x 18 GB FC, 4x 36 GB (striped) FC Other Hardware: None

Software

OpenMP Threads: 64 Parallel: -- Operating System: IRIX 6.5.12m Compiler: MIPSpro 7.3.1.2m C, Fortran90 File System: xfs System State: Multi-user

Notes/Tuning Information

Baseline flags: -64 -mp -Ofast=ip35 -LNO:fusion=2
Portability Flags:
   318.galgel_m: -fixedform -extend_source

Peak flags:
310.wupwise_m: -64 -mp -Ofast=ip27 -LNO:fusion=2:prefetch_ahead=5 -INLINE:aggressive=on
.            -IPA:space=1000:linear=on:plimit=10000:callee_limit=5000 -OPT:Olimit=0
312.swim_m: -64 -mp -Ofast=ip35 -LNO:fusion=2
314.mgrid_m: -64 -mp -Ofast=ip35 -LNO:fusion=2
316.applu_m: -64 -mp -Ofast=ip35 -LNO:ou_max=5:ou_prod_max=10:prefetch=0:fusion=2
.            -CG:ld_latency=3
318.galgel_m: -64 -mp -Ofast=ip35 -LNO:fusion=2
320.equake_m: -64 -mp -Ofast=ip35 -OPT:goto=off:unroll_size=160:unroll_times_max=4
.             -CG:ld_latency=3
324.apsi_m: -64 -mp -Ofast=ip35 -LNO:fusion=2 -TENV:X=4 -LNO:prefetch=0:blocking=off
326.gafort_m: -64 -mp -Ofast=ip35
328.fma3d_m: -64 -mp -Ofast=ip35 -LNO:fusion=2 -CG:ld_latency=3
.            -IPA:linear=on:use_intrinsic
330.art_m: -64 -mp -Ofast=ip35 -LNO:fusion=2
332.ammp_m: -64 -mp -Ofast=ip35 -LNO:fusion=2:prefetch=0

Baseline user environment:
   limit stacksize 512m

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2001, Standard Performance Evaluation Corporation SGI SGI Origin 3800 64X 500MHz R14k

SPECompMpeak2001 = SPECompMbase2001 =

17826 15758

SPEC license #:HPG0014 Tested by: SGI Test site: Test date: Jun-2001 Hardware Avail:Jun-2001 Software Avail:Mar-2001

Notes/Tuning Information (Continued)

   OMP_NUM_THREADS=64
   OMP_DYNAMIC=FALSE
   MPC_GANG=OFF
   _DSM_MUSTRUN=
   _DSM_WAIT=SPIN

Peak user environment:
316.applu_m: PAGESIZE_DATA=4096, PAGESIZE_STACK=4096, _DSM_PLACEMENT=ROUND_ROBIN
318.galgel_m: _DSM_PLACEMENT=ROUND_ROBIN, OMP_NUM_THREADS=40
320.equake_m: OMP_NUM_THREADS=48
324.apsi_m: PAGESIZE_DATA=4096, PAGESIZE_STACK=4096
332.ammp_m: PAGESIZE_DATA=1024, PAGESIZE_STACK=1024, _DSM_PLACEMENT=ROUND_ROBIN

The following O/S parameters were set via systune:
   percent_totalmem_4m_pages = 25 ; percent_totalmem_1m_pages = 25
   percent_totalmem_256k_pages = 10 ; percent_totalmem_64k_pages = 10