Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2001, Standard Performance Evaluation Corporation

Compaq Computer Corporation AlphaServer GS320 Model 32 64/731

SPECompMpeak2001 = SPECompMbase2001 = -- 5073

SPEC license #:HPG0009 Tested by: Compaq Computer Corp. Test site: Test date: June-2001 Hardware Avail:May-2000 Software Avail:Aug-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 5000 10000 15000

310.wupwise_m 6000 743 8076

312.swim_m 6000 585 10261

314.mgrid_m 7300 807 9041

316.applu_m 4000 661 6052

318.galgel_m 5100 1196 4265

320.equake_m 2600 692 3756

324.apsi_m 3400 686 4958

326.gafort_m 8700 1950 4461

328.fma3d_m 4600 995 4622

330.art_m 6400 1979 3234

332.ammp_m 7000 2936 2384

Hardware

CPU: Alpha 21264A CPU MHz: 731 FPU: Integrated CPU(s) enabled: 16 CPU(s) orderable: 1 to 32 Primary Cache: 64KB(I)+64KB(D) on chip Secondary Cache: 4MB off chip per CPU L3 Cache: None Other Cache: None Memory: 96GB Disk Subsystem: 1x18GB Other Hardware: None

Software

OpenMP Threads: 16 Parallel: -- Operating System: Tru64 UNIX V5.1 +Patch Kit 2 Compiler: Fortran V5.4 1686 - 46B5P C V6.4 -112 - 46B45 File System: ufs System State: Multi-user

Notes/Tuning Information

 If you run out of virtual memory, please see the
 the comments in the config file about setting
 limits in /etc/sysconfigtab.

 User environment:
       OMP_NUM_THREADS=16
 Base:
       All use   -v  -arch ev67
       F90  -fast -omp -O5
       cc   -fast -omp -O4
 Portability: 318.galgel_m: -extend_source

 Information on UNIX V5.1 Patches can be found at
 http://ftp1.service.digital.com/public/unix/v5.1/