Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Unisys Corporation ES7000/420

SPECompMpeak2001 = SPECompMbase2001 =

12207 11806

SPEC license #:HPG0016 Tested by: Unisys Corporation Test site: Salt Lake City Test date: Nov-2003 Hardware Avail:Jul-2003 Software Avail:Oct-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 10000 20000 30000

310.wupwise_m 6000 471 12728 471 12747

312.swim_m 6000 308 19488 308 19480

314.mgrid_m 7300 330 22100 333 21892

316.applu_m 4000 376 10640 354 11304

318.galgel_m 5100 411 12415 406 12577

320.equake_m 2600 192 13509 193 13470

324.apsi_m 3400 365 9319 328 10358

326.gafort_m 8700 1070 8132 1068 8148

328.fma3d_m 4600 665 6920 595 7733

330.art_m 6400 384 16682 384 16661

332.ammp_m 7000 964 7259 884 7922

Hardware

CPU: Itanium 2 processor CPU MHz: 1500 FPU: Integrated CPU(s) enabled: 8 CPU(s) orderable: 4,8,12,16 Primary Cache: 16KBI+16KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: 6MB(I+D) on chip Other Cache: None Memory: 64GB (blocked) Disk Subsystem: 2x36GB SCSI disk (mirrored) (15k rpm) Other Hardware:

Software

OpenMP Threads: 8 Parallel: OpenMP Operating System: SuSE LINUX Enterprise Server 8 for Intel Itanium Processor Family SP3 Compiler: Intel C/C++ Compiler 7.1 for Linux build 20030924

Intel Fortran Compiler 7.1 for Linux build 20030924

File System: ReiserFS/xfs System State: Runlevel 3 (multiuser+network)

Notes/Tuning Information

 Base tuning:
 C programs:       -O3 -ipo -openmp -ansi_alias
 Fortran programs: -O3 -ipo -openmp -stack_temps

 Peak tuning:
 default: -ipo -O3 -openmp -stack_temps
 310.wupwise_m: default
 312.swim_m: default
 314.mgrid_m: default
 316.applu_m: -ipo -openmp
 318.galgel_m: default
 320.equake_m: -ipo -O3 -openmp -ansi_alias
 324.apsi_m: -O3 -openmp -stack_temps
 326.gafort_m: default
 326.fma3d_m: -O3 -openmp -stack_temps -static
 330.art_m: -ipo -O3 -openmp -ansi_alias
 332.ammp_m: -openmp -ansi_alias

 Portability:
 318.galgel_m: -FI -132

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Unisys Corporation ES7000/420

SPECompMpeak2001 = SPECompMbase2001 =

12207 11806

SPEC license #:HPG0016 Tested by: Unisys Corporation Test site: Salt Lake City Test date: Nov-2003 Hardware Avail:Jul-2003 Software Avail:Oct-2003

Notes/Tuning Information (Continued)

 User environment:
 OMP_NUM_THREADS=8
 ulimit -s 2000000
 KMP_STACKSIZE=250000000
 KMP_LIBRARY=TURNAROUND

 Alternate sources for peak:
 SPEC OMPL2001 (srcalt=ompl) 64-bit source modified for OMPM2001.
 Used for 320.equake_m, 324.apsi_m, 328.fma3d_m.

 Notes:
 SP3 to kernel 2.4.21
 System was configured with 4 Procesor Modules with 2 processors per Processor Module
 ReiserFS is the root partition and xfs partition is for the benchmark.