Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright 1999-2008, Standard Performance Evaluation Corporation

Sun Microsystems

Sun Fire X2270 (Intel Xeon X5570 2.93GHz)

SPECompLpeak2001 =

SPECompLbase2001 =

254318

237781

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Menlo Park Test date: Mar-2009 Hardware Avail:Apr-2009 Software Avail:Jun-2009

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 1000000 2000000

311.wupwise_l 9200 504 292217 504 292216

313.swim_l 12500 1376 145331 1311 152583

315.mgrid_l 13500 887 243413 804 268546

317.applu_l 13500 1703 126851 1703 126851

321.equake_l 13000 1123 185219 930 223712

325.apsi_l 10500 662 253927 656 256181

327.gafort_l 11000 740 237879 737 238754

329.fma3d_l 23500 1783 210836 1784 210708

331.art_l 25000 509 785590 394 1016266

Hardware

CPU: Intel Xeon X5570 CPU MHz: 2933 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip, 2 threads/core CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 256 KB I+D on chip per core L3 Cache: 8 MB I+D on chip per chip Other Cache: None Memory: 24 GB (6 x 4 GB DDR3-1333) Disk Subsystem: 1 x 1 TB, SATA, 7200 RPM Other Hardware: None

Software

OpenMP Threads: 16 Parallel: OpenMP and Automatic parallel Operating System: OpenSolaris 2008.11 Compiler: Sun Studio 12 Update 1 (backend build 20090309) File System: zfs System State: Multi-User

Notes/Tuning Information

 Compiler Invocation:
   C   : cc
   F90 : f90
   F77 : f90

 Base tuning:
   Fortran :  -fast  -xtarget=nehalem -xarch=generic  -xpagesize=2M
              -xmodel=medium -xopenmp -xautopar -xipo=2 -xvector=lib
              -xprefetch -xprefetch_level=3 -m64 -lmtmalloc
   C       :  -fast -m64 -xmodel=medium -fns=no -xalias_level=layout
              -xdepend=no -xopenmp -lmvec
   ONESTEP=yes

 Peak tuning:
  ONESTEP=yes for all peak tests.

  311.wupwise_l   : -fast -xtarget=nehalem -xarch=generic -xpagesize=2M
                    -xmodel=medium -xopenmp -xautopar -xipo=2 -xvector=lib
                    -xprefetch -xprefetch_level=3 -m64 -lmtmalloc
  313.swim_l      : -fast -xpagesize=2M -xmodel=medium -xopenmp
                    -xautopar -xipo=2 -xvector=lib
                    -xprefetch -xprefetch_level=3 -m64 -lmtmalloc
                    SUNW_MP_PROCBIND="8 10 12 14 9 11 13 15"
                    OMP_NUM_THREADS=8
  315.mgrid_l     : -fast  -xtarget=nehalem -xarch=generic
                    -xpagesize=2M -xmodel=medium -xopenmp -xautopar

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright 1999-2008, Standard Performance Evaluation Corporation

Sun Microsystems

Sun Fire X2270 (Intel Xeon X5570 2.93GHz)

SPECompLpeak2001 =

SPECompLbase2001 =

254318

237781

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Menlo Park Test date: Mar-2009 Hardware Avail:Apr-2009 Software Avail:Jun-2009

Notes/Tuning Information (Continued)

                    -xipo=2 -xvector=lib -xprefetch -xprefetch_level=3 -m64
                    -lmtmalloc
                    SUNW_MP_PROCBIND="8 10 12 14 9 11 13 15"
                    OMP_NUM_THREADS=8
  317.applu_l     : basepeak=yes
  321.equake_l    : -fast -xmodel=medium -fns=no -xalias_level=layout
                    -m64 -xdepend=no -xopenmp -lmvec
                    SUNW_MP_PROCBIND="8 10 12 14 9 11 13 15"
                    OMP_NUM_THREADS=8
  325.apsi_l      : -fast -xpagesize=2M -xmodel=medium -xopenmp -xautopar
                    -xipo=2 -xvector=lib -xprefetch -xprefetch_level=3
                    -m64 -lmtmalloc
  327.gafort_l    : -fast -xmodel=medium -fstore  -aligncommon=8
                    -xpagesize=2m -xipo=2 -m64 -xvector=simd
                    -xopenmp -lmvec
  329.fma3d_l     : -fast -xpagesize=2M -xmodel=medium -xopenmp -xautopar
                    -xipo=2 -xvector=lib -xprefetch
                    -xprefetch_level=3  -m64 -lmtmalloc
  331.art_l       : -fast -xpagesize=2M -xmodel=medium -xopenmp
                    -xautopar -xipo=2 -xvector=lib -xprefetch
                    -xprefetch_level=3 -m64 -lmtmalloc
                    SUNW_MP_PROCBIND="8 10 12 14 9 11 13 15"
                    OMP_NUM_THREADS=8

 Extra art allowed flags:
   331.art_l      : -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Base and Peak User Environment:
   export OMP_NUM_THREADS=16
   export SUNW_MP_PROCBIND=TRUE
   export SUNW_MP_THR_IDLE=SPIN
   export OMP_NESTED=FALSE
   export STACKSIZE=16384
   export OMP_DYNAMIC=TRUE
   ulimit -s unlimited

 For a description of Sun Studio 12 Update 1 Compiler flags, portability flags
 and system parameters used to generate this result, please refer to
 SUN-20090504-Studio-Solaris-X86_64.txt file in the flags directory.

 Platform Notes:
   Intel Turbo Boost Technology up to 3.33 GHz
   Default BIOS settings used except:
     Hyper-Threading Technology Enabled (default),
     Intel VT-d: Disabled.  VT-d, if enabled, supports
     remapping of I/O DMA transfers for virtualization.