For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Sun Microsystems: Sun Fire 280R Zeus Technology Ltd.: Zeus 3.3.8.4

SPECweb99 = 2136

Test Date: Tester:

Apr-2001 Sun Microsystems

Hardware Avail: Mar-2001 OS Avail: Jul-2001 HTTP Software Avail: May-2001 Sup. Software Avail: -- SPEC license #: 6

Hardware

Vendor: Sun Microsystems Model: Sun Fire 280R Processor: 750MHz UltraSPARC III # Processors: 2 cores, 2 chips, 1 core/chip Primary Cache: 32KB(I)+64KB(D) on chip Secondary Cache: 8MB(I+D) off chip Other Cache: none Memory: 8GB Disk Subsystem: 1 x 36GB FC-AL 9 x 18GB Sun StorEdge T3 Disk Controllers: Integrated FC-AL PCI Single FC Network Adapter Other Hardware: 1 x Cisco Systems Catalyst 4912G

Software

Operating System: Solaris 8 4/01 + patches File System: UFS Other Software: none

HTTP Software

Vendor: Zeus Technology Ltd. HTTP Software: Zeus 3.3.8.4 API: ISAPI Server Cache: SNCA Log Mode: SNCA binary CLF

Test Sponsor

Test Date: Apr-2001 Tested By: Sun Microsystems SPEC License: 6

Network

# of Controllers: 2 Network Controllers: SUN Gigabit Ethernet # of Nets: 2 Type of Nets: Gigabit Ethernet Network Speed: 1000Mbit/sec MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 8 Model: Ultra 60 Processor: 450MHz UltraSPARC II # of Processors: 2 Memory: 512MB Network Controller: Sun Gigabit Ethernet Operating System: Solaris 8 10/00 Compiler: Sun Workshop 5.0 C

Notes/Tuning Information

SUT Notes

Operating System Notes

set sq_max_size=0, set segmap_percent=90 set ge:ge_intr_mode=1, set ge:ge_dmaburst_mode=1 set ge:ge_tx_fastdvma_min = 512, set ge:ge_nos_tmds = 2048 set rlim_fd_max=70000 set, rlim_fd_cur=70000 set pcisch:pci_stream_buf_enable = 0 set nca:nca_conn_req_max_q=100000, set nca:nca_conn_req_max_q0=100000 set nca:nca_ppmax=900000, set nca:nca_vpmax=900000 set nca:nca_conn_hash_size=82500, set nca:ncaurihash_sz = 12281 /usr/sbin/ndd -set /dev/nca nca_max_cache_size 900000 /usr/sbin/ndd -set /dev/nca nca_use_segmap 1 /etc/nca/nca.if: ge0 ge1, /etc/nca/ncakmod.conf: status=enabled /etc/nca/ncalogd.conf: status=enabled, logd_file_size=1000000000 /etc/nca/ncalogd.conf: logd_path_name=/http_logs/log0 ... /http_logs/log12 Solaris 8 patches: Kernel Update patch (108528-09 or newer) Solaris 8 patches: TCP patch (109472-06 or newer) Solaris 8 patches: NCA patch (109234-04 or newer) Solaris 8 patches: libproc patch (108995-02 or newer) Solaris 8 patches: pstack patch (111295-01 or newer) Solaris 8 patches: truss patch (109025-03 or newer) Solaris 8 patches: libc patch (108991-13 or newer) Solaris 8 patches: libsendfile patch (111297-01 or newer) Solaris 8 patches: Sun Gigabit Ethernet patch (108813-06 or newer)

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

Operating System Notes (Continued)

Solaris 8 patches: libdevinfo patch (111293-03 or newer)

HTTP Software Notes

Zeus 3.3.8.4 Tuning Enabled Modules - runningsites/wstest: cgi, get, index, isapi, map, mime Parameters - global.cfg:

tuning!modules!stats!enabled no tuning!use_nca yes tuning!cache_files 98041 tuning!cache_max_bytes 0 tuning!cache_small_file 4096 tuning!cache_large_file 1048576 tuning!cache_stat_expire 31536000 tuning!cache_flush_interval 31536000 tuning!cache_cooling_time 0 tuning!sendfile yes tuning!listen_queue_size 8192 tuning!so_wbuff_size 1048576 tuning!so_rbuff_size 0 tuning!modules!cgi!cleansize 0 tuning!cbuff_size 65536 tuning!sendfile_minsize 1 tuning!sendfile_reservefd 69000 tuning!bind_any no

Hardware Notes

Disk Configuration:

OS - 1 Internal FC-AL disk file_set & post log - T3, 6 disk RAID 0 LUN access log - T3, 3 disk RAID 0 LUN Default rd_ahead on and cache auto set in T3

Client Notes

set sq_max_size=0, set hires_tick=1 ndd -set /dev/tcp tcp_smallest_anon_port 2048 ndd -set /dev/tcp tcp_time_wait_interval 60000