For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

IBM: Netfinity 5600 Zeus Technology: Zeus Web Server 3.3.2

SPECweb99 = 545

Test Date: Tester:

Dec-1999 IBM Hardware Avail: Nov-1999 OS Avail: Nov-1999 HTTP Software Avail: Aug-1999 Sup. Software Avail: Nov-1999 SPEC license #: 11

Hardware

Vendor: IBM Model: Netfinity 5600 Processor: 533EB Pentium III # Processors: 1 core, 1 chip, 1 core/chip Primary Cache: 16KBI+16KBD on chip Secondary Cache: 256KB Other Cache: none Memory: 1.5 GB Disk Subsystem: 4 X 9.1GB SCSI (Seagate ST39102LC) Disk Controllers: IBM ServeRAID 3L Other Hardware:^{1 x ALTEON ACEswitch 180 GbE Switch}

Software

Operating System: RedHat Linux 6.1 File System: Ext2 Other Software: None

HTTP Software

Vendor: Zeus Technology HTTP Software: Zeus Web Server 3.3.2 API: ISAPI Server Cache: none Log Mode: Common Log Format

Test Sponsor

Test Date: Dec-1999 Tested By: IBM SPEC License: 11

Network

# of Controllers: 1 Network Controllers: Alteon ACEnic PCI # of Nets: 1 Type of Nets: Gigabit Ethernet Network Speed: 1Gb/s MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 6 Model: Intellistation Z Pro Processor: 450Mhz Pentium II Xeon # of Processors: 2 Memory: 256MB Network Controller: Alteon ACEnic PCI Operating System: Windows NT 4.0 SP4 Compiler: Microsoft Visual C++ 6.0

Notes/Tuning Information

Operating System Notes

Tuning parameters:

/proc/sys/fs/file-max 32768 /proc/sys/net/core/rmem-max 65536 /proc/sys/net/core/rmem-default 65536 /proc/sys/net/core/wmem-max 65536 /proc/sys/net/core/wmem-default 65536 /proc/sys/net/ipv4/ip_local_port_range 16384 65536

HTTP Software Notes

Tuning parameters:

tuning!cache_max_bytes=536870912 tuning!cache_files=30000 tuning!cache_small_file=9216 tuning!cache_stat_expire=2600 tuning!listen_queue_size=8192 tuning!sendfile_minsize=4096 tuning!so_wbuff_size=65536 tuning!use_poll=yes tuning!cache_flush_interval=2600 tuning!maxfds=100000 tuning!num_children=3

Hardware Notes

1 Disk OS and Logfile